EX-99.1 2 ex991.htm NEWS RELEASE DATED DECEMBER 8, 2021

Exhibit 99.1

| News Release

December 8, 2021

SSR MINING ANNOUNCES POSITIVE EXPLORATION RESULTS At Marigold

Oxide Intercepts Include 2.97 g/t Au Over 71.6 Meters and 10.47 g/t Over 16.8 Meters

DENVER - SSR Mining Inc. (NASDAQ/TSX: SSRM; ASX: SSR) (“SSR Mining” or the “Company”) is pleased to announce results from 288 drillholes (275 reverse circulation and 13 core drillholes) completed at the Marigold mine in Nevada, USA. The Company’s strategy to advance brownfields targets proximal to existing infrastructure has yielded exceptional results in Nevada, as evidenced by the extensive track record of mineral inventory growth throughout Marigold’s 32 years of consecutive production. The Marigold mine currently has a mine life in excess of 10 years, and these results support the extension and enhancement of future life of mine plans.

Resource development drilling at Marigold is focused in the New Millennium area around the Basalt-Antler pit that historically produced approximately 1 million ounces at a grade of 0.75 g/t. The New Millennium concept, unlocked by recent land acquisitions, targets low-cost resource and reserve additions proximal to the Marigold plan of operations with the potential to complement the existing life of mine plan. New oxide intercepts in New Millennium include:

| • | MRA7324: 10.47 g/t Au over 16.8 meters, including 18.72 g/t Au over 9.1 meters

| • | MRA7249: 7.88 g/t Au over 10.7 meters

| • | MRA7286: 1.51 g/t Au over 22.9 meters, including 2.17 g/t Au over 13.7 meters

| • | MRA7285: 0.96 g/t Au over 29.0 meters, including 1.45 g/t Au over 9.1 meters

| • | DDH7408: 1.49 g/t Au over 29.0 meters, including 2.78 g/t Au over 10.7 meters

In addition to drilling at New Millennium, SSR Mining continues to explore for supplemental oxide ore sources across the broader Marigold land package. At the Trenton Canyon project located ~4 km south of New Millennium (Figure 1), drilling has delivered exciting high-grade intercepts of predominantly oxide mineralization. Exploration at Trenton Canyon aims to define oxide material that leverages existing infrastructure at Marigold to provide an avenue for production growth in the future. Oxide intercepts from Trenton Canyon include:

| • | MRA7266: 2.97 g/t Au over 71.6 meters

| • | MRA7264: 6.53 g/t Au over 12.2 meters including 12.49 g/t Au over 6.1 meters

| • | MRA7316: 7.49 g/t Au over 10.7 meters

Rod Antal, President and CEO said, “These exploration results highlight the potential to add incremental oxide mineralization to Marigold’s already robust reserve life. By focusing on adding ounces proximal to existing infrastructure at New Millennium, we are demonstrating opportunities to build on Marigold’s near and medium-term future, while also continuing to systematically explore the larger property for longer-term targets. We are working to expand and accelerate our exploration efforts at Marigold as a precursor to completing an updated Marigold District Master Plan technical report later in 2022.”

1

Figure 1: Plan map showing target areas within the ~20,000-hectare Marigold land package

Marigold, Nevada

SSR Mining’s mineral holdings include a 100% owned ~20,000-hectare parcel containing the currently producing Marigold mine as well as the past producing Valmy, Trenton Canyon, North Peak, and Buffalo Valley mines.

Near mine exploration during the Exploration Period (May 1st, 2020 to September 30th, 2021) focused on Mineral Resource additions at New Millennium, enabled by land acquisitions completed in 2016, 2018 and 2019. New Millennium represents a low cost, high probability development opportunity in the Nevada portfolio and drilling at the target will continue with the ultimate goal to extend operations at Marigold beyond its current mine life to 2032. The New Millennium target area is comprised of six distinct zones which include East Basalt, Battle Cry, Antler, Section 6, Lil’ Gun and North Antler (Figure 2).

Exploration drilling on the recently acquired Section 6 parcel has returned intercepts analogous to the typical Marigold-style mineralization, including 22.9 meters at 1.51 g/t of Au from 248.4 meters in MRA7286, demonstrating bulk-tonnage potential at the far southern reaches of the Marigold system. As our definition drilling programs continue, there is potential for the discrete zones of mineralization to coalesce. Figure 3 provides select results from the drilling completed at Section 6 and other New Millennium zones. The Company is also undertaking a re-assay program of historical drill samples in the New Millennium area with potential to build on the success of the re-assay program at Marigold’s Mackay deposit during 2015-2016 which yielded a 23% increase in estimated tonnage and a 13% increase in gold ounces within the Mackay pits. The goal of this program is to capture low-grade gold assay values not recorded in the historical dataset and integrate the results with the updated resource model. The first phase of this program, which included the re-analysis of drill samples from two drill sections, yielded positive results (Figure 4) and will now be expanded to encompass the entire project area.

2

During the exploration period, a lesser amount of drilling was completed in the Valmy and Cross Fire resource area. In June of 2021, SSR Mining submitted a proposed amendment to the Marigold Plan of Operations to include the Valmy and Cross Fire resource areas. The Bureau of Land Management is currently reviewing the proposal and we expect a decision in Q4 2021, informing next steps with respect to National Environmental Policy Act requirements.

Figure 2. New Millennium project area at Marigold showing EOY2020 Mineral Resource outline

Figure 3. Oblique longitudinal section demonstrating potential impact of drilling reported during the Exploration Period on EOY2021 Mineral Resources

3

Figure 4. Cross section through Antler-Section 6 portion of New Millennium demonstrating positive impact of re-assay on selected drill section

SSR Mining is also continuing exploration on the 100% owned 8,900-hectare land package to the south of Marigold which includes the past producing Buffalo Valley, North Peak, and Trenton Canyon mines. Given the varied nature of the known deposits and the discovery potential of precious metal (distal Au-Ag) and polymetallic (skarn, porphyry) deposits in the district, the Marigold team employs a comprehensive approach to its exploration programs. This included the completion of a 14.5 km2 multi-element soil geochemistry survey, the recent acquisition of a proprietary airborne hyperspectral dataset, and completion of a 16.9 km seismic reflection survey. Integration of these data increase the predictive capabilities of our teams and helps to generate higher probability exploration targets. Exploration activities remain focused on the discovery of supplemental oxide material capable of bolstering Marigold’s intermediate to long-term production profile, leveraging spatial proximity to New Millennium and potential infrastructure synergies.

Trenton Canyon

SSR Mining’s exploration objective at Trenton Canyon is to delineate Mineral Resources and Reserves in oxide material capable of potentially supporting stand-alone heap leaching facilities. Confirmation drilling within the Relay Ridge deposit in hole MRA7266 returned 2.97 g/t Au over 71.6 meters (oxide) and illustrated the localized higher-grade nature of the mineralization. Similar to New Millennium, the oxide inventory at Trenton Canyon currently consists of isolated mineral centers. Definition drilling to delineate the extents of these mineral centers and potential continuity is ongoing.

4

Buffalo Valley

SSR Mining’s objective at Buffalo Valley is to convert the historically delineated mineral inventory into Mineral Resource and Reserve category with the goal of enabling a potential satellite operation to supplement Marigold’s intermediate to long-term production profile. The historical Indicated Mineral Resources for Buffalo Valley host approximately 418,000 ounces of gold (20 million tonnes at an average grade of 0.65 g/t) as of December 31, 20181. Geotechnical and metallurgical drilling proximal to the Buffalo Valley pit is scheduled for Q4 2021.

Table 1. Significant oxide gold intercepts at Marigold and Trenton Canyon.

Hole ID | From (m) | To (m) | Length (m) | Gold (g/t) | Oxidation State | Area
MRA7249 | 65.5 | 76.2 | 10.7 | 7.88 | Oxide | East Basalt
79.2 | 82.3 | 3.0 | 0.69 | Oxide
MRA7264 | 94.5 | 106.7 | 12.2 | 6.53 | Oxide | Trenton Canyon
including | 94.5 | 100.6 | 6.1 | 12.49 | Oxide
MRA7266 | 24.4 | 27.4 | 3.0 | 0.44 | Oxide | Trenton Canyon
32.0 | 44.2 | 12.2 | 1.22 | Oxide
56.4 | 128.0 | 71.6 | 2.97 | Oxide
including | 56.4 | 111.3 | 54.9 | 3.45 | Oxide
including | 115.8 | 125.0 | 9.1 | 1.95 | Oxide
MRA7285 | 115.8 | 121.9 | 6.1 | 3.44 | Oxide | Section 6
including | 115.8 | 118.9 | 3.0 | 6.22 | Oxide
| 204.2 | 211.8 | 7.6 | 2.64 | Oxide
including | 205.7 | 210.3 | 4.6 | 4.03 | Oxide
| 237.7 | 266.7 | 29.0 | 0.96 | Oxide
including | 242.3 | 245.4 | 3.0 | 1.65 | Oxide
including | 248.4 | 257.6 | 9.1 | 1.45 | Oxide
| 271.3 | 278.9 | 7.6 | 0.51 | Oxide
MRA7286 | 208.8 | 217.9 | 9.1 | 2.11 | Oxide | Section 6
including | 208.8 | 214.9 | 6.1 | 2.79 | Oxide
| 234.7 | 243.8 | 9.1 | 0.84 | Oxide
including | 236.2 | 240.8 | 4.6 | 1.14 | Oxide
| 248.4 | 271.3 | 22.9 | 1.51 | Oxide
including | 256.0 | 269.8 | 13.7 | 2.17 | Oxide
| 306.3 | 313.9 | 7.6 | 4.38 | Oxide
342.9 | 346.0 | 3.0 | 0.49 | Oxide
MRA7289 | 169.2 | 172.2 | 3.0 | 0.33 | Oxide | Section 6
176.8 | 185.9 | 9.1 | 0.83 | Oxide
including | 178.3 | 181.4 | 3.0 | 1.45 | Oxide
| 219.5 | 245.4 | 25.9 | 1.03 | Oxide
including | 219.5 | 228.6 | 9.1 | 1.59 | Oxide
| 253.0 | 263.7 | 10.7 | 0.62 | Oxide
266.7 | 269.8 | 3.0 | 0.49 | Oxide
356.6 | 362.7 | 6.1 | 0.92 | Oxide
including | 356.6 | 361.2 | 4.6 | 1.00 | Oxide

5

Hole ID | From (m) | To (m) | Length (m) | Gold (g/t) | Oxidation State | Area
MRA7324 | 227.1 | 243.8 | 16.8 | 10.47 | Oxide | East Basalt
including | 227.1 | 236.2 | 9.1 | 18.72 | Oxide
DDH7408 | 132.3 | 140.8 | 8.6 | 0.73 | Oxide | Section 6
168.2 | 197.2 | 29.0 | 1.49 | Oxide
including | 168.2 | 178.8 | 10.7 | 2.78 | Oxide
including | 182.7 | 186.5 | 3.8 | 1.05 | Oxide
| 226.2 | 235.3 | 9.1 | 0.85 | Oxide
including | 226.2 | 229.2 | 3.0 | 1.74 | Oxide
| 238.4 | 242.9 | 4.6 | 0.48 | Oxide

Drill intercepts reported above a gold grade of 0.3 g/t and with a minimum length 3.0 meters with a maximum contiguous internal dilution of 2.5 meters. All lengths reported above are downhole length and true thickness are not known at this stage.

Sulfide Exploration

While the Company continues targeting additional oxide inventory across the greater Marigold property, we are simultaneously exploring for structurally controlled sulfide mineralization potentially amenable to alternative mining & processing methods than those currently utilized at Marigold. Building on results announced May 14, 2020, exploration efforts have focused on the Tempest zone, a series of high-grade structures proximal to the past-producing South and West pits at Trenton Canyon (Figure 5). Results from drillhole MRA7405 include 9.1 meters at 18.69 g/t Au (sulfide) from 182.9 meters (Figure 6). At Buffalo Valley, exploration drilling is focused on understanding the geometry and orientation of mineralized structures identified by historical drilling outside of the mine area in addition to drill testing of new targets. Historical drilling previously returned exceptional results, including an anomalously high-grade intercept of 4.6 meters from 283.5 meters at 127.89 g/t Au in hole F95-1, 1.5 km northwest of the Buffalo Valley pit, demonstrating the excellent exploration potential throughout the land position.

The ongoing surface mapping along with results of our geochemical survey are informing interpretation of historical and recent SSR Mining drill results. We are applying this understanding to a robust collection of high-quality and underexplored targets throughout the extensive Trenton Canyon and Buffalo Valley projects.

6

Figure 5. Plan view of Trenton Canyon project area highlighting drilling focus on Tempest zone proximal to previously mined pits. Drillholes with prefix DNT are historical drillholes drilled by Newmont Corporation ("Newmont").

Figure 6. Oblique longitudinal section demonstrating potential impact of drilling reported during the Exploration Period on currently unclassified mineral inventory at Trenton Canyon proximal to the West pit. Drillholes with prefix DNT are historical drillholes drilled by Newmont.

7

Table 2. Significant sulfide gold intercepts at Trenton Canyon from the Exploration Period.

Hole ID | From (m) | To (m) | Length (m) | Gold (g/t) | Oxidation State | Area
MR7233 | 13.7 | 16.8 | 3.0 | 0.57 | Oxide | Trenton Canyon
41.1 | 45.7 | 4.6 | 1.40 | Oxide
140.2 | 143.3 | 3.0 | 0.43 | Sulfide
221.0 | 230.1 | 9.1 | 16.74 | Sulfide
including | 221.0 | 227.1 | 6.1 | 24.98 | Sulfide
| 233.2 | 242.3 | 9.1 | 0.95 | Sulfide
245.4 | 249.9 | 4.6 | 0.68 | Sulfide
292.6 | 315.5 | 22.9 | 0.53 | Sulfide
including | 301.8 | 304.8 | 3.0 | 1.26 | Sulfide
| 425.2 | 429.8 | 4.6 | 0.56 | Sulfide
MRA7405 | 157.0 | 163.1 | 6.1 | 5.66 | Sulfide | Trenton Canyon
169.2 | 172.2 | 3.0 | 0.94 | Sulfide
182.9 | 198.1 | 15.2 | 11.49 | Sulfide
including | 182.9 | 192.0 | 9.1 | 18.69 | Sulfide
| 208.8 | 211.8 | 3.0 | 0.38 | Sulfide
214.9 | 217.9 | 3.0 | 0.50 | Sulfide
227.1 | 230.1 | 3.0 | 0.39 | Sulfide
249.9 | 253.0 | 3.0 | 0.88 | Sulfide
268.2 | 272.8 | 4.6 | 1.02 | Sulfide
281.9 | 291.1 | 9.1 | 0.43 | Sulfide
294.1 | 326.1 | 32.0 | 1.33 | Sulfide
including | 306.3 | 318.5 | 12.2 | 2.53 | Sulfide
| 329.2 | 332.2 | 3.0 | 0.43 | Sulfide
335.3 | 346.0 | 10.7 | 0.44 | Sulfide
349.0 | 381.0 | 32.0 | 0.86 | Sulfide
including | 365.8 | 368.8 | 3.0 | 1.48 | Sulfide
including | 376.4 | 381.0 | 4.6 | 1.86 | Sulfide
| 385.6 | 388.6 | 3.0 | 0.93 | Sulfide
391.7 | 397.8 | 6.1 | 1.99 | Sulfide

Drill intercepts reported above a gold grade of 0.3 g/t and with a minimum length 3.0 meters with a maximum contiguous internal dilution of 2.5 meters. All lengths reported above are downhole length and true thickness are not known at this stage.

1 Mineral Resources disclosed by Newmont (Newmont Press release dated February 21, 2019) have been grossed up to illustrate 100% SSR Mining ownership of Buffalo Valley and are subject to rounding. Metal price used for Mineral Resources estimate is $1,400 per ounce of gold. Mineral Resources that are not Mineral Reserves and do not have demonstrated economic viability.

8

Sampling and Analytical Procedures

Drill samples from the Marigold mine drilling program were sent for processing and analysis to the offices of American Assay Laboratories, Inc. (“AAL”) in Sparks, Nevada which is an ISO 17025 accredited laboratory independent from SSR Mining. Fire assay was completed on a 30-gram sample (AAL method code FA-PB30-ICP) with an Inductively Coupled Plasma finish after a two-acid digestion. Samples with assay results greater than 10 g/t gold were fire assayed on a 30-gram sample (AAL method code Grav Au30) with a gravimetric finish. We employ a rigorous Quality Assurance/Quality Control (“QA/QC”) program, which includes real-time assay quality monitoring through the regular insertion of blanks, duplicates, and certified reference material, as well as reviewing laboratory-provided QA/QC data and confirming results at umpire labs.

Marigold mine also utilizes Paragon Geochemical Laboratories, a privately held corporation located in Sparks, Nevada. Analytical procedures utilized are ISO/IEC 17025:2017 accredited and ISO 9001:2015 certified. Samples were prepared under strictly controlled processes, and 30-gram aliquots fire assayed with lead collection. The analytical determinations were with aqua regia digestion and Inductively Coupled Plasma analysis (Au-OES30). Results greater than 8 g/t gold were fire assayed with gravimetric finish (Au-GR30). Quality control utilizes layers of embedded controls that are monitored during operations and used for final certification.

External review of data and processes relating to Marigold exploration data have been completed by an independent consultant F. C. Edmunds, P. Geo., in November 2021. There were no adverse material results detected and the QA/QC indicates the information collected is acceptable, and the database can be used for further studies.

Qualified Persons

The scientific and technical data contained in this news release relating to the Marigold mine has been reviewed and approved by James N. Carver, SME Registered Member, and a qualified person under National Instrument 43-101 - Standards of Disclosure for Mineral Projects (“NI 43- 101”). Mr. Carver is SSR Mining’s Exploration Manager at the Marigold mine.

About SSR Mining

SSR Mining Inc. is a leading, free cash flow focused intermediate gold company with four producing assets located in the USA, Turkey, Canada, and Argentina, combined with a global pipeline of high-quality development and exploration assets in the USA, Turkey, Mexico, Peru, and Canada. In 2020, the four operating assets produced approximately 711,000 gold-equivalent ounces. SSR Mining is listed under the ticker symbol SSRM on the NASDAQ and the TSX, and SSR on the ASX.

SSR Mining Contacts

F. Edward Farid, Executive Vice President, Chief Corporate Development Officer

Alex Hunchak, Director, Corporate Development and Investor Relations

SSR Mining Inc.

E-Mail: invest@ssrmining.com

Phone: +1 (416) 306-5789

To receive SSR Mining's news releases by e-mail, please register using the SSR Mining website at www.ssrmining.com.

SOURCE: SSR Mining Inc.

9

Cautionary Note Regarding Forward-Looking Information

Except for statements of historical fact relating to the Company, certain statements contained in this press release constitute forward-looking information, future oriented financial information, or financial outlooks (collectively “forward-looking information”) within the meaning of Canadian securities laws. Forward-looking information may be contained in this document and the Company’s other public filings. Forward-looking information relates to statements concerning the Company’s outlook and anticipated events or results and, in some cases, can be identified by terminology such as “may”, “will”, “could”, “should”, “expect”, “plan”, “anticipate”, “believe”, “intend”, “estimate”, “projects”, “predict”, “potential”, “continue” or other similar expressions concerning matters that are not historical facts.

Forward-looking information in this press release is based on certain key expectations and assumptions made by the Company. Although the Company believes that the expectations and assumptions on which such forward-looking information is based are reasonable, undue reliance should not be placed on the forward-looking information because the Company can give no assurance that they will prove to be correct. Forward-looking information is subject to various risks and uncertainties which could cause actual results and experience to differ materially from the anticipated results or expectations expressed in this press release. The key risks and uncertainties include, but are not limited to: local and global political and economic conditions; governmental and regulatory requirements and actions by governmental authorities, including changes in government policy, government ownership requirements, changes in environmental, tax and other laws or regulations and the interpretation thereof; developments with respect to COVID-19 pandemic, including the duration, severity and scope of the pandemic and potential impacts on mining operations; and other risk factors detailed from time to time in the Company’s reports filed with the Canadian securities regulatory authorities.

Forward-looking information in this press release include statements concerning, among other things: forecasts; outlook; timing of production; production, cost, operating and capital expenditure guidance; the Company’s intention to return excess attributable free cash flow to shareholders; the timing and implementation of the Company’s dividend policy; the implementation of any share buyback program and the amount thereof; statements regarding plans or expectations for the declaration of future dividends and the amount thereof; future cash costs and all in sustaining costs (“AISC”) per ounce of gold, silver and other metals sold; the prices of gold, silver and other metals; Mineral Resources, Mineral Reserves, realization of Mineral Reserves, and the existence or realization of Mineral Resource estimates; the Company’s ability to discover new areas of mineralization; the timing and extent of capital investment at the Company’s operations; the timing and extent of capitalized stripping at the Company’s operations; the timing of production and production levels and the results of the Company’s exploration and development programs; current financial resources being sufficient to carry out plans, commitments and business requirements for the next twelve months; movements in commodity prices not impacting the value of any financial instruments; estimated production rates for gold, silver and other metals produced by the Company; the estimated cost of sustaining capital; availability of sufficient financing; receipt of regulatory approvals; the timing of studies, announcements, and analysis; the timing of construction and development of proposed mines and process facilities; ongoing or future development plans and capital replacement; estimates of expected or anticipated economic returns from the Company’s mining projects, including future sales of metals, concentrate or other products produced by the Company and the timing thereof; the Company’s plans and expectations for its properties and operations; and all other timing, exploration, development, operational, financial, budgetary, economic, legal, social, environmental, regulatory, and political matters that may influence or be influenced by future events or conditions.

Such forward-looking information is based on a number of material factors and assumptions, including, but not limited in any manner to, those disclosed in any other of the Company’s filings, and include: the inherent speculative nature of exploration results; the ability to explore; communications with local stakeholders; maintaining community and governmental relations; status of negotiations and potential transactions, including joint ventures; weather conditions at the Company’s operations; commodity prices; the ultimate determination of and realization of Mineral Reserves; existence or realization of Mineral Resources; the development approach; availability and receipt of required approvals, titles, licenses and permits; sufficient working capital to develop and operate the mines and implement development plans; access to adequate services and supplies; foreign currency exchange rates; interest rates; access to capital markets and associated cost of funds; availability of a qualified work force; ability to negotiate, finalize, and execute relevant agreements; lack of social opposition to the Company’s mines or facilities; lack of legal challenges with respect to the Company’s properties; the timing and amount of future production; the ability to meet production, cost, and capital expenditure targets; timing and ability to produce studies and analyses; capital and operating expenditures; economic conditions; availability of sufficient financing; the ultimate ability to mine, process, and sell mineral products on economically favorable terms; and any and all other timing, exploration, development, operational, financial, budgetary, economic, legal, social, geopolitical, regulatory and political factors that may influence future events or conditions. While the Company considers these factors and assumptions to be reasonable based on information currently available to the Company, they may prove to be incorrect.

10

The above list is not exhaustive of the factors that may affect any of the Company’s forward-looking information. You should not place undue reliance on forward-looking information. Forward-looking information is only a prediction based on the Company’s current expectations and the Company’s projections about future events. Actual results may vary from such forward-looking information for a variety of reasons including, but not limited to, risks and uncertainties disclosed in the Company’s filings on the Company’s website at www.ssrmining.com, on SEDAR at www.sedar.com, on EDGAR at www.sec.gov and on the ASX at www.asx.com.au and other unforeseen events or circumstances. Other than as required by law, the Company does not intend, and undertake no obligation to update any forward-looking information to reflect, among other things, new information or future events.

All references to “$” in this press release are to U.S. dollars unless otherwise stated.

This press release includes Mineral Reserves and Mineral Resources classification terms that comply with reporting standards in Canada and the Mineral Reserves and the Mineral Resources estimates are made in accordance with NI 43-101. NI 43-101 is a rule developed by the Canadian Securities Administrators that establishes standards for all public disclosure an issuer makes of scientific and technical information concerning mineral projects. These standards differ significantly from the requirements of the SEC set out in the SEC rules that are applicable to domestic United States reporting companies. Consequently, Mineral Reserves and Mineral Resources information included in this press release may not be comparable to similar information that would generally be disclosed by domestic U.S. reporting companies subject to the reporting and disclosure requirements of the SEC. Accordingly, information concerning mineral deposits set forth herein may not be comparable with information made public by companies that report in accordance with U.S. standards.

11

Table 3. Assay results received during the Exploration Period for Marigold and Trenton Canyon

Hole ID | From (m) | To (m) | Interval (m) | Gold (g/t) | Oxidation State | Area
MR7042 | 99.1 | 102.1 | 3.0 | 0.93 | Oxide | Cross Fire
143.3 | 146.3 | 3.0 | 0.50 | Oxide
160.0 | 166.1 | 6.1 | 0.34 | Oxide
MRA7179 | 0.0 | 3.0 | 3.0 | 0.50 | Oxide | Trenton Canyon
19.8 | 22.9 | 3.0 | 1.50 | Oxide
61.0 | 64.0 | 3.0 | 1.11 | Oxide
178.3 | 182.9 | 4.6 | 1.34 | Sulfide
204.2 | 207.3 | 3.0 | 0.57 | Sulfide
243.8 | 246.9 | 3.0 | 0.47 | Sulfide
265.2 | 269.8 | 4.6 | 1.59 | Sulfide
306.3 | 309.4 | 3.0 | 0.39 | Sulfide
MR7182 | 288.0 | 294.1 | 6.1 | 0.80 | Oxide | East Basalt
MRA7186 | 13.7 | 27.4 | 13.7 | 0.56 | Oxide | Trenton Canyon
MRA7187 | 45.7 | 48.8 | 3.0 | 0.72 | Oxide | Trenton Canyon
MRA7188 | 22.9 | 27.4 | 4.6 | 0.76 | Mixed | Trenton Canyon
108.2 | 111.3 | 3.0 | 0.38 | Oxide
MRA7189 | 9.1 | 15.2 | 6.1 | 0.40 | Oxide | Trenton Canyon
47.2 | 62.5 | 15.2 | 0.39 | Oxide
102.1 | 106.7 | 4.6 | 0.56 | Oxide
184.4 | 187.5 | 3.0 | 0.30 | Oxide
MRA7190 | 172.2 | 176.8 | 4.6 | 0.47 | Sulfide | Trenton Canyon
MRA7191 | NSI | Trenton Canyon
MRA7192 | 170.7 | 175.3 | 4.6 | 0.32 | Oxide | Trenton Canyon
202.7 | 205.7 | 3.0 | 0.70 | Sulfide
MRA7193 | 29.0 | 36.6 | 7.6 | 0.84 | Oxide | Trenton Canyon
MR7197 | 44.2 | 54.9 | 10.7 | 1.80 | Oxide | Valmy
including | 45.7 | 51.8 | 6.1 | 2.70 | Oxide
DDH7202 | 178.3 | 188.4 | 10.1 | 8.03 | Sulfide | Exploration holes for deeper mineralization
including | 178.3 | 187.1 | 8.8 | 9.12 | Sulfide
| 300.5 | 304.7 | 4.2 | 3.34 | Sulfide
MRA7203 | 204.2 | 213.4 | 9.1 | 0.79 | Oxide | Cross Fire
216.4 | 222.5 | 6.1 | 0.52 | Oxide
MRA7204 | 9.1 | 12.2 | 3.0 | 1.52 | Oxide | Cross Fire
152.4 | 163.1 | 10.7 | 2.74 | Oxide
including | 153.9 | 161.5 | 7.6 | 3.63 | Oxide
MRA7205 | NSI | Cross Fire
MR7206 | NSI | Cross Fire
MR7207 | 109.7 | 114.3 | 4.6 | 0.41 | Oxide | Cross Fire
MR7208 | 77.7 | 82.3 | 4.6 | 0.33 | Oxide | Cross Fire

12

Hole ID | From (m) | To (m) | Interval (m) | Gold (g/t) | Oxidation State | Area
MRA7209 | 76.2 | 79.2 | 3.0 | 0.51 | Oxide | Trenton Canyon
MRA7210 | NSI | Trenton Canyon
MR7211 | NSI | Cross Fire
MR7212 | NSI | Cross Fire
MR7213 | NSI | Cross Fire
MRA7214 | NSI | Trenton Canyon
MR7215 | 21.3 | 25.9 | 4.6 | 1.18 | Oxide | Cross Fire
including | 21.3 | 24.4 | 3.0 | 1.48 | Oxide
| 67.1 | 71.6 | 4.6 | 0.40 | Oxide
MR7216 | NSI | Cross Fire
MR7217 | NSI | Cross Fire
MRA7218 | NSI | Trenton Canyon
MRA7219 | 0.0 | 7.6 | 7.6 | 0.42 | Oxide | Trenton Canyon
MRA7220 | 210.3 | 224.0 | 13.7 | 0.39 | Sulfide | Trenton Canyon
MRA7221 | NSI | Trenton Canyon
MRA7222 | 50.3 | 59.4 | 9.1 | 0.86 | Oxide | Trenton Canyon
including | 50.3 | 54.9 | 4.6 | 1.21 | Oxide
| 64.0 | 68.6 | 4.6 | 2.27 | Mixed
including | 65.5 | 68.6 | 3.0 | 3.02 | Sulfide
MRA7223 | 16.8 | 33.5 | 16.8 | 0.83 | Oxide | Trenton Canyon
MRA7224 | 170.7 | 176.8 | 6.1 | 0.65 | Mixed | Cross Fire
187.5 | 190.5 | 3.0 | 0.38 | Oxide
246.9 | 251.5 | 4.6 | 0.84 | Oxide
MRA7225 | 83.8 | 93.0 | 9.1 | 0.96 | Mixed | Cross Fire
233.2 | 236.2 | 3.0 | 0.92 | Sulfide
MRA7226 | NSI | Cross Fire
MRA7227 | 16.8 | 24.4 | 7.6 | 0.58 | Oxide | Cross Fire
29.0 | 35.1 | 6.1 | 0.44 | Oxide
173.7 | 176.8 | 3.0 | 0.40 | Mixed
MRA7228 | 19.8 | 22.9 | 3.0 | 0.83 | Oxide | Trenton Canyon
88.4 | 91.4 | 3.0 | 1.09 | Oxide
MRA7229 | 12.2 | 22.9 | 10.7 | 0.48 | Oxide | Trenton Canyon
MRA7230 | NSI | Trenton Canyon
MRA7232 | 164.6 | 176.8 | 12.2 | 0.65 | Oxide | Mackay
312.4 | 317.0 | 4.6 | 0.46 | Sulfide
329.2 | 333.8 | 4.6 | 0.33 | Sulfide
403.9 | 406.9 | 3.0 | 0.42 | Sulfide
MR7233 | 13.7 | 16.8 | 3.0 | 0.57 | Oxide | Trenton Canyon
41.1 | 45.7 | 4.6 | 1.40 | Oxide
140.2 | 143.3 | 3.0 | 0.43 | Sulfide | Trenton Canyon
221.0 | 230.1 | 9.1 | 16.74 | Sulfide
including | 221.0 | 227.1 | 6.1 | 24.98 | Sulfide
| 233.2 | 242.3 | 9.1 | 0.95 | Sulfide
245.4 | 249.9 | 4.6 | 0.68 | Sulfide
292.6 | 315.5 | 22.9 | 0.53 | Sulfide
including | 301.8 | 304.8 | 3.0 | 1.26 | Sulfide
| 425.2 | 429.8 | 4.6 | 0.56 | Sulfide

13

Hole ID | From (m) | To (m) | Interval (m) | Gold (g/t) | Oxidation State | Area
DDH7234 | 4.0 | 7.5 | 3.6 | 1.94 | Oxide | Exploration holes for deeper mineralization
MRA7235 | 38.1 | 42.7 | 4.6 | 0.35 | Oxide | Trenton Canyon
129.5 | 132.6 | 3.0 | 1.86 | Oxide
213.4 | 216.4 | 3.0 | 1.63 | Sulfide
227.1 | 231.7 | 4.6 | 2.35 | Sulfide
256.0 | 259.1 | 3.0 | 0.72 | Sulfide
307.9 | 313.9 | 6.1 | 0.94 | Sulfide
including | 309.4 | 312.4 | 3.0 | 1.41 | Sulfide
| 399.3 | 406.9 | 7.6 | 0.85 | Sulfide
MRA7236 | NSI | East Basalt
MRA7237 | 96.0 | 99.1 | 3.0 | 0.63 | Oxide | East Basalt
307.9 | 312.4 | 4.6 | 1.44 | Oxide
including | 307.9 | 310.9 | 3.0 | 2.00 | Oxide
| 321.6 | 324.6 | 3.0 | 3.02 | Oxide
MRA7238 | 231.7 | 237.7 | 6.1 | 0.45 | Oxide | East Basalt
MR7239 | 313.9 | 318.5 | 4.6 | 0.33 | Oxide | East Basalt
MRA7240 | NSI | East Basalt
MRA7241 | 121.9 | 129.5 | 7.6 | 1.21 | Mixed | Trenton Canyon
190.5 | 193.6 | 3.0 | 1.21 | Sulfide
204.2 | 210.3 | 6.1 | 5.31 | Sulfide
including | 205.7 | 210.3 | 4.6 | 6.80 | Sulfide
| 239.3 | 242.3 | 3.0 | 0.97 | Sulfide
277.4 | 281.9 | 4.6 | 0.32 | Sulfide
312.4 | 320.0 | 7.6 | 0.30 | Sulfide
361.2 | 379.5 | 18.3 | 0.49 | Sulfide
MRA7242 | 297.2 | 301.8 | 4.6 | 0.48 | Oxide | Mackay
367.3 | 370.3 | 3.0 | 0.36 | Oxide
MRA7243 | 155.4 | 163.1 | 7.6 | 1.12 | Sulfide | Trenton Canyon
including | 157.0 | 161.5 | 4.6 | 1.30 | Sulfide
| 204.2 | 210.3 | 6.1 | 1.12 | Sulfide

14

Hole ID | From (m) | To (m) | Interval (m) | Gold (g/t) | Oxidation State | Area
including | 204.2 | 208.8 | 4.6 | 1.32 | Sulfide | Trenton Canyon
| 221.0 | 224.0 | 3.0 | 1.38 | Sulfide
MR7244 | NSI | East Basalt
MR7245 | 246.9 | 253.0 | 6.1 | 3.02 | Oxide | East Basalt
including | 246.9 | 251.5 | 4.6 | 3.81 | Oxide
| 256.0 | 262.1 | 6.1 | 1.70 | Oxide
289.6 | 294.1 | 4.6 | 1.45 | Oxide
MRA7246 | 123.4 | 128.0 | 4.6 | 0.98 | Oxide | East Basalt
237.7 | 240.8 | 3.0 | 0.39 | Oxide
254.5 | 259.1 | 4.6 | 0.93 | Oxide
271.3 | 274.3 | 3.0 | 0.52 | Oxide
DDH7247 | 59.7 | 64.3 | 4.6 | 0.62 | Oxide | Exploration holes for deeper mineralization
118.9 | 125.3 | 6.5 | 4.56 | Oxide
208.8 | 212.1 | 3.4 | 3.67 | Sulfide
346.3 | 349.6 | 3.4 | 16.04 | Sulfide
MRA7248 | NSI | Mackay
MRA7249 | 65.5 | 76.2 | 10.7 | 7.88 | Oxide | East Basalt
79.2 | 82.3 | 3.0 | 0.69 | Oxide
MRA7250 | 56.4 | 62.5 | 6.1 | 0.39 | Oxide | East Basalt
70.1 | 76.2 | 6.1 | 2.02 | Oxide
including | 70.1 | 73.2 | 3.0 | 3.13 | Oxide
| 207.3 | 211.8 | 4.6 | 0.57 | Oxide
243.8 | 248.4 | 4.6 | 1.02 | Oxide
including | 243.8 | 246.9 | 3.0 | 1.04 | Oxide
MRA7251 | 73.2 | 79.2 | 6.1 | 0.56 | Sulfide | Trenton Canyon
233.2 | 253.0 | 19.8 | 1.79 | Sulfide
including | 233.2 | 237.7 | 4.6 | 1.93 | Sulfide
including | 242.3 | 251.5 | 9.1 | 2.51 | Sulfide
| 256.0 | 277.4 | 21.3 | 0.51 | Sulfide
304.8 | 312.4 | 7.6 | 0.50 | Sulfide
MRA7252 | 65.5 | 68.6 | 3.0 | 0.55 | Sulfide | Trenton Canyon
71.6 | 77.7 | 6.1 | 1.34 | Sulfide
including | 71.6 | 76.2 | 4.6 | 1.62 | Mixed
| 86.9 | 89.9 | 3.0 | 0.54 | Sulfide
231.7 | 234.7 | 3.0 | 0.57 | Sulfide
414.5 | 422.2 | 7.6 | 0.57 | Sulfide
MRA7253 | 73.2 | 80.8 | 7.6 | 2.78 | Oxide | Mackay
including | 73.2 | 77.7 | 4.6 | 4.46 | Oxide
| 248.4 | 272.8 | 24.4 | 1.05 | Sulfide

15

Hole ID | From (m) | To (m) | Interval (m) | Gold (g/t) | Oxidation State | Area
including | 253.0 | 265.2 | 12.2 | 1.32 | Sulfide | Mackay
| 281.9 | 292.6 | 10.7 | 0.63 | Sulfide
297.2 | 307.9 | 10.7 | 0.94 | Sulfide
including | 301.8 | 306.3 | 4.6 | 1.42 | Sulfide
| 317.0 | 320.0 | 3.0 | 0.53 | Sulfide
339.9 | 342.9 | 3.0 | 0.46 | Sulfide
358.1 | 364.2 | 6.1 | 0.31 | Sulfide
DDH7254 | 138.0 | 149.8 | 11.9 | 5.32 | Oxide | Exploration holes for deeper mineralization
including | 139.3 | 147.6 | 8.3 | 7.42 | Oxide
| 305.7 | 308.8 | 3.0 | 0.93 | Sulfide
432.9 | 436.5 | 3.5 | 0.70 | Sulfide
439.7 | 448.7 | 9.0 | 0.81 | Sulfide
461.5 | 465.7 | 4.3 | 0.37 | Sulfide
MRA7256 | 179.8 | 182.9 | 3.0 | 0.75 | Oxide | East Basalt
MRA7257 | 102.1 | 112.8 | 10.7 | 0.71 | Oxide | East Basalt
115.8 | 118.9 | 3.0 | 0.65 | Oxide
260.6 | 268.2 | 7.6 | 0.74 | Oxide
MR7258 | 3.0 | 6.1 | 3.0 | 0.71 | Oxide | East Basalt
227.1 | 231.7 | 4.6 | 0.71 | Oxide
MR7259 | 22.9 | 25.9 | 3.0 | 0.37 | Oxide | East Basalt
MRA7260 | 115.8 | 125.0 | 9.1 | 3.01 | Sulfide | Trenton Canyon
including | 115.8 | 123.4 | 7.6 | 3.47 | Sulfide
| 137.2 | 152.4 | 15.2 | 0.96 | Sulfide
including | 137.2 | 143.3 | 6.1 | 1.55 | Mixed
MRA7261 | NSI | Trenton Canyon
MR7262 | NSI | Mackay
MR7263 | 0.0 | 7.6 | 7.6 | 0.80 | Oxide | Mackay
MRA7264 | 94.5 | 106.7 | 12.2 | 6.53 | Oxide | Trenton Canyon
including | 94.5 | 100.6 | 6.1 | 12.49 | Oxide
MRA7265 | NSI | Trenton Canyon
MRA7266 | 24.4 | 27.4 | 3.0 | 0.44 | Oxide | Trenton Canyon
32.0 | 44.2 | 12.2 | 1.22 | Oxide
56.4 | 128.0 | 71.6 | 2.97 | Oxide
including | 56.4 | 111.3 | 54.9 | 3.45 | Oxide
including | 115.8 | 125.0 | 9.1 | 1.95 | Oxide
MRA7267 | 19.8 | 24.4 | 4.6 | 0.92 | Oxide | Trenton Canyon
47.2 | 65.5 | 18.3 | 1.95 | Oxide
including | 47.2 | 59.4 | 12.2 | 2.68 | Oxide
| 108.2 | 111.3 | 3.0 | 0.66 | Oxide
| 121.9 | 125.0 | 3.0 | 1.41 | Oxide
129.5 | 138.7 | 9.1 | 0.67 | Oxide
149.4 | 152.4 | 3.0 | 0.99 | Sulfide

16

Hole ID | From (m) | To (m) | Interval (m) | Gold (g/t) | Oxidation State | Area
MRA7268 | 68.6 | 71.6 | 3.0 | 0.38 | Oxide | Trenton Canyon
86.9 | 109.7 | 22.9 | 1.21 | Oxide
including | 88.4 | 94.5 | 6.1 | 2.31 | Oxide
including | 100.6 | 103.6 | 3.0 | 2.11 | Oxide
| 114.3 | 126.5 | 12.2 | 0.67 | Oxide
143.3 | 149.4 | 6.1 | 1.14 | Sulfide
MRA7269 | NSI | Section 6
MRA7270 | NSI | Trenton Canyon
MRA7271 | 208.8 | 217.9 | 9.1 | 0.36 | Mixed | Trenton Canyon
MRA7272 | 61.0 | 83.8 | 22.9 | 0.73 | Oxide | Trenton Canyon
including | 61.0 | 65.5 | 4.6 | 1.56 | Oxide
| 94.5 | 102.1 | 7.6 | 1.51 | Oxide
including | 94.5 | 97.5 | 3.0 | 3.04 | Oxide
| 105.2 | 114.3 | 9.1 | 0.68 | Oxide
135.6 | 146.3 | 10.7 | 1.88 | Sulfide
including | 138.7 | 144.8 | 6.1 | 2.96 | Sulfide
| 166.1 | 169.2 | 3.0 | 0.56 | Sulfide
MRA7273 | 310.9 | 324.6 | 13.7 | 0.78 | Oxide | East Basalt
MRA7274 | 0.0 | 3.0 | 3.0 | 0.34 | Mixed | Trenton Canyon
MRA7275 | 134.1 | 141.7 | 7.6 | 0.48 | Oxide | Section 6
262.1 | 265.2 | 3.0 | 0.35 | Mixed
MRA7276 | NSI | Section 6
MRA7277 | 131.1 | 140.2 | 9.1 | 1.26 | Oxide | Section 6
including | 131.1 | 135.6 | 4.6 | 1.89 | Oxide
| 155.4 | 178.3 | 22.9 | 0.73 | Oxide
including | 160.0 | 166.1 | 6.1 | 1.19 | Oxide
| 181.4 | 190.5 | 9.1 | 0.56 | Mixed
196.6 | 202.7 | 6.1 | 0.98 | Oxide
MR7278 | NSI | Trenton Canyon
MRA7279 | NSI | Trenton Canyon
DDH7280 | 179.2 | 183.1 | 3.9 | 0.37 | Sulfide | Exploration holes for deeper mineralization
307.7 | 311.5 | 3.8 | 1.08 | Sulfide
MRA7281 | 138.7 | 150.9 | 12.2 | 0.84 | Oxide | Section 6
160.0 | 207.3 | 47.2 | 0.58 | Oxide
MRA7282 | 65.5 | 79.2 | 13.7 | 1.28 | Oxide | East Basalt
including | 67.1 | 74.7 | 7.6 | 1.89 | Oxide
| 82.3 | 86.9 | 4.6 | 0.60 | Oxide

17

Hole ID | From (m) | To (m) | Interval (m) | Gold (g/t) | Oxidation State | Area
MRA7283 | 15.2 | 18.3 | 3.0 | 0.62 | Oxide | Trenton Canyon
MR7284 | 161.5 | 164.6 | 3.0 | 0.47 | Oxide | Section 6
205.7 | 208.8 | 3.0 | 0.57 | Oxide
216.4 | 227.1 | 10.7 | 0.86 | Mixed
236.2 | 239.3 | 3.0 | 0.54 | Sulfide
MRA7285 | 115.8 | 121.9 | 6.1 | 3.44 | Oxide | Section 6
including | 115.8 | 118.9 | 3.0 | 6.22 | Oxide
| 204.2 | 211.8 | 7.6 | 2.64 | Oxide
including | 205.7 | 210.3 | 4.6 | 4.03 | Oxide
| 237.7 | 266.7 | 29.0 | 0.96 | Oxide
including | 242.3 | 245.4 | 3.0 | 1.65 | Oxide
including | 248.4 | 257.6 | 9.1 | 1.45 | Oxide
| 271.3 | 278.9 | 7.6 | 0.51 | Oxide
MRA7286 | 208.8 | 217.9 | 9.1 | 2.11 | Oxide | Section 6
including | 208.8 | 214.9 | 6.1 | 2.79 | Oxide
| 234.7 | 243.8 | 9.1 | 0.84 | Oxide
including | 236.2 | 240.8 | 4.6 | 1.14 | Oxide
| 248.4 | 271.3 | 22.9 | 1.51 | Oxide
including | 256.0 | 269.8 | 13.7 | 2.17 | Oxide
| 306.3 | 313.9 | 7.6 | 4.38 | Oxide
342.9 | 346.0 | 3.0 | 0.49 | Oxide
MRA7287 | 170.7 | 173.7 | 3.0 | 0.43 | Oxide | Section 6
199.6 | 214.9 | 15.2 | 0.79 | Oxide
including | 202.7 | 208.8 | 6.1 | 1.22 | Oxide
| 324.6 | 327.7 | 3.0 | 0.40 | Oxide
341.4 | 344.4 | 3.0 | 0.42 | Oxide
355.1 | 362.7 | 7.6 | 0.33 | Oxide
MRA7288 | NSI | Section 6
MRA7289 | 169.2 | 172.2 | 3.0 | 0.33 | Oxide | Section 6
176.8 | 185.9 | 9.1 | 0.83 | Oxide
including | 178.3 | 181.4 | 3.0 | 1.45 | Oxide
| 219.5 | 245.4 | 25.9 | 1.03 | Oxide
including | 219.5 | 228.6 | 9.1 | 1.59 | Oxide
| 253.0 | 263.7 | 10.7 | 0.62 | Oxide
266.7 | 269.8 | 3.0 | 0.49 | Oxide
356.6 | 362.7 | 6.1 | 0.92 | Oxide
including | 356.6 | 361.2 | 4.6 | 1.00 | Oxide
MRA7290 | 205.7 | 210.3 | 4.6 | 0.50 | Oxide | Section 6

18

Hole ID | From (m) | To (m) | Interval (m) | Gold (g/t) | Oxidation State | Area
DDH7291 | 609.9 | 625.2 | 15.2 | 2.68 | Sulfide | Exploration holes for deeper mineralization
including | 609.9 | 621.9 | 12.0 | 3.26 | Sulfide
| 682.3 | 690.7 | 8.4 | 0.57 | Sulfide
MRA7292 | NSI | Section 6
MRA7293 | 170.7 | 178.3 | 7.6 | 1.40 | Oxide | Section 6
including | 170.7 | 175.3 | 4.6 | 2.04 | Oxide
| 182.9 | 187.5 | 4.6 | 0.71 | Oxide
MR7294 | 61.0 | 67.1 | 6.1 | 1.19 | Sulfide | Trenton Canyon
including | 62.5 | 65.5 | 3.0 | 1.87 | Sulfide
MRA7295 | 44.2 | 50.3 | 6.1 | 0.77 | Oxide | Trenton Canyon
77.7 | 82.3 | 4.6 | 0.57 | Sulfide
MRA7296 | NSI | Trenton Canyon
MRA7297 | NSI | Trenton Canyon
MRA7298 | 286.5 | 292.6 | 6.1 | 1.77 | Sulfide | Trenton Canyon
MRA7299 | NSI | Trenton Canyon
MR7300 | 166.1 | 175.3 | 9.1 | 1.15 | Oxide | Section 6
including | 167.6 | 172.2 | 4.6 | 1.84 | Oxide
| 327.7 | 330.7 | 3.0 | 0.56 | Oxide
MR7301 | NSI | Trenton Canyon
MRA7302 | 190.5 | 199.6 | 9.1 | 0.50 | Oxide | Section 6
MR7303 | 169.2 | 172.2 | 3.0 | 1.78 | Sulfide | Trenton Canyon
189.0 | 198.1 | 9.1 | 0.91 | Sulfide
including | 190.5 | 193.6 | 3.0 | 1.87 | Sulfide
MRA7304 | 96.0 | 105.2 | 9.1 | 0.64 | Mixed | Trenton Canyon
111.3 | 114.3 | 3.0 | 0.47 | Mixed
MRA7305 | NSI | East Basalt
MR7306 | 176.8 | 184.4 | 7.6 | 0.90 | Oxide | Valmy
187.5 | 224.0 | 36.6 | 0.91 | Oxide
including | 187.5 | 198.1 | 10.7 | 1.60 | Oxide
| 361.2 | 364.2 | 3.0 | 0.62 | Mixed
MR7307 | 182.9 | 190.5 | 7.6 | 0.56 | Oxide | Valmy
205.7 | 208.8 | 3.0 | 0.50 | Oxide
227.1 | 233.2 | 6.1 | 0.73 | Oxide
237.7 | 242.3 | 4.6 | 0.69 | Oxide
MR7308 | 228.6 | 234.7 | 6.1 | 3.87 | Oxide | Valmy
including | 228.6 | 233.2 | 4.6 | 5.00 | Oxide
| 254.5 | 262.1 | 7.6 | 0.88 | Oxide
including | 259.1 | 262.1 | 3.0 | 1.39 | Oxide
| 274.3 | 277.4 | 3.0 | 0.92 | Oxide

19

Hole ID | From (m) | To (m) | Interval (m) | Gold (g/t) | Oxidation State | Area
DDH7309 | 751.1 | 760.8 | 9.7 | 0.70 | Sulfide | Exploration holes for deeper mineralization
890.8 | 894.9 | 4.1 | 0.37 | Sulfide
MR7310 | 179.8 | 182.9 | 3.0 | 0.50 | Oxide | East Basalt
240.8 | 243.8 | 3.0 | 0.36 | Oxide
MRA7311 | NSI | East Basalt
MRA7312 | 91.4 | 99.1 | 7.6 | 8.42 | Oxide | East Basalt
including | 91.4 | 97.5 | 6.1 | 10.36 | Oxide
MRA7313 | 111.3 | 114.3 | 3.0 | 0.68 | Oxide | East Basalt
MRA7314 | 86.9 | 93.0 | 6.1 | 2.63 | Oxide | East Basalt
including | 86.9 | 91.4 | 4.6 | 3.34 | Oxide
MR7315 | 312.4 | 315.5 | 3.0 | 0.35 | Sulfide | East Basalt
MRA7316 | 193.6 | 204.2 | 10.7 | 7.49 | Oxide | Trenton Canyon
including | 193.6 | 199.6 | 6.1 | 12.79 | Oxide
| 214.9 | 228.6 | 13.7 | 3.25 | Sulfide
including | 214.9 | 219.5 | 4.6 | 8.24 | Sulfide
MRA7317 | NSI | Trenton Canyon
MRA7318 | 53.3 | 56.4 | 3.0 | 1.08 | Oxide | Trenton Canyon
MRA7319 | 288.0 | 292.6 | 4.6 | 0.81 | Sulfide | Trenton Canyon
342.9 | 353.6 | 10.7 | 2.10 | Sulfide
including | 344.4 | 353.6 | 9.1 | 2.40 | Sulfide
MRA7320 | NSI | Trenton Canyon
MRA7321 | 15.2 | 21.3 | 6.1 | 2.97 | Oxide | Trenton Canyon
68.6 | 73.2 | 4.6 | 0.82 | Sulfide
MRA7322 | 10.7 | 13.7 | 3.0 | 1.59 | Oxide | Trenton Canyon
56.4 | 59.4 | 3.0 | 0.35 | Sulfide
MRA7323 | 105.2 | 109.7 | 4.6 | 0.92 | Sulfide | East Basalt
190.5 | 195.1 | 4.6 | 1.41 | Oxide
including | 192.0 | 195.1 | 3.0 | 1.67 | Oxide
MRA7324 | 227.1 | 243.8 | 16.8 | 10.47 | Oxide | East Basalt
including | 227.1 | 236.2 | 9.1 | 18.72 | Oxide
MRA7325 | NSI | East Basalt
MRA7326 | 33.5 | 57.9 | 24.4 | 1.56 | Sulfide | Trenton Canyon
including | 39.6 | 44.2 | 4.6 | 5.33 | Oxide
MRA7328 | 140.2 | 144.8 | 4.6 | 0.46 | Sulfide | Trenton Canyon
MRA7329 | 67.1 | 70.1 | 3.0 | 2.32 | Mixed | Trenton Canyon
77.7 | 96.0 | 18.3 | 1.71 | Sulfide
including | 83.8 | 94.5 | 10.7 | 2.32 | Mixed
| 99.1 | 106.7 | 7.6 | 0.59 | Sulfide
MRA7330 | 256.0 | 259.1 | 3.0 | 1.70 | Sulfide | East Basalt

20

Hole ID | From (m) | To (m) | Interval (m) | Gold (g/t) | Oxidation State | Area
MRA7331 | NSI | East Basalt
MRA7332 | 137.2 | 141.7 | 4.6 | 8.19 | Sulfide | Trenton Canyon
MRA7333 | NSI | East Basalt
MRA7334 | NSI | East Basalt
MRA7335 | 1.5 | 4.6 | 3.0 | 0.49 | Oxide | East Basalt
MRA7336 | NSI | East Basalt
MRA7337 | NSI | Trenton Canyon
MR7338 | 50.3 | 62.5 | 12.2 | 0.68 | Oxide | North Pits
including | 57.9 | 61.0 | 3.0 | 1.34 | Oxide
MR7339 | 74.7 | 80.8 | 6.1 | 0.46 | Oxide | North Pits
118.9 | 121.9 | 3.0 | 0.35 | Oxide
MR7340 | NSI | North Pits
MRA7341 | 384.1 | 388.6 | 4.6 | 0.60 | Sulfide | East Basalt
MRA7342 | 62.5 | 67.1 | 4.6 | 1.08 | Oxide | North Pits
MR7343 | 47.2 | 56.4 | 9.1 | 1.92 | Oxide | North Pits
including | 48.8 | 54.9 | 6.1 | 2.51 | Oxide
| 74.7 | 88.4 | 13.7 | 1.21 | Oxide
including | 74.7 | 80.8 | 6.1 | 2.10 | Oxide
MR7344 | 41.1 | 44.2 | 3.0 | 0.59 | Oxide | North Pits
51.8 | 56.4 | 4.6 | 0.46 | Oxide
MR7345 | 53.3 | 61.0 | 7.6 | 1.80 | Oxide | North Pits
MR7346 | NSI | North Pits
DDH7347 | 79.2 | 108.1 | 28.9 | 1.70 | Oxide | North Pits
including | 79.2 | 106.9 | 27.6 | 1.77 | Oxide
DDH7348 | 69.5 | 87.8 | 18.3 | 1.90 | Oxide | North Pits
including | 72.5 | 86.3 | 13.7 | 2.31 | Oxide
| 90.8 | 94.8 | 4.0 | 0.64 | Oxide
MR7349 | 71.6 | 80.8 | 9.1 | 0.61 | Oxide | North Pits
MR7350 | 62.5 | 89.9 | 27.4 | 0.61 | Oxide | North Pits
including | 73.2 | 77.7 | 4.6 | 1.20 | Oxide
MRA7351 | NSI | East Basalt
MRA7352 | 71.6 | 77.7 | 6.1 | 2.02 | Oxide | East Basalt
including | 71.6 | 74.7 | 3.0 | 3.52 | Oxide
| 161.5 | 164.6 | 3.0 | 3.04 | Mixed
172.2 | 175.3 | 3.0 | 2.43 | Sulfide
MRA7353 | 321.6 | 327.7 | 6.1 | 0.72 | Oxide | East Basalt
MRA7354 | NSI | East Basalt
MRA7355 | 105.2 | 108.2 | 3.0 | 0.92 | Oxide | East Basalt
332.2 | 335.3 | 3.0 | 1.42 | Oxide

21

Hole ID | From (m) | To (m) | Interval (m) | Gold (g/t) | Oxidation State | Area
MRA7356 | 138.7 | 144.8 | 6.1 | 0.38 | Oxide | Section 6
149.4 | 167.6 | 18.3 | 0.58 | Oxide
222.5 | 228.6 | 6.1 | 0.96 | Oxide
352.0 | 355.1 | 3.0 | 0.97 | Sulfide
MRA7357 | 1.5 | 4.6 | 3.0 | 0.46 | Oxide | Section 6
132.6 | 137.2 | 4.6 | 0.45 | Oxide
146.3 | 155.4 | 9.1 | 0.38 | Oxide
237.7 | 243.8 | 6.1 | 0.55 | Oxide
285.0 | 288.0 | 3.0 | 0.46 | Oxide
MRA7358 | 9.1 | 12.2 | 3.0 | 0.78 | Oxide | Section 6
149.4 | 155.4 | 6.1 | 0.37 | Oxide
160.0 | 163.1 | 3.0 | 0.47 | Oxide
166.1 | 173.7 | 7.6 | 0.42 | Oxide
205.7 | 208.8 | 3.0 | 0.66 | Oxide
358.1 | 365.8 | 7.6 | 0.38 | Sulfide
382.5 | 387.1 | 4.6 | 0.45 | Sulfide
397.8 | 405.4 | 7.6 | 0.47 | Sulfide
MRA7359 | NSI | Section 6
MRA7360 | 196.6 | 201.2 | 4.6 | 0.83 | Oxide | Section 6
230.1 | 243.8 | 13.7 | 0.80 | Oxide
277.4 | 280.4 | 3.0 | 1.12 | Oxide
330.7 | 338.3 | 7.6 | 1.16 | Sulfide
including | 330.7 | 336.8 | 6.1 | 1.22 | Sulfide
MRA7361 | 134.1 | 140.2 | 6.1 | 0.51 | Oxide | Section 6
288.0 | 294.1 | 6.1 | 0.72 | Sulfide
312.4 | 324.6 | 12.2 | 0.40 | Sulfide
MRA7362 | 89.9 | 93.0 | 3.0 | 0.87 | Oxide | East Basalt
MRA7363 | 283.5 | 286.5 | 3.0 | 0.52 | Oxide | East Basalt
MR7364 | NSI | East Basalt
MRA7365 | 310.9 | 324.6 | 13.7 | 0.88 | Oxide | East Basalt
MRA7366 | NSI | East Basalt
MRA7367 | 182.9 | 189.0 | 6.1 | 0.84 | Oxide | East Basalt
MRA7368 | 426.7 | 435.9 | 9.1 | 0.61 | Sulfide | East Basalt
438.9 | 446.5 | 7.6 | 0.45 | Sulfide
MRA7369 | NSI | East Basalt
DDH7372 | 39.9 | 48.2 | 8.2 | 0.56 | Oxide | North Pits
including | 43.9 | 47.1 | 3.2 | 1.06 | Oxide
| 57.5 | 61.6 | 4.0 | 0.39 | Sulfide
71.3 | 76.3 | 5.0 | 0.35 | Mixed

22

Hole ID | From (m) | To (m) | Interval (m) | Gold (g/t) | Oxidation State | Area
DDH7373 | 25.9 | 31.5 | 5.5 | 1.59 | Oxide | North Pits
DDH7374 | NSI | North Pits
MR7376 | NSI | East Basalt
MRA7377 | NSI | East Basalt
MRA7378 | NSI | East Basalt
MRA7379 | 4.6 | 9.1 | 4.6 | 0.34 | Oxide | East Basalt
150.9 | 153.9 | 3.0 | 0.50 | Oxide
295.7 | 300.2 | 4.6 | 0.38 | Sulfide
MRA7380 | 82.3 | 86.9 | 4.6 | 0.67 | Sulfide | East Basalt
143.3 | 150.9 | 7.6 | 0.47 | Oxide
MR7381 | NSI | East Basalt
MRA7382 | 74.7 | 94.5 | 19.8 | 3.65 | Oxide | East Basalt
including | 74.7 | 88.4 | 13.7 | 4.73 | Oxide
| 97.5 | 106.7 | 9.1 | 0.46 | Sulfide
MRA7383 | NSI | East Basalt
MRA7384 | 114.3 | 117.3 | 3.0 | 1.14 | Sulfide | East Basalt
291.1 | 295.7 | 4.6 | 0.54 | Oxide
MRA7385 | 227.1 | 233.2 | 6.1 | 0.61 | Oxide | East Basalt
MR7386 | 88.4 | 91.4 | 3.0 | 0.54 | Oxide | East Basalt
MRA7387 | 44.2 | 48.8 | 4.6 | 0.45 | Oxide | East Basalt
MRA7388 | NSI | East Basalt
MRA7389 | 112.8 | 118.9 | 6.1 | 1.84 | Oxide | East Basalt
MR7390 | NSI | East Basalt
MRA7391 | 166.1 | 169.2 | 3.0 | 0.68 | Mixed | East Basalt
MR7392 | 327.7 | 330.7 | 3.0 | 1.88 | Oxide | East Basalt
MRA7393 | 222.5 | 225.6 | 3.0 | 0.40 | Oxide | East Basalt
MR7394 | 336.8 | 339.9 | 3.0 | 0.50 | Oxide | East Basalt
MR7395 | NSI | East Basalt
MRA7396 | NSI | East Basalt
MRA7397 | 306.3 | 323.1 | 16.8 | 1.03 | Oxide | East Basalt
including | 307.9 | 310.9 | 3.0 | 1.23 | Oxide
including | 315.5 | 321.6 | 6.1 | 1.31 | Oxide
MRA7398 | 313.9 | 321.6 | 7.6 | 0.58 | Oxide | East Basalt
MR7399 | NSI | East Basalt
MRA7400 | 105.2 | 115.8 | 10.7 | 2.30 | Sulfide | East Basalt
including | 105.2 | 112.8 | 7.6 | 3.01 | Sulfide
| 434.3 | 438.9 | 4.6 | 0.69 | Sulfide
MR7401 | 71.6 | 82.3 | 10.7 | 0.59 | Oxide | Section 6
including | 74.7 | 77.7 | 3.0 | 1.09 | Oxide

23

Hole ID | From (m) | To (m) | Interval (m) | Gold (g/t) | Oxidation State | Area
| 170.7 | 175.3 | 4.6 | 0.43 | Oxide | Section 6
181.4 | 189.0 | 7.6 | 0.57 | Oxide
211.8 | 214.9 | 3.0 | 0.51 | Oxide
242.3 | 246.9 | 4.6 | 0.62 | Oxide
291.1 | 313.9 | 22.9 | 0.63 | Oxide
324.6 | 330.7 | 6.1 | 0.39 | Oxide
MRA7402 | 353.6 | 358.1 | 4.6 | 0.36 | Sulfide | East Basalt
365.8 | 370.3 | 4.6 | 0.41 | Sulfide
MR7403 | 19.8 | 29.0 | 9.1 | 0.71 | Oxide | Section 6
102.1 | 105.2 | 3.0 | 0.59 | Oxide
114.3 | 131.1 | 16.8 | 0.50 | Oxide
140.2 | 146.3 | 6.1 | 0.39 | Oxide
149.4 | 157.0 | 7.6 | 0.63 | Oxide
163.1 | 166.1 | 3.0 | 0.50 | Oxide
300.2 | 306.3 | 6.1 | 1.22 | Oxide
including | 300.2 | 303.3 | 3.0 | 2.10 | Oxide
MRA7404 | 96.0 | 99.1 | 3.0 | 1.04 | Oxide | East Basalt
MRA7405 | 157.0 | 163.1 | 6.1 | 5.66 | Sulfide | Trenton Canyon
169.2 | 172.2 | 3.0 | 0.94 | Sulfide
182.9 | 198.1 | 15.2 | 11.49 | Sulfide
including | 182.9 | 192.0 | 9.1 | 18.69 | Sulfide
| 208.8 | 211.8 | 3.0 | 0.38 | Sulfide
214.9 | 217.9 | 3.0 | 0.50 | Sulfide
227.1 | 230.1 | 3.0 | 0.39 | Sulfide
249.9 | 253.0 | 3.0 | 0.88 | Sulfide
268.2 | 272.8 | 4.6 | 1.02 | Sulfide
281.9 | 291.1 | 9.1 | 0.43 | Sulfide
294.1 | 326.1 | 32.0 | 1.33 | Sulfide
including | 306.3 | 318.5 | 12.2 | 2.53 | Sulfide
| 329.2 | 332.2 | 3.0 | 0.43 | Sulfide
335.3 | 346.0 | 10.7 | 0.44 | Sulfide
349.0 | 381.0 | 32.0 | 0.86 | Sulfide
including | 365.8 | 368.8 | 3.0 | 1.48 | Sulfide
including | 376.4 | 381.0 | 4.6 | 1.86 | Sulfide
| 385.6 | 388.6 | 3.0 | 0.93 | Sulfide
391.7 | 397.8 | 6.1 | 1.99 | Sulfide
MRA7406 | 243.8 | 251.5 | 7.6 | 0.78 | Oxide | North Pits
283.5 | 292.6 | 9.1 | 0.83 | Oxide
including | 283.5 | 286.5 | 3.0 | 1.51 | Oxide

24

Hole ID | From (m) | To (m) | Interval (m) | Gold (g/t) | Oxidation State | Area
MRA7407 | 146.3 | 149.4 | 3.0 | 0.42 | Oxide | North Pits
224.0 | 227.1 | 3.0 | 0.41 | Oxide
260.6 | 268.2 | 7.6 | 2.61 | Oxide
including | 260.6 | 263.7 | 3.0 | 5.49 | Oxide
DDH7408 | 132.3 | 140.8 | 8.6 | 0.73 | Oxide | Section 6
168.2 | 197.2 | 29.0 | 1.49 | Oxide
including | 168.2 | 178.8 | 10.7 | 2.78 | Oxide
including | 182.7 | 186.5 | 3.8 | 1.05 | Oxide
| 226.2 | 235.3 | 9.1 | 0.85 | Oxide
including | 226.2 | 229.2 | 3.0 | 1.74 | Oxide
| 238.4 | 242.9 | 4.6 | 0.48 | Oxide
MRA7409 | 97.5 | 105.2 | 7.6 | 0.97 | Oxide | North Pits
161.5 | 166.1 | 4.6 | 2.79 | Oxide
169.2 | 172.2 | 3.0 | 0.77 | Oxide
196.6 | 199.6 | 3.0 | 0.73 | Oxide
MRA7410 | NSI | North Pits
MRA7411 | 7.6 | 10.7 | 3.0 | 0.40 | Oxide | North Pits
53.3 | 65.5 | 12.2 | 0.91 | Oxide
including | 56.4 | 64.0 | 7.6 | 1.23 | Oxide
| 94.5 | 99.1 | 4.6 | 0.65 | Oxide
108.2 | 112.8 | 4.6 | 0.48 | Oxide
MRA7412 | 126.5 | 132.6 | 6.1 | 0.67 | Oxide | North Pits
MRA7413 | 32.0 | 39.6 | 7.6 | 0.69 | Oxide | North Pits
74.7 | 82.3 | 7.6 | 0.68 | Oxide
93.0 | 97.5 | 4.6 | 0.40 | Oxide
105.2 | 108.2 | 3.0 | 0.34 | Oxide
MRA7414 | 4.6 | 10.7 | 6.1 | 0.50 | Oxide | North Pits
147.8 | 152.4 | 4.6 | 0.43 | Oxide
MRA7415 | 38.1 | 44.2 | 6.1 | 1.21 | Oxide | North Pits
including | 39.6 | 44.2 | 4.6 | 1.28 | Oxide
| 62.5 | 65.5 | 3.0 | 0.82 | Oxide
68.6 | 76.2 | 7.6 | 0.59 | Oxide
MRA7416 | 89.9 | 99.1 | 9.1 | 0.42 | Oxide | North Pits
MRA7417 | 97.5 | 102.1 | 4.6 | 0.57 | Oxide | North Pits
MRA7418 | 89.9 | 93.0 | 3.0 | 0.57 | Oxide | North Pits
115.8 | 123.4 | 7.6 | 0.71 | Oxide
131.1 | 134.1 | 3.0 | 0.85 | Oxide
MRA7419 | 6.1 | 10.7 | 4.6 | 0.32 | Oxide | North Pits
MRA7420 | 172.2 | 190.5 | 18.3 | 0.60 | Oxide | Section 6

25

Hole ID | From (m) | To (m) | Interval (m) | Gold (g/t) | Oxidation State | Area
MRA7421 | 147.8 | 153.9 | 6.1 | 0.41 | Oxide | Section 6
172.2 | 176.8 | 4.6 | 0.62 | Oxide
231.7 | 234.7 | 3.0 | 0.34 | Oxide
MRA7422 | 100.6 | 108.2 | 7.6 | 4.65 | Sulfide | Trenton Canyon
including | 102.1 | 106.7 | 4.6 | 7.37 | Sulfide
| 138.7 | 141.7 | 3.0 | 0.60 | Mixed
160.0 | 163.1 | 3.0 | 0.58 | Oxide
MRA7424 | 4.6 | 7.6 | 3.0 | 0.49 | Mixed | East Basalt
MRA7425 | NSI | East Basalt
MRA7426 | 155.4 | 161.5 | 6.1 | 0.36 | Oxide | Section 6
164.6 | 175.3 | 10.7 | 0.60 | Oxide
190.5 | 193.6 | 3.0 | 0.47 | Oxide
199.6 | 217.9 | 18.3 | 0.74 | Oxide
221.0 | 230.1 | 9.1 | 0.80 | Oxide
249.9 | 256.0 | 6.1 | 0.38 | Oxide
MRA7427 | 102.1 | 117.3 | 15.2 | 0.54 | Oxide | Section 6
182.9 | 189.0 | 6.1 | 0.67 | Oxide
207.3 | 211.8 | 4.6 | 0.32 | Oxide
246.9 | 256.0 | 9.1 | 1.11 | Oxide
including | 248.4 | 254.5 | 6.1 | 1.48 | Oxide
| 291.1 | 294.1 | 3.0 | 0.38 | Oxide
312.4 | 315.5 | 3.0 | 0.58 | Oxide
318.5 | 327.7 | 9.1 | 0.42 | Sulfide
MRA7428 | 120.4 | 128.0 | 7.6 | 0.55 | Oxide | Section 6
184.4 | 192.0 | 7.6 | 0.32 | Oxide
242.3 | 245.4 | 3.0 | 0.58 | Oxide
269.8 | 292.6 | 22.9 | 0.45 | Oxide
349.0 | 355.1 | 6.1 | 1.79 | Sulfide
402.3 | 410.0 | 7.6 | 0.59 | Sulfide
MRA7429 | 126.5 | 141.7 | 15.2 | 0.48 | Oxide | Section 6
147.8 | 152.4 | 4.6 | 0.34 | Oxide
166.1 | 169.2 | 3.0 | 0.33 | Oxide
179.8 | 195.1 | 15.2 | 0.34 | Oxide
234.7 | 237.7 | 3.0 | 0.47 | Oxide
MRA7430 | 93.0 | 96.0 | 3.0 | 1.43 | Oxide | East Basalt
167.6 | 170.7 | 3.0 | 0.38 | Oxide
MRA7431 | 56.4 | 64.0 | 7.6 | 1.74 | Oxide | East Basalt
including | 56.4 | 59.4 | 3.0 | 3.42 | Oxide
| 118.9 | 121.9 | 3.0 | 0.39 | Oxide

26

Hole ID | From (m) | To (m) | Interval (m) | Gold (g/t) | Oxidation State | Area
MRA7432 | 102.1 | 112.8 | 10.7 | 0.70 | Oxide | Section 6
125.0 | 135.6 | 10.7 | 0.57 | Oxide
149.4 | 152.4 | 3.0 | 0.32 | Oxide
193.6 | 204.2 | 10.7 | 1.30 | Oxide
including | 195.1 | 199.6 | 4.6 | 2.21 | Oxide
| 213.4 | 225.6 | 12.2 | 1.23 | Oxide
including | 213.4 | 221.0 | 7.6 | 1.60 | Oxide
| 268.2 | 275.8 | 7.6 | 0.75 | Oxide
including | 272.8 | 275.8 | 3.0 | 1.17 | Oxide
| 347.5 | 350.5 | 3.0 | 0.47 | Sulfide
MRA7433 | 118.9 | 131.1 | 12.2 | 1.18 | Oxide | Section 6
including | 121.9 | 128.0 | 6.1 | 1.74 | Oxide
| 227.1 | 230.1 | 3.0 | 0.70 | Oxide
MRA7434 | 77.7 | 80.8 | 3.0 | 2.87 | Oxide | East Basalt
including | 77.7 | 80.8 | 3.0 | 2.87 | Oxide
MRA7435 | 184.4 | 196.6 | 12.2 | 1.81 | Oxide | Section 6
including | 187.5 | 193.6 | 6.1 | 3.12 | Oxide
MR7436 | 318.5 | 324.6 | 6.1 | 2.93 | Sulfide | Trenton Canyon
including | 318.5 | 321.6 | 3.0 | 5.25 | Sulfide
| 374.9 | 379.5 | 4.6 | 0.36 | Sulfide
MRA7437 | 51.8 | 56.4 | 4.6 | 2.43 | Oxide | Trenton Canyon
including | 53.3 | 56.4 | 3.0 | 3.49 | Oxide
| 141.7 | 147.8 | 6.1 | 0.94 | Sulfide
269.8 | 275.8 | 6.1 | 1.68 | Sulfide
MRA7438 | 25.9 | 29.0 | 3.0 | 3.44 | Oxide | Trenton Canyon
82.3 | 85.3 | 3.0 | 0.45 | Oxide
123.4 | 131.1 | 7.6 | 1.25 | Sulfide
including | 123.4 | 126.5 | 3.0 | 2.58 | Sulfide
| 185.9 | 189.0 | 3.0 | 0.65 | Sulfide
283.5 | 286.5 | 3.0 | 1.30 | Sulfide
MRA7439 | 111.3 | 118.9 | 7.6 | 0.48 | Mixed | Trenton Canyon
MRA7440 | 105.2 | 112.8 | 7.6 | 2.30 | Sulfide | Trenton Canyon
including | 105.2 | 108.2 | 3.0 | 4.98 | Sulfide
| 184.4 | 187.5 | 3.0 | 0.48 | Sulfide
192.0 | 195.1 | 3.0 | 0.62 | Sulfide
201.2 | 205.7 | 4.6 | 0.31 | Sulfide
367.3 | 370.3 | 3.0 | 1.82 | Sulfide
MRA7441 | 137.2 | 147.8 | 10.7 | 2.62 | Oxide | Section 6
including | 141.7 | 146.3 | 4.6 | 5.30 | Oxide

27

Hole ID | From (m) | To (m) | Interval (m) | Gold (g/t) | Oxidation State | Area
| 199.6 | 217.9 | 18.3 | 1.23 | Oxide | Section 6
including | 205.7 | 211.8 | 6.1 | 2.00 | Oxide
MRA7442 | NSI | Section 6
MRA7443 | 50.3 | 53.3 | 3.0 | 1.15 | Oxide | Trenton Canyon
132.6 | 137.2 | 4.6 | 1.73 | Oxide
including | 132.6 | 135.6 | 3.0 | 2.41 | Oxide
MRA7444 | NSI | Trenton Canyon
MRA7445 | NSI | Trenton Canyon
MRA7446 | NSI | Trenton Canyon
MRA7447 | NSI | Trenton Canyon
MRA7448 | 135.6 | 141.7 | 6.1 | 0.43 | Oxide | Section 6
144.8 | 150.9 | 6.1 | 0.34 | Oxide
155.4 | 160.0 | 4.6 | 0.49 | Oxide
169.2 | 187.5 | 18.3 | 1.07 | Oxide
including | 173.7 | 181.4 | 7.6 | 1.59 | Oxide
MRA7449 | 189.0 | 199.6 | 10.7 | 0.75 | Oxide | Valmy
including | 193.6 | 196.6 | 3.0 | 1.33 | Oxide
| 202.7 | 211.8 | 9.1 | 1.84 | Oxide
including | 204.2 | 207.3 | 3.0 | 4.39 | Oxide
| 239.3 | 242.3 | 3.0 | 0.74 | Oxide
MRA7450 | 269.8 | 277.4 | 7.6 | 1.82 | Sulfide | Trenton Canyon
including | 269.8 | 274.3 | 4.6 | 2.78 | Sulfide
MRA7451 | 108.2 | 111.3 | 3.0 | 0.41 | Oxide | Cross Fire
MRA7454 | 196.6 | 199.6 | 3.0 | 0.44 | Oxide | Cross Fire
MRA7455 | NSI | Cross Fire
MRA7457 | 62.5 | 74.7 | 12.2 | 0.58 | Oxide | Cross Fire
including | 62.5 | 65.5 | 3.0 | 1.12 | Oxide
MRA7458 | 41.1 | 47.2 | 6.1 | 0.57 | Sulfide | Trenton Canyon
291.1 | 294.1 | 3.0 | 2.07 | Sulfide
320.0 | 333.8 | 13.7 | 0.41 | Sulfide
MRA7459 | 4.6 | 7.6 | 3.0 | 0.41 | Oxide | Cross Fire
24.4 | 41.1 | 16.8 | 0.47 | Oxide
MR7460 | NSI | Cross Fire
MRA7461 | 91.4 | 100.6 | 9.1 | 0.96 | Mixed | Trenton Canyon
including | 91.4 | 96.0 | 4.6 | 1.43 | Oxide
| 169.2 | 173.7 | 4.6 | 0.44 | Sulfide
309.4 | 317.0 | 7.6 | 1.50 | Sulfide
MRA7462 | 153.9 | 158.5 | 4.6 | 1.77 | Sulfide | Trenton Canyon
including | 153.9 | 157.0 | 3.0 | 2.44 | Sulfide

28

Hole ID | From (m) | To (m) | Interval (m) | Gold (g/t) | Oxidation State | Area
MRA7463 | 4.6 | 7.6 | 3.0 | 0.59 | Sulfide | Trenton Canyon
MRA7464 | NSI | Trenton Canyon
MRA7465 | 4.6 | 9.1 | 4.6 | 1.97 | Mixed | Trenton Canyon
including | 4.6 | 7.6 | 3.0 | 2.77 | Oxide
MRA7466 | 137.2 | 176.8 | 39.6 | 0.62 | Oxide | Section 6
including | 163.1 | 167.6 | 4.6 | 1.30 | Oxide
MRA7467 | 47.2 | 50.3 | 3.0 | 2.27 | Sulfide | Trenton Canyon
MR7468 | 150.9 | 160.0 | 9.1 | 0.52 | Oxide | Section 6
MRA7470 | 32.0 | 35.1 | 3.0 | 1.17 | Mixed | Trenton Canyon
38.1 | 45.7 | 7.6 | 0.68 | Sulfide
70.1 | 74.7 | 4.6 | 1.81 | Mixed
including | 70.1 | 73.2 | 3.0 | 2.47 | Mixed
MRA7471 | 36.6 | 45.7 | 9.1 | 0.82 | Sulfide | Trenton Canyon
including | 42.7 | 45.7 | 3.0 | 1.00 | Sulfide
| 71.6 | 74.7 | 3.0 | 0.39 | Sulfide
MRA7475 | 64.0 | 67.1 | 3.0 | 0.99 | Sulfide | Trenton Canyon
MRA7476 | 173.7 | 178.3 | 4.6 | 0.32 | Oxide | Section 6
181.4 | 189.0 | 7.6 | 0.45 | Oxide
242.3 | 245.4 | 3.0 | 0.42 | Oxide
285.0 | 297.2 | 12.2 | 1.46 | Oxide
including | 286.5 | 294.1 | 7.6 | 1.96 | Oxide
MRA7477 | 144.8 | 161.5 | 16.8 | 1.18 | Oxide | Section 6
including | 150.9 | 158.5 | 7.6 | 1.59 | Oxide
| 239.3 | 254.5 | 15.2 | 0.58 | Oxide
315.5 | 338.3 | 22.9 | 1.24 | Oxide
including | 318.5 | 321.6 | 3.0 | 3.19 | Oxide
including | 324.6 | 332.2 | 7.6 | 1.59 | Oxide
MRA7479 | 9.1 | 19.8 | 10.7 | 3.15 | Oxide | Trenton Canyon
27.4 | 32.0 | 4.6 | 0.78 | Sulfide
44.2 | 48.8 | 4.6 | 0.79 | Mixed
93.0 | 96.0 | 3.0 | 0.67 | Sulfide
MRA7481 | NSI | Section 6
MRA7482 | 275.8 | 278.9 | 3.0 | 4.17 | Oxide | Section 6
288.0 | 292.6 | 4.6 | 3.19 | Oxide
including | 288.0 | 291.1 | 3.0 | 4.47 | Oxide
MRA7485 | 286.5 | 307.9 | 21.3 | 1.89 | Sulfide | Trenton Canyon
including | 286.5 | 297.2 | 10.7 | 2.97 | Sulfide
including | 303.3 | 306.3 | 3.0 | 1.91 | Mixed
| 310.9 | 320.0 | 9.1 | 0.79 | Sulfide
342.9 | 346.0 | 3.0 | 0.94 | Sulfide |
358.1 | 362.7 | 4.6 | 0.74 | Sulfide

29

Hole ID | From (m) | To (m) | Interval (m) | Gold (g/t) | Oxidation State | Area
MRA7486 | 207.3 | 216.4 | 9.1 | 0.82 | Mixed | Trenton Canyon
including | 207.3 | 210.3 | 3.0 | 1.55 | Sulfide
MRA7487 | 176.8 | 189.0 | 12.2 | 1.82 | Sulfide | Trenton Canyon
including | 176.8 | 181.4 | 4.6 | 3.84 | Sulfide
MRA7488 | NSI | Trenton Canyon
MR7492 | 105.2 | 109.7 | 4.6 | 0.35 | Sulfide | Section 6
192.0 | 213.4 | 21.3 | 0.75 | Oxide
including | 202.7 | 205.7 | 3.0 | 1.03 | Oxide
| 224.0 | 231.7 | 7.6 | 0.58 | Oxide
MRA7498 | 265.2 | 269.8 | 4.6 | 0.43 | Mixed | Section 6
MRA7499 | 100.6 | 106.7 | 6.1 | 0.61 | Oxide | Section 6
| 118.9 | 135.6 | 16.8 | 0.71 | Oxide
including | 121.9 | 125.0 | 3.0 | 1.30 | Oxide
| 163.1 | 172.2 | 9.1 | 0.36 | Oxide
MR7500 | 48.8 | 65.5 | 16.8 | 0.72 | Oxide | Mackay
102.1 | 112.8 | 10.7 | 0.42 | Oxide
143.3 | 157.0 | 13.7 | 0.80 | Oxide
including | 149.4 | 153.9 | 4.6 | 1.28 | Oxide
| 524.3 | 527.3 | 3.0 | 0.31 | Sulfide
MR7501 | NSI | Mackay
MRA7503 | 187.5 | 195.1 | 7.6 | 0.38 | Oxide | Section 6
263.7 | 266.7 | 3.0 | 0.57 | Oxide
269.8 | 275.8 | 6.1 | 1.12 | Oxide
including | 271.3 | 274.3 | 3.0 | 1.52 | Mixed
| 285.0 | 289.6 | 4.6 | 2.39 | Oxide
292.6 | 298.7 | 6.1 | 0.71 | Oxide
327.7 | 330.7 | 3.0 | 0.57 | Oxide
MRA7504 | 216.4 | 221.0 | 4.6 | 0.47 | Oxide | Section 6
324.6 | 327.7 | 3.0 | 1.28 | Oxide
344.4 | 352.0 | 7.6 | 0.36 | Oxide

Drill intercepts reported above a gold grade of 0.3 g/t and a minimum length of 3.0 meters and a maximum contiguous dilution of 2.5 meters. All lengths reported above are downhole length and true thickness are not known at this stage.

NSI - No significant intercept

30

Supporting Drilling Information to SSR Mining Announcement

This document provides supporting drill collar locations and composite assay results for the Marigold drilling program referenced in the announcement “SSR Mining announces positive exploration results at Marigold”, dated December 8, 2021.

Drill collar locations are surveyed in UTM Zone 11, NAD27 grid using differential GPS in units of meters. The Hole ID prefix DDH is used for HQ (63.5 mm core diameter) and NQ (47.6 mm core diameter) core drilling, the MR and MRA prefixes designate reverse circulation drill holes.

Table 4. Drill Collar Coordinates

Hole ID | Easting | Northing | Elevation (m) | Azimuth (deg.) | Dip (deg.) | Length (m) | Area
MR7042 | 487651 | 4505055 | 1793 | 133 | -89 | 306.3 | Cross Fire
MRA7179 | 484802 | 4499317 | 2262 | 88 | -82 | 336.8 | Trenton Canyon
MR7182 | 486043 | 4503645 | 1866 | 193 | -89 | 367.3 | East Basalt
MRA7186 | 483908 | 4499894 | 2191 | 92 | -45 | 275.8 | Trenton Canyon
MRA7187 | 483891 | 4500051 | 2178 | 89 | -44 | 275.8 | Trenton Canyon
MRA7188 | 483877 | 4500141 | 2182 | 88 | -75 | 306.3 | Trenton Canyon
MRA7189 | 483877 | 4500141 | 2181 | 84 | -45 | 306.3 | Trenton Canyon
MRA7190 | 483936 | 4499490 | 2262 | 85 | -75 | 275.8 | Trenton Canyon
MRA7191 | 483936 | 4499490 | 2262 | 89 | -44 | 275.8 | Trenton Canyon
MRA7192 | 483922 | 4499529 | 2242 | 94 | -75 | 275.8 | Trenton Canyon
MRA7193 | 483922 | 4499529 | 2242 | 87 | -44 | 275.8 | Trenton Canyon
MR7197 | 486802 | 4504438 | 1919 | 87 | -89 | 336.8 | Valmy
DDH7202 | 484525 | 4499602 | 2262 | 272 | -70 | 721.5 | Exploration holes for deeper mineralization
MRA7203 | 487540 | 4504923 | 1850 | 270 | -76 | 336.8 | Cross Fire
MRA7204 | 487609 | 4504925 | 1823 | 269 | -71 | 214.9 | Cross Fire
MRA7205 | 487685 | 4504796 | 1877 | 273 | -78 | 306.3 | Cross Fire
MR7206 | 487538 | 4505658 | 1709 | 282 | -89 | 245.4 | Cross Fire
MR7207 | 487593 | 4505599 | 1717 | 98 | -90 | 184.4 | Cross Fire
MR7208 | 487611 | 4505535 | 1724 | 256 | -90 | 214.9 | Cross Fire
MRA7209 | 483978 | 4499303 | 2322 | 91 | -76 | 275.8 | Trenton Canyon
MRA7210 | 483978 | 4499303 | 2322 | 91 | -44 | 275.8 | Trenton Canyon
MR7211 | 487466 | 4505657 | 1710 | 163 | -89 | 245.4 | Cross Fire
MR7212 | 487577 | 4505623 | 1714 | 296 | -89 | 184.4 | Cross Fire
MR7213 | 487527 | 4505321 | 1756 | 163 | -89 | 245.4 | Cross Fire
MRA7214 | 484113 | 4498839 | 2407 | 238 | -85 | 306.3 | Trenton Canyon
MR7215 | 487623 | 4505201 | 1764 | 127 | -89 | 275.8 | Cross Fire
MR7216 | 487592 | 4505202 | 1767 | 17 | -89 | 275.8 | Cross Fire
MR7217 | 487588 | 4505321 | 1756 | 302 | -90 | 214.9 | Cross Fire
MRA7218 | 484098 | 4499142 | 2358 | 90 | -75 | 275.8 | Trenton Canyon

31

Hole ID | Easting | Northing | Elevation (m) | Azimuth (deg.) | Dip (deg.) | Length (m) | Area
MRA7219 | 484098 | 4499142 | 2358 | 11 | -71 | 275.8 | Trenton Canyon
MRA7220 | 484019 | 4499143 | 2327 | 90 | -74 | 275.8 | Trenton Canyon
MRA7221 | 484019 | 4499143 | 2327 | 90 | -48 | 275.8 | Trenton Canyon
MRA7222 | 484014 | 4499192 | 2335 | 87 | -76 | 275.8 | Trenton Canyon
MRA7223 | 484014 | 4499192 | 2335 | 84 | -45 | 275.8 | Trenton Canyon
MRA7224 | 487693 | 4504649 | 1937 | 269 | -73 | 275.8 | Cross Fire
MRA7225 | 487756 | 4504595 | 1947 | 270 | -73 | 336.8 | Cross Fire
MRA7226 | 488215 | 4504619 | 1965 | 270 | -63 | 336.8 | Cross Fire
MRA7227 | 487823 | 4504592 | 1954 | 269 | -71 | 336.8 | Cross Fire
MRA7228 | 484461 | 4498750 | 2439 | 267 | -77 | 306.3 | Trenton Canyon
MRA7229 | 484460 | 4498750 | 2439 | 268 | -46 | 306.3 | Trenton Canyon
MRA7230 | 484532 | 4498312 | 2453 | 273 | -76 | 257.6 | Trenton Canyon
MR7233 | 484836 | 4499287 | 2262 | 27 | -89 | 458.7 | Trenton Canyon
MRA7232 | 485029 | 4506670 | 1627 | 90 | -60 | 426.7 | Mackay
DDH7234 | 484872 | 4499274 | 2261 | 75 | -89 | 483.7 | Exploration holes for deeper mineralization
MRA7235 | 484836 | 4499287 | 2262 | 273 | -80 | 458.7 | Trenton Canyon
MRA7236 | 485902 | 4503858 | 1867 | 270 | -67 | 367.3 | East Basalt
MRA7237 | 485907 | 4503677 | 1865 | 89 | -72 | 336.8 | East Basalt
MRA7238 | 485991 | 4503676 | 1863 | 88 | -72 | 336.8 | East Basalt
MR7239 | 485923 | 4503220 | 1880 | 163 | -90 | 397.8 | East Basalt
MRA7240 | 485926 | 4503280 | 1884 | 271 | -47 | 382.5 | East Basalt
MRA7241 | 484941 | 4499226 | 2262 | 273 | -75 | 446.5 | Trenton Canyon
MRA7242 | 484779 | 4508008 | 1590 | 132 | -51 | 518.2 | Mackay
MRA7243 | 484942 | 4499226 | 2262 | 272 | -84 | 458.7 | Trenton Canyon
MR7244 | 485942 | 4503401 | 1869 | 98 | -71 | 382.5 | East Basalt
MR7245 | 485934 | 4503372 | 1874 | 2 | -89 | 367.3 | East Basalt
MRA7246 | 485959 | 4503435 | 1865 | 86 | -76 | 367.3 | East Basalt
DDH7247 | 484835 | 4499287 | 2262 | 273 | -65 | 416.7 | Exploration holes for deeper mineralization
MRA7248 | 484779 | 4508011 | 1590 | 88 | -56 | 486.2 | Mackay
MRA7249 | 486007 | 4503548 | 1841 | 90 | -72 | 367.3 | East Basalt
MRA7250 | 485964 | 4503587 | 1843 | 90 | -71 | 382.5 | East Basalt
MRA7251 | 484895 | 4499401 | 2196 | 177 | -52 | 312.4 | Trenton Canyon
MRA7252 | 484895 | 4499401 | 2196 | 181 | -66 | 428.2 | Trenton Canyon
MRA7253 | 485220 | 4508923 | 1539 | 282 | -85 | 365.8 | Mackay
DDH7254 | 484926 | 4499033 | 2273 | 265 | -79 | 1032.4 | Exploration holes for deeper mineralization
MRA7256 | 486025 | 4503621 | 1861 | 89 | -74 | 382.5 | East Basalt
MRA7257 | 485980 | 4503612 | 1852 | 92 | -77 | 382.5 | East Basalt

32

Hole ID | Easting | Northing | Elevation (m) | Azimuth (deg.) | Dip (deg.) | Length (m) | Area
MR7258 | 486046 | 4503466 | 1865 | 115 | -89 | 367.3 | East Basalt
MR7259 | 485886 | 4503100 | 1875 | 14 | -90 | 452.6 | East Basalt
MRA7260 | 484897 | 4499402 | 2195 | 20 | -44 | 190.5 | Trenton Canyon
MRA7261 | 484897 | 4499401 | 2195 | 18 | -61 | 248.4 | Trenton Canyon
MR7262 | 485359 | 4508219 | 1433 | 118 | -90 | 213.4 | Mackay
MR7263 | 485126 | 4508010 | 1387 | 1 | -89 | 167.6 | Mackay
MRA7264 | 484988 | 4499413 | 2195 | 18 | -51 | 166.1 | Trenton Canyon
MRA7265 | 484988 | 4499413 | 2195 | 18 | -61 | 184.4 | Trenton Canyon
MRA7266 | 483611 | 4500494 | 2001 | 90 | -60 | 169.2 | Trenton Canyon
MRA7267 | 483649 | 4500547 | 1996 | 100 | -80 | 153.9 | Trenton Canyon
MRA7268 | 483623 | 4500556 | 1986 | 92 | -69 | 169.2 | Trenton Canyon
MRA7269 | 485074 | 4502888 | 1816 | 92 | -69 | 367.3 | Section 6
MRA7270 | 485654 | 4498190 | 2139 | 273 | -75 | 306.3 | Trenton Canyon
MRA7271 | 485662 | 4498187 | 2139 | 88 | -44 | 306.3 | Trenton Canyon
MRA7272 | 483630 | 4500609 | 1972 | 91 | -52 | 169.2 | Trenton Canyon
MRA7273 | 485897 | 4503768 | 1853 | 89 | -68 | 367.3 | East Basalt
MRA7274 | 485704 | 4498047 | 2149 | 273 | -73 | 306.3 | Trenton Canyon
MRA7275 | 485004 | 4502853 | 1823 | 96 | -69 | 367.3 | Section 6
MRA7276 | 485081 | 4502854 | 1822 | 92 | -70 | 367.3 | Section 6
MRA7277 | 485007 | 4502791 | 1828 | 105 | -70 | 367.3 | Section 6
MR7278 | 485709 | 4497908 | 2125 | 168 | -90 | 306.3 | Trenton Canyon
MRA7279 | 485712 | 4497908 | 2125 | 93 | -44 | 306.3 | Trenton Canyon
DDH7280 | 485280 | 4499522 | 2038 | 248 | -78 | 759.3 | Exploration holes for deeper mineralization
MRA7281 | 485009 | 4502764 | 1830 | 92 | -71 | 367.3 | Section 6
MRA7282 | 486043 | 4503555 | 1843 | 103 | -70 | 367.3 | East Basalt
MRA7283 | 485738 | 4497644 | 2153 | 270 | -43 | 306.3 | Trenton Canyon
MR7284 | 484886 | 4502547 | 1792 | 353 | -89 | 367.3 | Section 6
MRA7285 | 484900 | 4502522 | 1791 | 86 | -57 | 367.3 | Section 6
MRA7286 | 484853 | 4502525 | 1777 | 88 | -56 | 367.3 | Section 6
MRA7287 | 485042 | 4502274 | 1802 | 93 | -55 | 367.3 | Section 6
MRA7288 | 484954 | 4502275 | 1796 | 94 | -57 | 283.5 | Section 6
MRA7289 | 485020 | 4502638 | 1828 | 87 | -71 | 367.3 | Section 6
MRA7290 | 484883 | 4502702 | 1797 | 89 | -69 | 367.3 | Section 6
DDH7291 | 484462 | 4502302 | 1840 | 267 | -80 | 1054.9 | Exploration holes for deeper mineralization
MRA7292 | 484926 | 4502152 | 1778 | 81 | -54 | 458.7 | Section 6
MRA7293 | 485018 | 4502151 | 1800 | 91 | -53 | 458.7 | Section 6
MR7294 | 485822 | 4500044 | 2148 | 227 | -89 | 251.5 | Trenton Canyon
MRA7295 | 485821 | 4500045 | 2148 | 315 | -67 | 306.3 | Trenton Canyon

33

Hole ID | Easting | Northing | Elevation (m) | Azimuth (deg.) | Dip (deg.) | Length (m) | Area
MRA7296 | 485889 | 4500052 | 2133 | 313 | -66 | 306.3 | Trenton Canyon
MRA7297 | 485887 | 4500050 | 2133 | 240 | -66 | 306.3 | Trenton Canyon
MRA7298 | 485742 | 4500909 | 1955 | 268 | -76 | 306.3 | Trenton Canyon
MRA7299 | 485741 | 4500909 | 1955 | 270 | -48 | 306.3 | Trenton Canyon
MR7300 | 485065 | 4502548 | 1820 | 261 | -89 | 382.5 | Section 6
MR7301 | 485459 | 4501140 | 1972 | 72 | -90 | 239.3 | Trenton Canyon
MRA7302 | 484761 | 4502885 | 1758 | 85 | -69 | 371.9 | Section 6
MR7303 | 485875 | 4499793 | 2160 | 111 | -89 | 367.3 | Trenton Canyon
MRA7304 | 485874 | 4499793 | 2160 | 270 | -57 | 306.3 | Trenton Canyon
MRA7305 | 485891 | 4503619 | 1857 | 271 | -55 | 382.5 | East Basalt
MR7306 | 487130 | 4504375 | 1914 | 76 | -89 | 367.3 | Valmy
MR7307 | 487175 | 4504381 | 1905 | 110 | -89 | 367.3 | Valmy
MR7308 | 487166 | 4504347 | 1920 | 190 | -89 | 417.6 | Valmy
DDH7309 | 486780 | 4504646 | 1883 | 268 | -84 | 1466.1 | Exploration holes for deeper mineralization
MR7310 | 486051 | 4503492 | 1859 | 34 | -89 | 397.8 | East Basalt
MRA7311 | 486082 | 4503550 | 1849 | 90 | -71 | 339.9 | East Basalt
MRA7312 | 486114 | 4503554 | 1860 | 89 | -70 | 336.8 | East Basalt
MRA7313 | 486059 | 4503614 | 1860 | 92 | -70 | 367.3 | East Basalt
MRA7314 | 486107 | 4503615 | 1859 | 90 | -71 | 367.3 | East Basalt
MR7315 | 486114 | 4503492 | 1854 | 274 | -88 | 367.3 | East Basalt
MRA7316 | 484502 | 4499558 | 2259 | 128 | -86 | 306.3 | Trenton Canyon
MRA7317 | 484662 | 4499547 | 2262 | 18 | -45 | 184.4 | Trenton Canyon
MRA7318 | 484658 | 4499537 | 2262 | 16 | -59 | 184.4 | Trenton Canyon
MRA7319 | 485012 | 4499147 | 2262 | 11 | -71 | 355.1 | Trenton Canyon
MRA7320 | 484426 | 4499410 | 2248 | 189 | -47 | 184.4 | Trenton Canyon
MRA7321 | 485077 | 4499431 | 2157 | 19 | -79 | 184.4 | Trenton Canyon
MRA7322 | 485077 | 4499433 | 2157 | 18 | -46 | 184.4 | Trenton Canyon
MRA7323 | 486046 | 4503463 | 1865 | 93 | -76 | 367.3 | East Basalt
MRA7324 | 486056 | 4503313 | 1900 | 89 | -71 | 367.3 | East Basalt
MRA7325 | 485965 | 4503312 | 1890 | 89 | -71 | 367.3 | East Basalt
MRA7326 | 484843 | 4499454 | 2203 | 31 | -61 | 184.4 | Trenton Canyon
MRA7328 | 484941 | 4499402 | 2194 | 19 | -60 | 184.4 | Trenton Canyon
MRA7329 | 484841 | 4499452 | 2203 | 32 | -42 | 184.4 | Trenton Canyon
MRA7330 | 486287 | 4503036 | 1933 | 104 | -71 | 367.3 | East Basalt
MRA7331 | 486202 | 4503067 | 1923 | 90 | -70 | 367.3 | East Basalt
MRA7332 | 485079 | 4499427 | 2158 | 202 | -58 | 285.0 | Trenton Canyon
MRA7333 | 486128 | 4503126 | 1912 | 97 | -70 | 367.3 | East Basalt
MRA7334 | 486046 | 4503159 | 1902 | 101 | -73 | 367.3 | East Basalt
MRA7335 | 485985 | 4503189 | 1894 | 89 | -71 | 367.3 | East Basalt

34

Hole ID | Easting | Northing | Elevation (m) | Azimuth (deg.) | Dip (deg.) | Length (m) | Area
MRA7336 | 486113 | 4503189 | 1910 | 98 | -71 | 367.3 | East Basalt
MRA7337 | 484299 | 4499635 | 2167 | 29 | -45 | 184.4 | Trenton Canyon
MR7338 | 486973 | 4513033 | 1427 | 0 | -90 | 123.4 | North Pits
MR7339 | 487065 | 4513003 | 1426 | 0 | -90 | 137.2 | North Pits
MR7340 | 487034 | 4513003 | 1426 | 0 | -90 | 137.2 | North Pits
MRA7341 | 486072 | 4503249 | 1909 | 102 | -70 | 397.8 | East Basalt
MRA7342 | 486471 | 4512820 | 1435 | 270 | -85 | 108.2 | North Pits
MR7343 | 486561 | 4512422 | 1443 | 0 | -90 | 93.0 | North Pits
MR7344 | 486456 | 4512363 | 1444 | 0 | -90 | 93.0 | North Pits
MR7345 | 486442 | 4512303 | 1446 | 0 | -90 | 68.6 | North Pits
MR7346 | 486195 | 4511143 | 1472 | 0 | -90 | 138.7 | North Pits
DDH7347 | 486212 | 4511022 | 1475 | 84 | -90 | 139.3 | North Pits
DDH7348 | 486203 | 4510930 | 1477 | 345 | -89 | 144.8 | North Pits
MR7349 | 486243 | 4510809 | 1479 | 0 | -90 | 121.9 | North Pits
MR7350 | 486246 | 4510778 | 1480 | 0 | -90 | 121.9 | North Pits
MRA7351 | 486067 | 4503310 | 1901 | 91 | -70 | 382.5 | East Basalt
MRA7352 | 486033 | 4503370 | 1889 | 93 | -71 | 458.7 | East Basalt
MRA7353 | 485992 | 4503433 | 1871 | 91 | -71 | 367.3 | East Basalt
MRA7354 | 486003 | 4503308 | 1896 | 103 | -76 | 458.7 | East Basalt
MRA7355 | 486006 | 4503344 | 1892 | 90 | -77 | 458.7 | East Basalt
MRA7356 | 484691 | 4503676 | 1735 | 90 | -66 | 402.3 | Section 6
MRA7357 | 484704 | 4503584 | 1744 | 91 | -61 | 385.6 | Section 6
MRA7358 | 484710 | 4503615 | 1741 | 82 | -61 | 458.7 | Section 6
MRA7359 | 485082 | 4502803 | 1828 | 93 | -70 | 378.0 | Section 6
MRA7360 | 484700 | 4503890 | 1743 | 90 | -66 | 458.7 | Section 6
MRA7361 | 484770 | 4503798 | 1744 | 88 | -66 | 449.6 | Section 6
MRA7362 | 486034 | 4503370 | 1889 | 91 | -85 | 397.8 | East Basalt
MRA7363 | 485924 | 4503220 | 1882 | 79 | -83 | 397.8 | East Basalt
MR7364 | 485880 | 4503830 | 1857 | 325 | -88 | 367.3 | East Basalt
MRA7365 | 485905 | 4503707 | 1862 | 90 | -71 | 397.8 | East Basalt
MRA7366 | 485908 | 4503646 | 1864 | 271 | -76 | 428.2 | East Basalt
MRA7367 | 485889 | 4503618 | 1857 | 268 | -45 | 428.2 | East Basalt
MRA7368 | 485896 | 4503765 | 1853 | 268 | -71 | 458.7 | East Basalt
MRA7369 | 486078 | 4503679 | 1872 | 89 | -71 | 458.7 | East Basalt
DDH7372 | 485143 | 4508127 | 1373 | 91 | -64 | 83.8 | North Pits
DDH7373 | 485122 | 4508157 | 1373 | 90 | -62 | 68.6 | North Pits
DDH7374 | 485184 | 4508277 | 1373 | 95 | -79 | 38.4 | North Pits
MR7376 | 486104 | 4503639 | 1869 | 247 | -89 | 428.2 | East Basalt
MRA7377 | 486153 | 4503613 | 1860 | 93 | -74 | 367.3 | East Basalt
MRA7378 | 486199 | 4503613 | 1869 | 90 | -75 | 336.8 | East Basalt

35

Hole ID | Easting | Northing | Elevation (m) | Azimuth (deg.) | Dip (deg.) | Length (m) | Area
MRA7379 | 486073 | 4503580 | 1851 | 89 | -75 | 367.3 | East Basalt
MRA7380 | 486031 | 4503582 | 1849 | 88 | -74 | 385.6 | East Basalt
MR7381 | 486181 | 4503493 | 1880 | 50 | -89 | 382.5 | East Basalt
MRA7382 | 486148 | 4503555 | 1874 | 91 | -76 | 382.5 | East Basalt
MRA7383 | 486188 | 4503552 | 1884 | 93 | -76 | 440.4 | East Basalt
MRA7384 | 486048 | 4503463 | 1866 | 98 | -65 | 458.7 | East Basalt
MRA7385 | 485827 | 4503949 | 1844 | 97 | -51 | 275.8 | East Basalt
MR7386 | 485903 | 4503679 | 1866 | 60 | -89 | 458.7 | East Basalt
MRA7387 | 485902 | 4503680 | 1866 | 270 | -76 | 458.7 | East Basalt
MRA7388 | 485901 | 4503679 | 1866 | 270 | -54 | 434.3 | East Basalt
MRA7389 | 485978 | 4503403 | 1877 | 95 | -71 | 367.3 | East Basalt
MR7390 | 485977 | 4503375 | 1882 | 318 | -89 | 458.7 | East Basalt
MRA7391 | 486014 | 4503400 | 1881 | 89 | -64 | 458.7 | East Basalt
MR7392 | 485942 | 4503643 | 1862 | 324 | -90 | 458.7 | East Basalt
MRA7393 | 486032 | 4503679 | 1866 | 89 | -71 | 446.5 | East Basalt
MR7394 | 486014 | 4503647 | 1866 | 222 | -90 | 428.2 | East Basalt
MR7395 | 485898 | 4503766 | 1853 | 160 | -90 | 458.7 | East Basalt
MRA7396 | 485897 | 4503766 | 1853 | 271 | -50 | 434.3 | East Basalt
MRA7397 | 485950 | 4503679 | 1865 | 90 | -71 | 455.7 | East Basalt
MRA7398 | 485940 | 4503770 | 1861 | 93 | -75 | 458.7 | East Basalt
MR7399 | 485963 | 4503313 | 1891 | 20 | -90 | 458.7 | East Basalt
MRA7400 | 486085 | 4503463 | 1863 | 86 | -61 | 458.7 | East Basalt
MR7401 | 484703 | 4503584 | 1744 | 95 | -90 | 440.4 | Section 6
MRA7402 | 486114 | 4503312 | 1892 | 87 | -71 | 458.7 | East Basalt
MR7403 | 484746 | 4503525 | 1748 | 337 | -89 | 349.0 | Section 6
MRA7404 | 486115 | 4503583 | 1856 | 89 | -76 | 428.2 | East Basalt
MRA7405 | 484643 | 4499562 | 2261 | 265 | -60 | 397.8 | Trenton Canyon
MRA7406 | 485088 | 4507182 | 1601 | 89 | -56 | 352.0 | North Pits
MRA7407 | 485117 | 4507242 | 1601 | 89 | -64 | 352.0 | North Pits
DDH7408 | 484709 | 4503222 | 1729 | 96 | -74 | 1161.0 | Section 6
MRA7409 | 485347 | 4506758 | 1601 | 89 | -67 | 199.6 | North Pits
MRA7410 | 485533 | 4507181 | 1592 | 93 | -58 | 123.4 | North Pits
MRA7411 | 485390 | 4507660 | 1494 | 94 | -70 | 123.4 | North Pits
MRA7412 | 485354 | 4507640 | 1498 | 91 | -71 | 184.4 | North Pits
MRA7413 | 485265 | 4507553 | 1547 | 95 | -71 | 224.0 | North Pits
MRA7414 | 485311 | 4507525 | 1552 | 94 | -65 | 160.0 | North Pits
MRA7415 | 485407 | 4507456 | 1563 | 91 | -69 | 153.9 | North Pits
MRA7416 | 485503 | 4507303 | 1581 | 89 | -71 | 138.7 | North Pits
MRA7417 | 485524 | 4507242 | 1587 | 89 | -74 | 157.0 | North Pits
MRA7418 | 485525 | 4507211 | 1589 | 95 | -70 | 175.3 | North Pits

36

Hole ID | Easting | Northing | Elevation (m) | Azimuth (deg.) | Dip (deg.) | Length (m) | Area
MRA7419 | 485351 | 4507662 | 1498 | 93 | -69 | 153.9 | North Pits
MRA7420 | 484732 | 4503339 | 1731 | 94 | -50 | 403.9 | Section 6
MRA7421 | 484782 | 4503275 | 1744 | 92 | -56 | 344.4 | Section 6
MRA7422 | 484643 | 4499562 | 2261 | 268 | -72 | 413.0 | Trenton Canyon
MRA7424 | 485994 | 4503523 | 1848 | 90 | -76 | 458.7 | East Basalt
MRA7425 | 486032 | 4503524 | 1849 | 88 | -76 | 214.9 | East Basalt
MRA7426 | 484792 | 4503035 | 1760 | 92 | -61 | 342.9 | Section 6
MRA7427 | 484777 | 4503097 | 1755 | 95 | -46 | 355.1 | Section 6
MRA7428 | 484800 | 4503158 | 1757 | 90 | -61 | 410.0 | Section 6
MRA7429 | 484766 | 4503218 | 1744 | 89 | -63 | 385.6 | Section 6
MRA7430 | 486115 | 4503524 | 1857 | 94 | -77 | 367.3 | East Basalt
MRA7431 | 486074 | 4503521 | 1847 | 94 | -77 | 367.3 | East Basalt
MRA7432 | 484916 | 4502969 | 1784 | 90 | -52 | 403.9 | Section 6
MRA7433 | 484991 | 4502966 | 1803 | 87 | -52 | 443.5 | Section 6
MRA7434 | 486155 | 4503522 | 1871 | 92 | -76 | 367.3 | East Basalt
MRA7435 | 485087 | 4502961 | 1796 | 89 | -52 | 367.3 | Section 6
MR7436 | 484496 | 4499528 | 2257 | 92 | -90 | 397.8 | Trenton Canyon
MRA7437 | 484496 | 4499528 | 2257 | 271 | -76 | 397.8 | Trenton Canyon
MRA7438 | 484471 | 4499498 | 2256 | 300 | -89 | 397.8 | Trenton Canyon
MRA7439 | 484525 | 4499591 | 2261 | 275 | -86 | 397.8 | Trenton Canyon
MRA7440 | 484637 | 4499592 | 2261 | 266 | -68 | 397.8 | Trenton Canyon
MRA7441 | 484939 | 4502886 | 1803 | 92 | -72 | 367.3 | Section 6
MRA7442 | 485008 | 4502883 | 1819 | 92 | -67 | 397.8 | Section 6
MRA7443 | 484564 | 4499626 | 2262 | 274 | -66 | 245.4 | Trenton Canyon
MRA7444 | 483967 | 4498358 | 2446 | 75 | -75 | 306.3 | Trenton Canyon
MRA7445 | 483967 | 4498358 | 2446 | 64 | -43 | 306.3 | Trenton Canyon
MRA7446 | 483934 | 4498429 | 2447 | 67 | -76 | 294.1 | Trenton Canyon
MRA7447 | 483935 | 4498430 | 2447 | 64 | -44 | 306.3 | Trenton Canyon
MRA7448 | 484707 | 4503371 | 1727 | 90 | -50 | 341.4 | Section 6
MRA7449 | 487368 | 4504357 | 1895 | 268 | -81 | 352.0 | Valmy
MRA7450 | 485085 | 4499301 | 2175 | 235 | -72 | 458.7 | Trenton Canyon
MRA7451 | 487947 | 4504654 | 1969 | 272 | -70 | 355.1 | Cross Fire
MRA7454 | 487885 | 4504714 | 1922 | 269 | -66 | 336.8 | Cross Fire
MRA7455 | 487875 | 4504801 | 1891 | 270 | -65 | 367.3 | Cross Fire
MRA7457 | 487709 | 4505414 | 1770 | 269 | -66 | 312.4 | Cross Fire
MRA7458 | 484888 | 4499590 | 2140 | 273 | -64 | 367.3 | Trenton Canyon
MRA7459 | 487589 | 4505414 | 1744 | 272 | -65 | 275.8 | Cross Fire
MR7460 | 487576 | 4505657 | 1712 | 132 | -89 | 275.8 | Cross Fire
MRA7461 | 484625 | 4499615 | 2262 | 270 | -81 | 458.7 | Trenton Canyon
MRA7462 | 484763 | 4499363 | 2262 | 92 | -60 | 214.9 | Trenton Canyon

37

Hole ID | Easting | Northing | Elevation (m) | Azimuth (deg.) | Dip (deg.) | Length (m) | Area
MRA7463 | 484794 | 4499503 | 2211 | 272 | -66 | 123.4 | Trenton Canyon
MRA7464 | 484794 | 4499503 | 2210 | 274 | -46 | 123.4 | Trenton Canyon
MRA7465 | 484783 | 4499523 | 2209 | 271 | -65 | 184.4 | Trenton Canyon
MRA7466 | 485006 | 4502791 | 1828 | 90 | -60 | 306.3 | Section 6
MRA7467 | 484816 | 4499465 | 2210 | 231 | -45 | 123.4 | Trenton Canyon
MR7468 | 484758 | 4502888 | 1757 | 56 | -89 | 349.0 | Section 6
MRA7470 | 484889 | 4499437 | 2187 | 271 | -66 | 184.4 | Trenton Canyon
MRA7471 | 484889 | 4499437 | 2187 | 269 | -45 | 184.4 | Trenton Canyon
MRA7475 | 484794 | 4499589 | 2178 | 266 | -64 | 123.4 | Trenton Canyon
MRA7476 | 484934 | 4502794 | 1810 | 93 | -71 | 342.9 | Section 6
MRA7477 | 484882 | 4502885 | 1787 | 90 | -71 | 367.3 | Section 6
MRA7479 | 484948 | 4499531 | 2134 | 267 | -65 | 184.4 | Trenton Canyon
MRA7481 | 485074 | 4502763 | 1834 | 92 | -72 | 367.3 | Section 6
MRA7482 | 484879 | 4502794 | 1794 | 90 | -71 | 390.1 | Section 6
MRA7485 | 484675 | 4499103 | 2394 | 275 | -65 | 367.3 | Trenton Canyon
MRA7486 | 484645 | 4498982 | 2389 | 273 | -54 | 275.8 | Trenton Canyon
MRA7487 | 484617 | 4498948 | 2386 | 275 | -55 | 260.6 | Trenton Canyon
MRA7488 | 484617 | 4498948 | 2386 | 279 | -69 | 260.6 | Trenton Canyon
MR7492 | 484704 | 4503370 | 1727 | 35 | -89 | 289.6 | Section 6
MRA7498 | 484776 | 4503096 | 1755 | 93 | -76 | 332.2 | Section 6
MRA7499 | 484911 | 4503006 | 1780 | 93 | -46 | 275.8 | Section 6
MR7500 | 485167 | 4506690 | 1626 | 0 | -90 | 560.8 | Mackay
MR7501 | 484123 | 4507499 | 1646 | 0 | -90 | 426.7 | Mackay
MRA7503 | 484881 | 4502762 | 1796 | 88 | -73 | 367.3 | Section 6
MRA7504 | 484879 | 4502639 | 1797 | 92 | -74 | 367.3 | Section 6

38