EX-10.1 2 ex10-1.htm

PROTECTED SENSITIVE

TASK ORDER AGREEMENT FOR

SMALL SCALE SITES REMEDIATION PACKAGE
# 03*

TASK ORDER#: 541369

BETWEEN

CANADIAN NUCLEAR LABORATORIES LTD. /
LABORATOIRES NUCLÉAIRES CANADIENS LTÉE.

AND

PERMA-FIX CANADA INC.

*INFORMATION IN THIS DOCUMENT HAS BEEN EXCLUDED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 1 |

PROTECTED SENSITIVE

1. | Contract Title | SMALL SCALE SITES REMEDIATION PACKAGE # 02
2. | Task Order Execution Date | April 30, 2019 | 3. | Task Order No. Contractor shall use for all invoicing | 541369
4. | Framework Reference | 507595 | 5. | The Contract Type is: | Fixed Price
6. | Control Order No. | Not Applicable | 7. | The Task Order Price is: | $11,494,654.34
8. | Contractor HST# |  | 9. | Currency is: | Canadian
10. | The Site is: | Municipality of Port Hope, Ontario | 11. | Price Schedule is provided in SCHEDULE 2
12. | The Schedule and Key Dates : | Per Schedule 3 |  |  |
|  | The agreed Work Schedule is provided in Schedule 3

| 13. | The Task Order Term is as set out below:
| a) | The Task Order Effective Date is: | Upon Execution | b) | The Task Order Completion date is: | December 16, 2019

14. | Warranty Period | 12 Months for commercial/residential properties from issue of CNL’s Certificate of Substantial Performance, and 24 Months for municipal properties from issue of CNL’s Certificate of Substantial Performance. In accordance to MPH By-Law 50-2014 Phase 2 in Standard Operating Guideline Section 2.9
15. | Addresses for Notices under this Task Order

a) CNL Representative(s) | b) Contractor Representative
CNL at: Project Lead – Scott Schumacher Email: scott.schumacher@cnl.ca Cell:905-376-8913 With copy to: Tina Burghardt – tina.burghardt@cnl.ca | Contractor at [Address] Email: John Kelly, jkelly@perma-fix.com Cell: 865-313-3107 With copy to: Ben Nacarrato, bnaccarato@perma-fix.com
c) CNL Contracting Officer | d) Contractor’s Supervisor
CNL at: Yvonne Rogers Email: yvonne.rogers@cnl.ca Tel: 905-885-8830, ext 45649 | Contractor at [Address] Email: Ray Cyr, rcyr@lakeland-multitrade.com Cell: 905-375-8051

CNL Task Order No. 541369 | 2 |

PROTECTED SENSITIVE

16. | Other communication: | Not Applicable
17. | Periods of Reply | As specified in Schedule 1 and the Framework Agreement

This Task Order is issued pursuant to, and fully incorporates, the terms and conditions set forth within the governing Framework Agreement for Environmental Remediation Construction Works, No. 507935, with a Contract Date of 2017 October 18, by and between Canadian Nuclear Laboratories (CNL) and Milestone Environmental Contracting Inc.

Part 1: Description of the Work/Services

18. | Description of scope of Work (Schedule 1) | In summary, Task Order Agreement is issued for remediation and construction work at specific sites within the Municipality of Port Hope, Ontario. These sites have been impacted with industrial waste and low-level radioactive waste (“LLRW”). The scope of work is summarized as follows (the “Work”):

|  | 1. | Remediation of a portion of the properties as per Specifications and Drawings Group 1B, 1C, !G, 1H and 1I (31 properties in total)
|  | 2. | The safe removal, collecting and verification of soil know to contain LLRW
|  | 3. | Transportation of waste along designated routes to the Long-Term Waste Management Facility (LTWMF) in the Municipality of Port Hope.
|  | 4. | Rehabilitation and Reconstruction/Restoration as per Specifications

|  | (Refer to Schedule 1)
19. | Drawings & Documents | Refer to Schedule 1
20. | Deliverables | As set out Schedule 1
21. | Exclusions and Battery limits | None
22. | Assumptions and Risk Register | As set out in Framework Agreement GC 6.1
23. | Constraints or interdependencies | Waste deliveries to the PH LTWMF must be coordinated with the LTWMF Contractor and CNL. This includes respective SOP’s and Owner’s access agreements between CNL and the Owners. As set out Schedule 1 – hours of operations.
24. | CNL provided items and Rely-Upon Information | Refer to Schedule 1 (as referred to in Appendix D of the RFP)

CNL Task Order No. 541369 | 3 |

PROTECTED SENSITIVE

Part 2: Key Data

25. | Task Order Limits of Liability | The Contractor’s limit of liability for this Task Order is: | Task Order Price

|  | All in accordance with the provisions of the GC 11.4.2 of the Framework Agreement.
26. | Bonds and Guarantees | Performance Bond in accordance with GC 2.9 of the Framework Agreement in the amount of 50% of the Task Order Price. Labour & Material Payment Bond in accordance with GC 2.9 of the Framework Agreement in the amount of 50% of the Task Order Price (at CNL’s request and discretion, to be determined upon award).
27. | Insurances | Insurance to be furnished in accordance with GC 10.1 of the Framework Agreement and as set out below:
|  | **Commercial General Liability coverage required: $ 5,000,000
|  | Automobile and Transportation Liability Insurance coverage required: $ 3,000,000
|  | Contractor’s Pollution Liability Insurance coverage required: $ 5,000,000
|  | Contractors Equipment Insurance (sufficient to cover all property, tools and equipment of the contractor)
|  | CNL AECL, and the Municipality shall appear as additional insureds and the policy will provide coverage for non-owned auto (if not otherwise covered below), mobile equipment, cross liability, blanket contractual liability, and an agreement by underwriters to waive rights of recourse against CNL, AECL and the Municipality. Coverage in the amount set out in this Task Order per occurrence will be maintained.
|  | Prior to award, the Contractor will have to add the Property Owner’s name on their Insurance Certificate and/or, if applicable the mortgagee’s name, CNL’s will provide all the information.
|  | Insurance to be provided and shall remain in effect in accordance with the terms of the Framework Agreement, Part 10.
28. | Incentives | Not applicable
29. | Payment | In accordance with the agreed Schedule of Values forming part of Schedule 2 and in accordance with the Framework Agreement, Article 5 Payment and Invoicing
30. | Contractual Holdback | The amount of Contractual Holdback applicable to this Task Order is: | 10% in accordance with the Framework Agreement, Article 5.1(a)
31. | Delay Liquidated Damages (if applicable) | Delay Liquidated Damages are: $5,000 per Working Day from Completion The maximum Delay Liquidated Damages payable is: 10% of the Task Order Price
32. | The Task Order Special Conditions are: |
33. | Adjacent Operators | Not Applicable

CNL Task Order No. 541369 | 4 |

PROTECTED SENSITIVE

Part 3: Contract Execution Requirements

34. | HSSEQ Requirements | As specified in Schedule 1
35. | Quality Designation of Work | As specified in Schedule 1
36. | Training and Security | As specified in Schedule 1
37. | Codes, Standards & Regulatory Requirements | As specified in Schedule 1
38. | Performance, Communication and Reporting | As specified in Schedule 8 – STAKEHOLDER ENGAGEMENT
39. | Responsibilities | As specified in the Framework Agreement
40. | Reporting Requirements | As specified in Schedule 1

Part 4: Schedules
Relevant documents to this Task Order.

| ● | Schedule 1: Technical Statement of Work;
| ● | Schedule 2: Price Schedule;
| ● | Schedule 3: Work Schedule;
| ● | Schedule 4: Special Conditions, Contractor’s Methodology
| ● | Schedule 5: Subcontractors;
| ● | Schedule 6: Field Equipment List;
| ● | Schedule 7: Aboriginal and/or Local, Small and Medium-sized Business Engagement Plan
| ● | Schedule 8 Contractor Stakeholder Engagement

Part 5: Execution of Task Order |
Canadian Nuclear Laboratories | Perma-Fix Canada Inc.

Name/Position: | Mark Lesinski/President & CEO |  | Name/Position: | Ben Naccarato, Vice President of Finance
Signature: | /s/Mark Lesinski |  | Signature: | /s/Ben Naccarato
Date: | 6th May 2019 |  | Date: | 4-30-2019
Name/Position: | Monica Steedman/VP Finance & CFO |  | Name/Position: | PERMA-FIX DOES NOT REQUIRE A SECOND SIGNATORY
Signature: | /s/Monica Steedman |  | Signature: |
Date: | 6th May 2019 |  | Date: |

CNL Task Order No. 541369 | 5 |

PROTECTED SENSITIVE

SCHEDULE 1 – TECHNICAL STATEMENT OF WORK

CNL Task Order No. 541369 | 1 | Schedule 1

PROTECTED SENSITIVE

The Technical Statement of Work comprise the following:

4501-01340-TS-001, latest revision – Construction Package 3 Issued for Construction Specifications – Design Groups 1B, 1C, 1G, 1H and 1I in Port Hope, ON prepared by AMEC Foster Wheeler – .

4501-508120-MD-001, latest revision – Construction Package 3 Issued for Construction Drawings – Design Group 1B prepared by AMEC Foster Wheeler

4501-508120-MD-002, latest revision – Construction Package 3 Issued for Construction Drawings – Design Group 1G prepared by AMEC Foster Wheeler

4501-508120-MD-003, latest revision – Construction Package 3 Issued for Construction Drawings – Design Group 1C prepared by AMEC Foster Wheeler

4501-508120-MD-004, latest revision – Construction Package 3 Issued for Construction Drawings – Design Group 1H prepared by AMEC Foster Wheeler

4501-508120-MD-005, latest revision – Construction Package 3 Issued for Construction Drawings – Design Group 1I prepared by AMEC Foster Wheeler

In addition to the above, the following documents are hereby incorporated into and form part of this Task Oder by reference:

CNL Task Order No. 541369 | 2 | Schedule 1

PROTECTED SENSITIVE

SCHEDULE 2 – PRICE SCHEDULE

CNL Task Order No. 541369 | 1 | Schedule 2

PROTECTED SENSITIVE

Task Order Price

1. Unit Price quantities shown are estimates only. The associated unit prices will be used to calculate the actual value of Work performed. CNL makes no guarantee as to the quantities of Work to be actually performed by the Selected Proponent.

2. All lump sum pricing and unit pricing shall be firm, fixed and not subject to adjustment for the duration of the Task Order Term.

3. Note that where the items on the Pricing Form tab are inconsistent with the Measurement Procedures set out in the various Sections of the Specifications, the Pricing Form shall govern and take precedence over the Specifications.

4. Pricing for Labour Rates and Equipment Rates are in firm Canadian funds and will be adjusted annually in accordance with the Consumer Price Index (CPI) for the Province of Ontario (December of previous year to January of current year) using the following formula:

(December- current year/January - previous year)*100-100

The first annual adjustment of rates as set out above shall occur no sooner than eighteen months after the Effective Date.

5. Note that all Laboratory Analysis costs incurred by the Contractor for this project will be reimbursed at cost with no Contractor mark-up of any kind. Contractor’s invoices for third party laboratory costs shall include the actual costs incurred (not to exceed the Ceiling Price per Unit set out in the Pricing Form (for each chemical analysis performed) and shall be supported by the accredited laboratory’s ac

tual invoices paid by the Contractor for this project.

CNL Task Order No. 541369 | 2 | Schedule 2

PROTECTED SENSITIVE

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 3 | Schedule 2

PROTECTED SENSITIVE

|  | Specification Reference |  | Description |  | Unit of Measure |  | Estimated Quantity |  |  | Price per Unit |  |  | Total Price |
Group B - General Requirements |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 02 61 00 |  | Mobilization and Project Startup |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
2 |  | 02 61 00 |  | Demobilization and Project Closeout |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
3 |  | 01 31 19 |  | Project Meetings |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
4 |  | 01 32 00 |  | Construction Progress Documentation |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
5 |  | 01 32 16 |  | Construction Progress Schedule |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
6 |  | 01 35 29 |  | Health and Safety Plan |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
7 |  | 01 35 29 |  | Implementation of Health and Safety - All Sites |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
8 |  | 01 35 30 |  | Radiation Protection Plan - All Sites |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
9 |  | 01 35 30 |  | Implementation of Radiation Protection - All Sites |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
10 |  | 01 35 43 |  | Environmental Protection Manual and Dust Management Plan - All Sites |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
11 |  | 01 35 43 |  | Implementation of Environmental Protection and Dust Management - All Sites |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
12 |  | 01 45 00 |  | Quality Assurance Plan |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
13 |  | 01 45 00 |  | Implementation of QA/QC - All Sites |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
14 |  | 01 51 00 |  | Provision and Maintenance of Temporary Utilities - (Contractor Use) |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
15 |  | 01 52 00 |  | Provision and Construction Facilities - All Sites |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 4 | Schedule 2

PROTECTED SENSITIVE

16 |  | 02 61 00 |  | Permitting as per OBC and MPH SOP-SOG, OMOECC, CN/CP - all sites |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
17 |  |  |  | Traffic Control - All sites |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
18 |  | 01 33 00 |  | All Other Submittals |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
19 |  | 01 14 00 |  | Site Security |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
20 |  |  |  | Bonding & Insurance |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
21 |  | 01 14 00 |  | Training and Security Clearance |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
22 |  | 01 78 00 |  | Closeout Submittal |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
23 |  | 01 56 00 |  | Supply, Install, Maintain, and Remove Sediment Erosion Control fencing |  | Linear meters |  |  | 95 |  |  | $ | *** |  |  | $ | *** |
24 |  | 01 56 00 |  | Supply, Install, Maintain, and Remove - Perimeter Safety Fencing |  | Linear meters |  |  | 185 |  |  | $ | *** |  |  | $ | *** |
25 |  | 02 61 00 |  | Supply, Install, Maintain and Remove Access Gates as shown |  | each |  |  | 4 |  |  | $ | *** |  |  | $ | *** |
26 |  | See Figure attached |  | Tree Protection Fencing |  | Linear meters |  |  | 40 |  |  | $ | *** |  |  | $ | *** |
Total Price - General Requirements | $ | *** |

Group B Requirements - 24 Smith Street

Removals |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 02 61 00 |  | Pre-construction Property Condition Assessment |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
2 |  | 02 61 00 |  | Complete gamma survey and XRF scan of completed excavation surface |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
3 |  | 02 61 00 |  | Collection of soil sample for signature COPCs and the reporting of results following Laboratory Analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 5 | Schedule 2

PROTECTED SENSITIVE

4 |  | 02 61 00 |  | Laboratory Analysis of soil sample for signature COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
5 |  | 02 61 00 |  | Collection of soil sample for secondary COPCs and the reporting of results following laboratory analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
6 |  | 02 61 00 |  | Laboratory Analysis of composite soil sample for secondary COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
7 |  | 02 61 00 |  | Preparation and Submission of Verification Documentation |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
8 |  | 02 41 16 |  | Demolish Existing Site Structures that require removal, verify not radiologically impacted and dispose off site a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
9 |  | 02 41 13 |  | Concrete Sidewalk Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq. meters |  |  | 12 |  |  | $ | *** |  |  | $ | *** |
10 |  | 02 41 13 |  | Concrete Stair Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
11 |  | 02 61 00 |  | Remove and Dispose of Trees, shrubs, hedges, and all other plants above ground, verify not radiological impacted and dispose offsite at a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
12 |  | 02 61 00 |  | Remove all other surface landscape features, relocate offsite to secure location for future re-installment |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
13 |  | 02 61 00 |  | Excavate, stockpile, load, haul and dispose at LTWMF Facility Contaminated soil and tree roots |  | cubic meters |  |  | 10 |  |  | $ | *** |  |  | $ | *** |
14 |  |  |  | Secondary Excavation (if required) |  | cubic meters |  |  |  |  |  | $ | *** |  |  |  |  |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 6 | Schedule 2

PROTECTED SENSITIVE

Earthworks |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 31 00 01 |  | Supply, place, compact and grade clean imported fill per MPH SOP/SOGs (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 2 |  |  | $ | *** |  |  | $ | *** |
2 |  | 31 00 01 |  | Supply, place, compact and grade Granular A (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 4 |  |  | $ | *** |  |  | $ | *** |
3 |  | 31 00 01 |  | Supply, place, compact and grade Granular B (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 4 |  |  | $ | *** |  |  | $ | *** |
4 |  | 31 00 01 |  | Supply, place, and grade Topsoil |  | cubic meters |  |  | 5 |  |  | $ | *** |  |  | $ | *** |
Site Restoration |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | as per Drawings |  | Supply and Place Concrete Sidewalk as per specifications |  | sq. meters |  |  | 12 |  |  | $ | *** |  |  | $ | *** |
2 |  | 31 32 50 |  | Water management, sampling, transportation, and disposal at LTMWF |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
3 |  | as per Drawings |  | Supply and Place concrete stairs as per specifications |  | treads |  |  | 9 |  |  | $ | *** |  |  | $ | *** |
4 |  | 32 90 00 |  | Landscape Restoration |  | Allowance |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
Total Price - 24 Smith | $ | *** |

Group B Requirements - 26 Smith Street

Removals |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 02 61 00 |  | Pre-construction Property Condition Assessment |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
2 |  | 02 61 00 |  | Complete gamma survey and XRF scan of completed excavation surface |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 7 | Schedule 2

PROTECTED SENSITIVE

3 |  | 02 61 00 |  | Collection of soil sample for signature COPCs and the reporting of results following Laboratory Analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
4 |  | 02 61 00 |  | Laboratory analysis of soil sample for signature COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
5 |  | 02 61 00 |  | Collection of soil sample for secondary COPCs and the reporting of results following laboratory analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
6 |  | 02 61 00 |  | Laboratory analysis of composite soil sample for secondary COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
7 |  | 02 61 00 |  | Preparation and submission of Verification Documentation |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
8 |  | 02 41 13 |  | Gravel Driveway Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 9 |  |  | $ | *** |  |  | $ | *** |
9 |  | 02 41 16 |  | Demolish Existing Site Structures that require removal, verify not radiologically impacted and dispose off site a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
10 |  | 02 41 13 |  | Concrete Sidewalk Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq. meters |  |  | 23 |  |  | $ | *** |  |  | $ | *** |
11 |  | 02 41 13 |  | Concrete Patio Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq. meters |  |  | 40 |  |  | $ | *** |  |  | $ | *** |
12 |  | 31 11 00 |  | Remove and Dispose of Trees, shrubs, hedges, and all other plants above ground, verify not radiological impacted and dispose offsite at a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 8 | Schedule 2

PROTECTED SENSITIVE

13 |  | 02 61 00 |  | Remove all other surface landscape features, relocate off-site to secure location for future re-installment |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
14 |  | 02 61 00 |  | Excavate, stockpile, load, haul and dispose at LTWMF Facility Contaminated soil and tree roots |  | cubic meters |  |  | 60 |  |  | $ | *** |  |  | $ | *** |
15 |  |  |  | Secondary Excavation (if required) |  | cubic meters |  |  |  |  |  | $ | *** |  |  |  |  |
Earthworks |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 31 00 01 |  | Supply, place, compact and grade clean imported fill per MPH SOP/SOGs (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 40 |  |  | $ | *** |  |  | $ | *** |
2 |  | 31 00 01 |  | Supply, place, compact and grade Granular A (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 20 |  |  | $ | *** |  |  | $ | *** |
3 |  | 31 00 01 |  | Supply, place, compact and grade Granular B (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 20 |  |  | $ | *** |  |  | $ | *** |
4 |  | 31 00 01 |  | Supply, place, and grade Topsoil |  | cubic meters |  |  | 20 |  |  | $ | *** |  |  | $ | *** |
Site Restoration |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | as per Drawings |  | Supply and Install covered porch as shown including all footings, etc., inluding all permits |  | square meters |  |  | 22 |  |  | $ | *** |  |  | $ | *** |
2 |  | as per Drawings |  | Supply, Place, Gravel Driveway as per specifications |  | square meters |  |  | 9 |  |  | $ | *** |  |  | $ | *** |
2 |  | as per Drawings |  | Supply and Place Concrete Sidewalk as per specifications |  | square meters |  |  | 23 |  |  | $ | *** |  |  | $ | *** |
3 |  | as per Drawings |  | Supply and Place Concrete Patio as per specifications |  | square meters |  |  | 40 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 9 | Schedule 2

PROTECTED SENSITIVE

4 |  | as per Drawings |  | Supply and Place concrete stairs as per specifications |  | treads |  |  | 10 |  |  | $ | *** |  |  | $ | *** |
5 |  | 32 90 00 |  | Landscape Restoration |  | Allowance |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
6 |  | 31 32 50 |  | Water management, sampling, transportation, and disposal at LTMWF |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
7 |  | as per Drawings |  | Supply and Place Fence |  | Linear meters |  |  | 25.00 |  |  | $ | *** |  |  | $ | *** |
Total Price - 26 Smith | $ | *** |

Group B Requirements - 28 Smith Street

Removals |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 02 61 00 |  | Pre-construction Property Condition Assessment |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
2 |  | 02 61 00 |  | Complete gamma survey and XRF scan of completed excavation surface |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
3 |  | 02 61 00 |  | Collection of soil sample for signature COPCs and the reporting of results following Laboratory Analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
4 |  | 02 61 00 |  | Laboratory analysis of soil sample for signature COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
5 |  | 02 61 00 |  | Collection of soil sample for secondary COPCs and the reporting of results following laboratory analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
6 |  | 02 61 00 |  | Laboratory analysis of composite soil sample for secondary COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
7 |  | 02 61 00 |  | Preparation and submission of Verification Documentation |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
8 |  | 02 41 16 |  | Demolish Existing Site Structures that require removal, verify not radiologically impacted and dispose off site a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 10 | Schedule 2

PROTECTED SENSITIVE

9 |  | 02 41 13 |  | Concrete Sidewalk Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | square meters |  |  | 23 |  |  | $ | *** |  |  | $ | *** |
10 |  | 02 41 13 |  | Concrete Patio Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | square meters |  |  | 40 |  |  | $ | *** |  |  | $ | *** |
11 |  | 02 41 13 |  | Retaining Wall Removal - verify not radiologically impacted, offsite disposal at a licensed receiving facility, include all necessary support and bracing as required |  | Lump sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
12 |  | 02 41 13 |  | Concrete Stair Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
13 |  | 31 11 00 |  | Remove and Dispose of Trees, shrubs, hedges, and all other plants above ground, verify not radiological impacted and dispose offsite at a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
14 |  |  |  | Remove all other surface landscape features, relocate offsite to secure location for future re-installment |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
15 |  |  |  | Removal of Outbuilding Contents, storage in secured area, and return of objects upon restoration |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
16 |  | 02 61 00 |  | Excavate, stockpile, load, haul and dispose at LTWMF Facility Contaminated soil and tree roots |  | cubic meters |  |  | 195 |  |  | $ | *** |  |  | $ | *** |
17 |  |  |  | Secondary Excavation (if required) |  | cubic meters |  |  |  |  |  | $ | *** |  |  |  |  |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 11 | Schedule 2

PROTECTED SENSITIVE

Earthworks |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 31 00 01 |  | Supply, place, compact and grade clean imported fill per MPH SOP/SOGs (based on 2 tonnes per cubic meter) |  | Tonnes |  |  | 140 |  |  | $ | *** |  |  | $ | *** |
2 |  | 31 00 01 |  | Supply, place, compact and grade Granular A (based on 2 tonnes per cubic meter) |  | Tonnes |  |  | 50 |  |  | $ | *** |  |  | $ | *** |
3 |  | 31 00 01 |  | Supply, place, compact and grade Granular B (based on 2 tonnes per cubic meter) |  | Tonnes |  |  | 50 |  |  | $ | *** |  |  | $ | *** |
4 |  | 31 00 01 |  | Supply, place, and grade Topsoil |  | cubic meters |  |  | 75 |  |  | $ | *** |  |  | $ | *** |
Site Restoration |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | as per Drawings |  | Supply and Install detached Garage as shown including all footings, floors etc. |  | square meters |  |  | 56 |  |  | $ | *** |  |  | $ | *** |
2 |  | as per Drawings |  | Supply and Place Concrete Sidewalk as per specifications |  | square meters |  |  | 23 |  |  | $ | *** |  |  | $ | *** |
3 |  | as per Drawings |  | Supply and Place Concrete Patio as per specifications |  | square meters |  |  | 40 |  |  | $ | *** |  |  | $ | *** |
4 |  | as per Drawings |  | Supply and install Covered Porch (Rear) as shown including all permits |  | square meters |  |  | 22 |  |  | $ | *** |  |  | $ | *** |
5 |  | as per Drawings |  | Supply and Place Retaining Wall as per specifications |  | Linear meters |  |  | 5 |  |  | $ | *** |  |  | $ | *** |
6 |  | as per Drawings |  | Supply and Place concrete stairs as per specifications |  | treads |  |  | 10 |  |  | $ | *** |  |  | $ | *** |
7 |  | 32 90 00 |  | Landscape Restoration |  | Allowance |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
8 |  | 31 32 50 |  | Water management, sampling, transportation, and disposal at LTMWF |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
Total Price - 28 Smith | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 12 | Schedule 2

PROTECTED SENSITIVE

Group B Requirements - 30 Smith Street

Removals |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 02 61 00 |  | Pre-construction Property Condition Assessment |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
2 |  | 02 61 00 |  | Complete gamma survey and XRF scan of completed excavation surface |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
3 |  | 02 61 00 |  | Collection of soil sample for signature COPCs and the reporting of results following Laboratory Analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
4 |  | 02 61 00 |  | Laboratory analysis of soil sample for signature COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
5 |  | 02 61 00 |  | Collection of soil sample for secondary COPCs and the reporting of results following laboratory analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
6 |  | 02 61 00 |  | Laboratory analysis of composite soil sample for secondary COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
7 |  | 02 61 00 |  | Preparation and submission of Verification Documentation |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
8 |  | 02 41 16 |  | Demolish existing Site structures that require removal, verify not radiologically impacted and dispose off site a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
9 |  | 02 41 13 |  | Gravel Driveway Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 7 |  |  | $ | *** |  |  | $ | *** |
10 |  | 02 41 13 |  | Concrete Sidewalk Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 14 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 13 | Schedule 2

PROTECTED SENSITIVE

11 |  | 02 41 13 |  | Paving stone / interlocking brick patio Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | square meters |  |  | 66 |  |  | $ | *** |  |  | $ | *** |
12 |  | 02 41 13 |  | Retaining Wall Removal - verify not radiologically impacted, offsite disposal at a licensed receiving facility, include all necessary support and bracing as required |  | Lump sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
13 |  | 02 41 13 |  | Concrete Stair Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
14 |  | 02 41 13 |  | Remove existing fence, verify not radiologically impacted and dispose offiste at licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
15 |  | 31 11 00 |  | Remove and Dispose of Trees, shrubs, hedges, and all other plants above ground, verify not radiological impacted and dispose offsite at a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
16 |  |  |  | Remove all other surface landscape features, relocate offsite to secure location for future re-installment |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
17 |  |  |  | Removal of Outbuilding Contents, storage in secured area, and return of objects upon restoration |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
18 |  | 02 61 00 |  | Excavate, stockpile, load, haul and dispose at LTWMF Facility Contaminated soil and tree roots |  | cubic meters |  |  | 425 |  |  | $ | *** |  |  | $ | *** |
19 |  |  |  | Secondary Excavation (if required) |  | cubic meters |  |  |  |  |  | $ | *** |  |  |  |  |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 14 | Schedule 2

PROTECTED SENSITIVE

Earthworks |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 31 00 01 |  | Supply, place, compact and grade clean imported fill per MPH SOP/SOGs (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 510 |  |  | $ | *** |  |  | $ | *** |
2 |  | 31 00 01 |  | Supply, place, compact and grade Granular A (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 80 |  |  | $ | *** |  |  | $ | *** |
3 |  | 31 00 01 |  | Supply, place, compact and grade Granular B (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 80 |  |  | $ | *** |  |  | $ | *** |
4 |  | 31 00 01 |  | Supply, place, and grade Topsoil |  | cubic meters |  |  | 90 |  |  | $ | *** |  |  | $ | *** |
Site Restoration |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | as per Drawings |  | Supply and Install Storage Sheds as shown including all footings, floors etc. |  | each |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
2 |  | as per Drawings |  | Supply, Place, Gravel Driveway as per specifications |  | square meters |  |  | 7 |  |  | $ | *** |  |  | $ | *** |
3 |  | as per Drawings |  | Supply and Place Concrete Sidewalk as per specifications |  | square meters |  |  | 14 |  |  | $ | *** |  |  | $ | *** |
4 |  | as per Drawings |  | Supply, Place Covered Porch (Front) as shown including all permits |  | square meters |  |  | 23 |  |  | $ | *** |  |  | $ | *** |
5 |  | 06 15 00 |  | Supply, Place Wooden deck (Rear) as shown including all permits |  | square meters |  |  | 18 |  |  | $ | *** |  |  | $ | *** |
6 |  | as per Drawings |  | Supply and Place Paving Stone / Interlocking Brick Patio Patio as per specifications |  | square meters |  |  | 66 |  |  | $ | *** |  |  | $ | *** |
7 |  | as per Drawings |  | Supply and Place Retaining Wall as per specifications |  | Linear meters |  |  | 25 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 15 | Schedule 2

PROTECTED SENSITIVE

8 |  | as per Drawings |  | Supply and Place concrete stairs as per specifications |  | treads |  |  | 6 |  |  | $ | *** |  |  | $ | *** |
9 |  | 31 32 50 |  | Water management, sampling, transportation, and disposal at LTMWF |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
10 |  | as per Drawings |  | Supply and Place Fence |  | Linear meters |  |  | 26 |  |  | $ | *** |  |  | $ | *** |
11 |  | 32 90 00 |  | Landscape Restoration |  | Allowance |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
Total Price - 30 Smith | $ | *** |
Total Remediation, Earthworks and Restoration Only | $ | *** |

|  | Specification Reference |  | Description |  | Unit of Measure |  | Estimated Quantity |  |  | Price per Unit |  |  | Total Price |
Group C - General Requirements |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 02 61 00 |  | Mobilization and Project Startup |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
2 |  | 02 61 00 |  | Demobilization and Project Closeout |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
3 |  | 01 31 19 |  | Project Meetings |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
4 |  | 01 32 00 |  | Construction Progress Documentation |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
5 |  | 01 32 16 |  | Construction Progress Schedule |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
6 |  | 01 35 29 |  | Health and Safety Plan |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
7 |  | 01 35 29 |  | Implementation of Health and Safety - All Sites |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
8 |  | 01 35 30 |  | Radiation Protection Plan - All Sites |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
9 |  | 01 35 30 |  | Implementation of Radiation Protection - All Sites |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
10 |  | 01 35 43 |  | Environmental Protection Manual and Dust Management Plan - All Sites |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 16 | Schedule 2

PROTECTED SENSITIVE

11 |  | 01 35 43 |  | Implementation of Environmental Protection and Dust Management - All Sites |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
12 |  | 01 45 00 |  | Quality Assurance Plan |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
13 |  | 01 45 00 |  | Implementation of QA/QC - All Sites |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
14 |  | 01 51 00 |  | Provision and Maintenance of Temporary Utilities - (Contractor Use) |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
15 |  | 01 52 00 |  | Provision and Construction Facilities - All Sites |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
16 |  | 02 61 00 |  | Permitting as per OBC and MPH SOP-SOG, OMOECC, CN/CP - all sites |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
17 |  |  |  | Traffic Control - All sites |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
18 |  | 01 33 00 |  | All Other Submittals |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
19 |  | 01 14 00 |  | Site Security |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
20 |  |  |  | Bonding & Insurance |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
21 |  | 01 14 00 |  | Training and Security Clearance |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
22 |  | 01 78 00 |  | Closeout Submittal |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
23 |  | 01 56 00 |  | Supply, Install, Maintain, and Remove Sediment Erosion Control fencing |  | Linear meters |  |  | 165 |  |  | $ | *** |  |  | $ | *** |
24 |  | 01 56 00 |  | Supply, Install, Maintain, and Remove - Perimeter Safety Fencing |  | Linear meters |  |  | 330 |  |  | $ | *** |  |  | $ | *** |
25 |  | 02 61 00 |  | Supply, Install, Maintain and Remove Access Gates as shown |  | each |  |  | 6 |  |  | $ | *** |  |  | $ | *** |
26 |  | See Figure Attached |  | Tree Protection Fencing |  | Linear meters |  |  | 180 |  |  | $ | *** |  |  | $ | *** |
Total Price - General Requirements | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 17 | Schedule 2

PROTECTED SENSITIVE

Group C Requirements - 21 Elizabeth Street

Removals |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 02 61 00 |  | Pre-construction Property Condition Assessment |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
2 |  | 02 61 00 |  | Complete gamma survey and XRF scan of completed excavation surface |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
3 |  | 02 61 00 |  | Collection of soil sample for signature COPCs and the reporting of results following Laboratory Analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
4 |  | 02 61 00 |  | Laboratory Analysis of soil sample for signature COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
5 |  | 02 61 00 |  | Collection of soil sample for secondary COPCs and the reporting of results following laboratory analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
6 |  | 02 61 00 |  | Laboratory Analysis of composite soil sample for secondary COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
7 |  | 02 61 00 |  | Preparation and Submission of Verification Documentation |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
8 |  | 02 41 16 |  | Demolish Existing Site Structures that require removal, verify not radiologically impacted and dispose off site a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
9 |  | 02 41 13 |  | Gravel Driveway Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 11 |  |  | $ | *** |  |  | $ | *** |
10 |  | 02 41 13 |  | Concrete Sidewalk Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 9 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 18 | Schedule 2

PROTECTED SENSITIVE

11 |  | 02 41 13 |  | Remove existing fence, verify not radiologically impacted and dispose offiste at licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
12 |  | 02 61 00 |  | Remove and Dispose of Trees, shrubs, hedges, and all other plants above ground, verify not radiological impacted and dispose offsite at a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
13 |  | 02 61 00 |  | Remove all other surface landscape features, relocate offsite to secure location for future re-installment |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
14 |  | 02 61 00 |  | Removal of Outbuilding Contents, storage in secured area, and return of objects upon restoration |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
15 |  | 02 61 00 |  | Excavate, stockpile, load, haul and dispose at LTWMF Facility Contaminated soil and tree roots |  | cubic meters |  |  | 165 |  |  | $ | *** |  |  | $ | *** |
16 |  |  |  | Secondary Excavation (if required) |  | cubic meters |  |  |  |  |  | $ | *** |  |  |  |  |
Earthworks |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 31 00 01 |  | Supply, place, compact and grade clean imported fill per MPH SOP/SOGs (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 120 |  |  | $ | *** |  |  | $ | *** |
2 |  | 31 00 01 |  | Supply, place, compact and grade Granular A (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 40 |  |  | $ | *** |  |  | $ | *** |
3 |  | 31 00 01 |  | Supply, place, compact and grade Granular B (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 40 |  |  | $ | *** |  |  | $ | *** |
4 |  | 31 00 01 |  | Supply, place, and grade Topsoil |  | cubic meters |  |  | 65 |  |  | $ | *** |  |  | $ | *** |
Site Restoration |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 19 | Schedule 2

PROTECTED SENSITIVE

1 |  | as per Drawings |  | Supply and Install shed as shown including all footings, etc., inluding all permits |  | square meters |  |  | 4 |  |  | $ | *** |  |  | $ | *** |
2 |  | as per Drawings |  | Supply and Place Gravel Drivway as per specifications |  | square meters |  |  | 11 |  |  | $ | *** |  |  | $ | *** |
3 |  | as per Drawings |  | Supply and Place Concrete Sidewalk as per specifications |  | square meters |  |  | 9 |  |  | $ | *** |  |  | $ | *** |
4 |  | 31 32 50 |  | Water management, sampling, transportation, and disposal at LTMWF |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
5 |  | 32 90 00 |  | Landscape Restoration |  | Allowance |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
6 |  | as per Drawings |  | Supply and Place Fence |  | Linear meters |  |  | 15.00 |  |  | $ | *** |  |  | $ | *** |
Total Price - 21 Elizabeth Street | $ | *** |

Group C Requirements - 11-15 Elizabeth Street

Removals |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 02 61 00 |  | Pre-construction Property Condition Assessment |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
2 |  | 02 61 00 |  | Complete gamma survey and XRF scan of completed excavation surface |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
3 |  | 02 61 00 |  | Collection of soil sample for signature COPCs and the reporting of results following Laboratory Analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
4 |  | 02 61 00 |  | Laboratory analysis of soil sample for signature COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
5 |  | 02 61 00 |  | Collection of soil sample for secondary COPCs and the reporting of results following laboratory analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 20 | Schedule 2

PROTECTED SENSITIVE

6 |  | 02 61 00 |  | Laboratory analysis of composite soil sample for secondary COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
7 |  | 02 61 00 |  | Preparation and submission of Verification Documentation |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
8 |  | 02 41 16 |  | Demolish Existing Site Structures that require removal, verify not radiologically impacted and dispose off site a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
9 |  | 02 41 13 |  | Concrete Sidewalk Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 5 |  |  | $ | *** |  |  | $ | *** |
10 |  | 02 41 13 |  | Gravel Driveway Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 7 |  |  | $ | *** |  |  | $ | *** |
11 |  | 02 41 13 |  | Remove existing fence, verify not radiologically impacted and dispose offiste at licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
12 |  | 02 41 13 |  | Concrete Stair Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
13 |  | 31 11 00 |  | Remove and Dispose of Trees, shrubs, hedges, and all other plants above ground, verify not radiological impacted and dispose offsite at a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
14 |  | 02 61 00 |  | Remove all other surface landscape features, relocate offsite to secure location for future re-installment |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 21 | Schedule 2

PROTECTED SENSITIVE

15 |  | 02 61 00 |  | Removal of Outbuilding Contents, storage in secured area, and return of objects upon restoration |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
16 |  | 02 61 00 |  | Excavate, stockpile, load, haul and dispose at LTWMF Facility Contaminated soil and tree roots |  | cubic meters |  |  | 330 |  |  | $ | *** |  |  | $ | *** |
17 |  |  |  | Secondary Excavation (if required) |  | cubic meters |  |  |  |  |  | $ | *** |  |  |  |  |
Earthworks |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 31 00 01 |  | Supply, place, compact and grade clean imported fill per MPH SOP/SOGs (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 520 |  |  | $ | *** |  |  | $ | *** |
2 |  | 31 00 01 |  | Supply, place, compact and grade Granular A (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 40 |  |  | $ | *** |  |  | $ | *** |
3 |  | 31 00 01 |  | Supply, place, compact and grade Granular B (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 40 |  |  | $ | *** |  |  | $ | *** |
4 |  | 31 00 01 |  | Supply, place, and grade Topsoil |  | cubic meters |  |  | 30 |  |  | $ | *** |  |  | $ | *** |
Site Restoration |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | as per Drawings |  | Supply and Install wooden deck as shown including all footings, etc., inluding all permits |  | square meters |  |  | 29 |  |  | $ | *** |  |  | $ | *** |
2 |  | as per Drawings |  | Supply and Place Gravel Drivway as per specifications |  | square meters |  |  | 7 |  |  | $ | *** |  |  | $ | *** |
3 |  | as per Drawings |  | Supply and Place Concrete Sidewalk as per specifications |  | square meters |  |  | 5 |  |  | $ | *** |  |  | $ | *** |
4 |  | as per Drawings |  | Supply and Place concrete stairs as per specifications |  | treads |  |  | 7 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 22 | Schedule 2

PROTECTED SENSITIVE

5 |  | 31 32 50 |  | Water management, sampling, transportation, and disposal at LTMWF |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
6 |  | 32 90 00 |  | Landscape Restoration |  | Allowance |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
7 |  | as per Drawings |  | Supply and Place Fence |  | Linear meters |  |  | 18.00 |  |  | $ | *** |  |  | $ | *** |
Total Price - 11-15 Elizabeth Street | $ | *** |

Group C Requirements - 9 Elizabeth Street

Removals |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 02 61 00 |  | Pre-construction Property Condition Assessment |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
2 |  | 02 61 00 |  | Complete gamma survey and XRF scan of completed excavation surface |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
3 |  | 02 61 00 |  | Collection of soil sample for signature COPCs and the reporting of results following Laboratory Analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
4 |  | 02 61 00 |  | Laboratory analysis of soil sample for signature COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
5 |  | 02 61 00 |  | Collection of soil sample for secondary COPCs and the reporting of results following laboratory analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
6 |  | 02 61 00 |  | Laboratory analysis of composite soil sample for secondary COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
7 |  | 02 61 00 |  | Preparation and submission of Verification Documentation |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 23 | Schedule 2

PROTECTED SENSITIVE

8 |  | 02 41 16 |  | Demolish Existing Site Structures that require removal, verify not radiologically impacted and dispose off site a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
9 |  | 02 41 13 |  | Gravel Driveway Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 42 |  |  | $ | *** |  |  | $ | *** |
10 |  | 02 41 13 |  | Concrete Sidewalk Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 5 |  |  | $ | *** |  |  | $ | *** |
11 |  | 02 41 13 |  | Paving Stone / Interlocking Brick Sidewalk Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 24 |  |  | $ | *** |  |  | $ | *** |
12 |  | 02 41 13 |  | Paving Stone / Interlocking Brick Patio Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 11 |  |  | $ | *** |  |  | $ | *** |
13 |  | 02 41 13 |  | Concrete Stair Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
14 |  | 02 41 13 |  | Remove existing fence, verify not radiologically impacted and dispose offiste at licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
15 |  | 02 41 13 |  | Remove existing Retaining wall, verify not radiologically impacted and dispose offiste at licensed receiving facility |  |  |  |  |  |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 24 | Schedule 2

PROTECTED SENSITIVE

16 |  | 31 11 00 |  | Remove and Dispose of Trees, shrubs, hedges, and all other plants above ground, verify not radiological impacted and dispose offsite at a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
17 |  | 02 41 13 |  | Remove all other surface landscape features, relocate offsite to secure location for future re-installment |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
18 |  | 02 41 13 |  | Removal of Outbuilding Contents, storage in secured area, and return of objects upon restoration |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
19 |  | 02 61 00 |  | Excavate, stockpile, load, haul and dispose at LTWMF Facility Contaminated soil and tree roots |  | cubic meters |  |  | 340 |  |  | $ | *** |  |  | $ | *** |
20 |  |  |  | Secondary Excavation (if required) |  | cubic meters |  |  |  |  |  | $ | *** |  |  | $ | *** |
Earthworks |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 31 00 01 |  | Supply, place, compact and grade clean imported fill per MPH SOP/SOGs (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 360 |  |  | $ | *** |  |  | $ | *** |
2 |  | 31 00 01 |  | Supply, place, compact and grade Granular A (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 60 |  |  | $ | *** |  |  | $ | *** |
3 |  | 31 00 01 |  | Supply, place, compact and grade Granular B (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 60 |  |  | $ | *** |  |  | $ | *** |
4 |  | 31 00 01 |  | Supply, place, and grade Topsoil |  | cubic meters |  |  | 100 |  |  | $ | *** |  |  | $ | *** |
Site Restoration |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | as per Drawings |  | Supply and Place Gravel Driveway as per specifications |  | square meters |  |  | 42 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 25 | Schedule 2

PROTECTED SENSITIVE

2 |  | as per Drawings |  | Supply and Place Concrete Sidewalk as per specifications |  | square meters |  |  | 5 |  |  | $ | *** |  |  | $ | *** |
3 |  | as per Drawings |  | Supply and Place Paving Stone / Interlocking Brick Sidewalk as per specifications |  | square meters |  |  | 24 |  |  | $ | *** |  |  | $ | *** |
4 |  | as per Drawings |  | Supply and install Covered Porch (Front) as shown including all permits |  |  |  |  |  |  |  | $ | *** |  |  | $ | *** |
5 |  | as per Drawings |  | Supply and install Wooden Deck (other) as shown including all permits |  | square meters |  |  | 14 |  |  | $ | *** |  |  | $ | *** |
6 |  | as per Drawings |  | Supply and install Attached Mudroom as shown, including all permits |  | square meters |  |  | 8 |  |  | $ | *** |  |  | $ | *** |
7 |  | as per Drawings |  | Supply and Place Retaining Wall as per specifications |  |  |  |  |  |  |  | $ | *** |  |  | $ | *** |
8 |  | as per Drawings |  | Supply and Place concrete stairs as per specifications |  | treads |  |  | 18 |  |  | $ | *** |  |  | $ | *** |
9 |  | 32 90 00 |  | Landscape Restoration |  | Allowance |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
10 |  | 31 32 50 |  | Water management, sampling, transportation, and disposal at LTMWF |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
11 |  | as per Drawings |  | Supply and Place Fence |  | Linear meters |  |  | 38.00 |  |  | $ | *** |  |  | $ | *** |
Total Price - 9 Elizabeth Street |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 26 | Schedule 2

PROTECTED SENSITIVE

Group C Requirements - 30 Catherine Street |  |  |  |  |  |  |  |  |  |  |
Removals |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 02 61 00 |  | Pre-construction Property Condition Assessment |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
2 |  | 02 61 00 |  | Complete gamma survey and XRF scan of completed excavation surface |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
3 |  | 02 61 00 |  | Collection of soil sample for signature COPCs and the reporting of results following Laboratory Analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
4 |  | 02 61 00 |  | Laboratory analysis of soil sample for signature COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
5 |  | 02 61 00 |  | Collection of soil sample for secondary COPCs and the reporting of results following laboratory analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
6 |  | 02 61 00 |  | Laboratory analysis of composite soil sample for secondary COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
7 |  | 02 61 00 |  | Preparation and submission of Verification Documentation |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
8 |  | 02 41 16 |  | Demolish existing Site structures that require removal, verify not radiologically impacted and dispose off site a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
9 |  | 02 41 13 |  | Gravel Driveway Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 52 |  |  | $ | *** |  |  | $ | *** |
10 |  | 02 41 13 |  | Paving stone / interlocking brick sidewalk removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 7 |  |  | $ | *** |  |  | $ | *** |
11 |  | 02 41 13 |  | Concrete Patio Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 22 |  |  | $ | *** |  |  | $ | *** |
12 |  | 02 41 13 |  | Concrete Stair Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 27 | Schedule 2

PROTECTED SENSITIVE

13 |  | 02 41 13 |  | Remove existing fence, verify not radiologically impacted and dispose offiste at licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
14 |  | 02 41 13 |  | Remove Retaining Wall, verify not radiologically impacted and dispose offiste at licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
15 |  | 31 11 00 |  | Remove and Dispose of Trees, shrubs, hedges, and all other plants above ground, verify not radiological impacted and dispose offsite at a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
16 |  |  |  | Remove all other surface landscape features, relocate offsite to secure location for future re-installment |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
17 |  |  |  | Removal of Outbuilding Contents, storage in secured area, and return of objects upon restoration |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
18 |  | 02 61 00 |  | Excavate, stockpile, load, haul and dispose at LTWMF Facility Contaminated soil and tree roots |  | cubic meters |  |  | 210 |  |  | $ | *** |  |  | $ | *** |
19 |  |  |  | Secondary Excavation (if required) |  | cubic meters |  |  |  |  |  | $ | *** |  |  |  |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 28 | Schedule 2

PROTECTED SENSITIVE

Earthworks |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 31 00 01 |  | Supply, place, compact and grade clean imported fill per MPH SOP/SOGs (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 140 |  |  | $ | *** |  |  | $ | *** |
2 |  | 31 00 01 |  | Supply, place, compact and grade Granular A (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 60 |  |  | $ | *** |  |  | $ | *** |

3 |  | 31 00 01 |  | Supply, place, compact and grade Granular B (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 60 |  |  | $ | *** |  |  | $ | *** |
4 |  | 31 00 01 |  | Supply, place, and grade Topsoil |  | cubic meters |  |  | 80 |  |  | $ | *** |  |  | $ | *** |
Site Restoration |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | as per Drawings |  | Supply and Install shed as shown including all footings, floors etc. |  | square meters |  |  | 12 |  |  | $ | *** |  |  | $ | *** |
2 |  | as per Drawings |  | Supply, Place, Gravel Driveway as per specifications |  | square meters |  |  | 52 |  |  | $ | *** |  |  | $ | *** |
3 |  | as per Drawings |  | Supply and Place Paving stone / interlocking brick sidewalk as per specifications |  | square meters |  |  | 7 |  |  | $ | *** |  |  | $ | *** |
4 |  | as per Drawings |  | Supply and Place Concrete patio as per specifications |  | square meters |  |  | 22 |  |  | $ | *** |  |  | $ | *** |
5 |  | as per Drawings |  | Supply and Install Covered Porch (Front) as shown including all permits |  | square meters |  |  | 13 |  |  | $ | *** |  |  | $ | *** |
6 |  | 06 15 00 |  | Supply, Place Wooden deck (other) as shown including all permits |  | square meters |  |  | 11 |  |  | $ | *** |  |  | $ | *** |
7 |  | as per Drawings |  | Supply and Place concrete stairs as per specifications |  | treads |  |  | 17 |  |  | $ | *** |  |  | $ | *** |
7 |  | as per Drawings |  | Supply and Place retaining wall as per specifications |  | Linear meters |  |  | 14 |  |  | $ | *** |  |  | $ | *** |
8 |  | as per Drawings |  | Supply and Place Fence |  | Linear meters |  |  | 5 |  |  | $ | *** |  |  | $ | *** |
9 |  | 31 32 50 |  | Water management, sampling, transportation, and disposal at LTMWF |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
10 |  | 32 90 00 |  | Landscape Restoration |  | Allowance |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
Total Price - 30 Catherine Street |  |  |  |  |  |  |  |  |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 29 | Schedule 2

PROTECTED SENSITIVE

Group C Requirements - 24 Harris Street |  |  |  |  |  |  |  |  |  |  |
Removals |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 02 61 00 |  | Pre-construction Property Condition Assessment |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
2 |  | 02 61 00 |  | Complete gamma survey and XRF scan of completed excavation surface |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
3 |  | 02 61 00 |  | Collection of soil sample for signature COPCs and the reporting of results following Laboratory Analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
4 |  | 02 61 00 |  | Laboratory analysis of soil sample for signature COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
5 |  | 02 61 00 |  | Collection of soil sample for secondary COPCs and the reporting of results following laboratory analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
6 |  | 02 61 00 |  | Laboratory analysis of composite soil sample for secondary COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
7 |  | 02 61 00 |  | Preparation and submission of Verification Documentation |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
8 |  | 02 41 16 |  | Demolish existing Site structures that require removal, verify not radiologically impacted and dispose off site a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
9 |  | 02 41 13 |  | Gravel Driveway Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 10 |  |  | $ | *** |  |  | $ | *** |
10 |  | 02 41 13 |  | Paving stone / interlocking brick sidewalk removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 9 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 30 | Schedule 2

PROTECTED SENSITIVE

11 |  | 02 41 13 |  | Retaining Wall Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
12 |  | 02 41 13 |  | Concrete Stair Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
13 |  | 02 41 13 |  | Remove existing fence, verify not radiologically impacted and dispose offiste at licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
14 |  | 31 11 00 |  | Remove and Dispose of Trees, shrubs, hedges, and all other plants above ground, verify not radiological impacted and dispose offsite at a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
15 |  |  |  | Remove all other surface landscape features, relocate offsite to secure location for future re-installment |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
16 |  |  |  | Removal of Outbuilding Contents, storage in secured area, and return of objects upon restoration |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
17 |  | 02 61 00 |  | Excavate, stockpile, load, haul and dispose at LTWMF Facility Contaminated soil and tree roots |  | cubic meters |  |  | 170 |  |  | $ | *** |  |  | $ | *** |
18 |  |  |  | Secondary Excavation (if required) |  | cubic meters |  |  |  |  |  | $ | *** |  |  |  |  |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 31 | Schedule 2

PROTECTED SENSITIVE

Earthworks |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 31 00 01 |  | Supply, place, compact and grade clean imported fill per MPH SOP/SOGs (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 160 |  |  | $ | *** |  |  | $ | *** |

2 |  | 31 00 01 |  | Supply, place, compact and grade Granular A (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 50 |  |  | $ | *** |  |  | $ | *** |
3 |  | 31 00 01 |  | Supply, place, compact and grade Granular B (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 50 |  |  | $ | *** |  |  | $ | *** |
4 |  | 31 00 01 |  | Supply, place, and grade Topsoil |  | cubic meters |  |  | 40 |  |  | $ | *** |  |  | $ | *** |
Site Restoration |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | as per Drawings |  | Supply and Install Gazebo as shown including all footings, floors etc. |  | square meters |  |  | 9 |  |  | $ | *** |  |  | $ | *** |
2 |  | as per Drawings |  | Supply, Place, Gravel Driveway as per specifications |  | square meters |  |  | 10 |  |  | $ | *** |  |  | $ | *** |
3 |  | as per Drawings |  | Supply and Place Paving stone / interlocking brick sidewalk as per specifications |  | square meters |  |  | 9 |  |  | $ | *** |  |  | $ | *** |
4 |  | as per Drawings |  | Supply and Install Retaining Wall as shown, including all permits |  | Linear meters |  |  | 11 |  |  | $ | *** |  |  | $ | *** |
5 |  | as per Drawings |  | Supply and Install Covered Porch (Front) as shown, including all permits |  | square meters |  |  | 19 |  |  | $ | *** |  |  | $ | *** |
6 |  | as per Drawings |  | Supply and Place concrete stairs as per specifications |  | treads |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
7 |  | as per Drawings |  | Supply and Place Fence |  | Linear meters |  |  | 41 |  |  | $ | *** |  |  | $ | *** |
8 |  | 31 32 50 |  | Water management, sampling, transportation, and disposal at LTMWF |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
9 |  | 32 90 00 |  | Landscape Restoration |  | Allowance |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
Total Price - 24 Harris Street |  |  |  |  |  |  |  |  |  |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 32 | Schedule 2

PROTECTED SENSITIVE

Group C Requirements - 22 Harris Street |  |  |  |  |  |  |  |  |  |  |
Removals |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 02 61 00 |  | Pre-construction Property Condition Assessment |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
2 |  | 02 61 00 |  | Complete gamma survey and XRF scan of completed excavation surface |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
3 |  | 02 61 00 |  | Collection of soil sample for signature COPCs and the reporting of results following Laboratory Analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
4 |  | 02 61 00 |  | Laboratory analysis of soil sample for signature COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
5 |  | 02 61 00 |  | Collection of soil sample for secondary COPCs and the reporting of results following laboratory analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
6 |  | 02 61 00 |  | Laboratory analysis of composite soil sample for secondary COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
7 |  | 02 61 00 |  | Preparation and submission of Verification Documentation |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
8 |  | 02 41 16 |  | Demolish existing Site structures that require removal, verify not radiologically impacted and dispose off site a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
9 |  | 02 41 13 |  | Gravel Driveway Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 67 |  |  | $ | *** |  |  | $ | *** |
10 |  | 02 41 13 |  | Paving stone / interlocking brick sidewalk removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 18 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 33 | Schedule 2

PROTECTED SENSITIVE

11 |  | 02 41 13 |  | Remove retaining wall, verify not radiologically impacted and dispose offiste at licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
12 |  | 02 41 13 |  | Concrete Stair Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
13 |  | 02 41 13 |  | Remove existing fence, verify not radiologically impacted and dispose offiste at licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
14 |  | 31 11 00 |  | Remove and Dispose of Trees, shrubs, hedges, and all other plants above ground, verify not radiological impacted and dispose offsite at a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
15 |  |  |  | Remove all other surface landscape features, relocate offsite to secure location for future re-installment |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
16 |  |  |  | Removal of Outbuilding Contents, storage in secured area, and return of objects upon restoration |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
17 |  | 02 61 00 |  | Excavate, stockpile, load, haul and dispose at LTWMF Facility Contaminated soil and tree roots |  | cubic meters |  |  | 430 |  |  | $ | *** |  |  | $ | *** |
18 |  |  |  | Secondary Excavation (if required) |  | cubic meters |  |  |  |  |  | $ | *** |  |  |  |  |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 34 | Schedule 2

PROTECTED SENSITIVE

Earthworks |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 31 00 01 |  | Supply, place, compact and grade clean imported fill per MPH SOP/SOGs (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 520 |  |  | $ | *** |  |  | $ | *** |

2 |  | 31 00 01 |  | Supply, place, compact and grade Granular A (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 80 |  |  | $ | *** |  |  | $ | *** |
3 |  | 31 00 01 |  | Supply, place, compact and grade Granular B (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 80 |  |  | $ | *** |  |  | $ | *** |
4 |  | 31 00 01 |  | Supply, place, and grade Topsoil |  | cubic meters |  |  | 90 |  |  | $ | *** |  |  | $ | *** |
Site Restoration |  |  |  |  |  |  |  |  |  | $ | *** |  |  | $ | *** |
1 |  | as per Drawings |  | Supply and Install shed as shown including all footings, floors etc. |  | square meters |  |  | 10 |  |  | $ | *** |  |  | $ | *** |
2 |  | as per Drawings |  | Supply, Place, Gravel Driveway as per specifications |  | square meters |  |  | 67 |  |  | $ | *** |  |  | $ | *** |
3 |  | as per Drawings |  | Supply and Place Paving stone / interlocking brick sidewalk as per specifications |  | square meters |  |  | 18 |  |  | $ | *** |  |  | $ | *** |
4 |  | as per Drawings |  | Supply and Place retaining wall as per specifications |  | square meters |  |  | 46 |  |  | $ | *** |  |  | $ | *** |
5 |  | as per Drawings |  | Supply, Place Covered Porch (Front) as shown including all permits |  | square meters |  |  | 10 |  |  | $ | *** |  |  | $ | *** |
6 |  | as per Drawings |  | Supply and Place concrete stairs as per specifications |  | treads |  |  | 8 |  |  | $ | *** |  |  | $ | *** |
7 |  | as per Drawings |  | Supply and Place Fence |  | Linear meters |  |  | 3 |  |  | $ | *** |  |  | $ | *** |
8 |  | 31 32 50 |  | Water management, sampling, transportation, and disposal at LTMWF |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
9 |  | 32 90 00 |  | Landscape Restoration |  | Allowance |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
Total Price - 22 Harris Street |  |  |  |  |  |  |  |  |  |  |  | $ | *** |
Total Remediation, Earthworks and Restoration Only |  |  |  |  |  |  |  |  |  |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 35 | Schedule 2

PROTECTED SENSITIVE

|  | Specification Reference |  | Description |  | Unit of Measure |  | Estimated Quantity |  |  | Price per Unit |  |  | Total Price |
Group G - General Requirements |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 02 61 00 |  | Mobilization and Project Startup |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
2 |  | 02 61 00 |  | Demobilization and Project Closeout |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
3 |  | 01 31 19 |  | Project Meetings |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
4 |  | 01 32 00 |  | Construction Progress Documentation |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
5 |  | 01 32 16 |  | Construction Progress Schedule |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
6 |  | 01 35 29 |  | Health and Safety Plan |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
7 |  | 01 35 29 |  | Implementation of Health and Safety - All Sites |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
8 |  | 01 35 30 |  | Radiation Protection Plan - All Sites |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
9 |  | 01 35 30 |  | Implementation of Radiation Protection - All Sites |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
10 |  | 01 35 43 |  | Environmental Protection Manual and Dust Management Plan - All Sites |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
11 |  | 01 35 43 |  | Implementation of Environmental Protection and Dust Management - All Sites |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
12 |  | 01 45 00 |  | Quality Assurance Plan |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
13 |  | 01 45 00 |  | Implementation of QA/QC - All Sites |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
14 |  | 01 51 00 |  | Provision and Maintenance of Temporary Utilities - (Contractor Use) |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
15 |  | 01 52 00 |  | Provision and Construction Facilities - All Sites |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 36 | Schedule 2

PROTECTED SENSITIVE

16 |  | 02 61 00 |  | Permitting as per OBC and MPH SOP-SOG, OMOECC, CN/CP - all sites |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
17 |  |  |  | Traffic Control - All sites |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
18 |  | 01 33 00 |  | All Other Submittals |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
19 |  | 01 14 00 |  | Site Security |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
20 |  |  |  | Bonding & Insurance |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
21 |  | 01 14 00 |  | Training and Security Clearance |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
22 |  | 01 78 00 |  | Closeout Submittal |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
23 |  | 01 56 00 |  | Supply, Install, Maintain, and Remove Sediment Erosion Control fencing |  | Linear meters |  |  | 165 |  |  | $ | *** |  |  | $ | *** |
24 |  | 01 56 00 |  | Supply, Install, Maintain, and Remove - Perimeter Safety Fencing |  | Linear meters |  |  | 330 |  |  | $ | *** |  |  | $ | *** |
25 |  | 02 61 00 |  | Supply, Install, Maintain and Remove Access Gates as shown |  | each |  |  | 7 |  |  | $ | *** |  |  | $ | *** |
26 |  | See Figure Attached |  | Tree Protection Fencing |  | Linear meters |  |  | 120 |  |  | $ | *** |  |  | $ | *** |
Total Price - General Requirements | $ | *** |

Group G Requirements - 32 Alexander Street

Removals
1 |  | 02 61 00 |  | Pre-construction Property Condition Assessment |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
2 |  | 02 61 00 |  | Complete gamma survey and XRF scan of completed excavation surface |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
3 |  | 02 61 00 |  | Collection of soil sample for signature COPCs and the reporting of results following Laboratory Analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 37 | Schedule 2

PROTECTED SENSITIVE

4 |  | 02 61 00 |  | Laboratory Analysis of soil sample for signature COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
5 |  | 02 61 00 |  | Collection of soil sample for secondary COPCs and the reporting of results following laboratory analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
6 |  | 02 61 00 |  | Laboratory Analysis of composite soil sample for secondary COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
7 |  | 02 61 00 |  | Preparation and Submission of Verification Documentation |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
8 |  | 02 41 16 |  | Demolish Existing Site Structures that require removal, verify not radiologically impacted and dispose off site a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
9 |  | 02 41 13 |  | Gravel Driveway Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 106 |  |  | $ | *** |  |  | $ | *** |
10 |  | 02 41 13 |  | Asphalt Driveway Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 41 |  |  | $ | *** |  |  | $ | *** |
11 |  | 02 41 13 |  | Concrete Driveway Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 33 |  |  | $ | *** |  |  | $ | *** |
12 |  | 02 41 13 |  | Concrete Sidewalk Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 4 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 38 | Schedule 2

PROTECTED SENSITIVE

13 |  | 02 41 13 |  | Paving Stone / Interlocking Brick Patio Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 9 |  |  | $ | *** |  |  | $ | *** |
14 |  | 02 41 13 |  | Remove existing fence, verify not radiologically impacted and dispose offiste at licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
15 |  | 02 41 13 |  | Remove Retaining Wall, verify not radiologically impacted and dispose offiste at licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
16 |  | 02 61 00 |  | Remove and Dispose of Trees, shrubs, hedges, and all other plants above ground, verify not radiological impacted and dispose offsite at a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
17 |  | 02 61 00 |  | Remove all other surface landscape features, relocate offsite to secure location for future re-installment |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
18 |  | 02 61 00 |  | Removal of Outbuilding Contents, storage in secured area, and return of objects upon restoration |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
19 |  | 02 61 00 |  | Excavate, stockpile, load, haul and dispose at LTWMF Facility Contaminated soil and tree roots |  | cubic meters |  |  | 780 |  |  | $ | *** |  |  | $ | *** |
20 |  |  |  | Secondary Excavation (if required) |  | cubic meters |  |  |  |  |  | $ | *** |  |  |  |  |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 39 | Schedule 2

PROTECTED SENSITIVE

Earthworks
1 |  | 31 00 01 |  | Supply, place, compact and grade clean imported fill per MPH SOP/SOGs (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 1,060 |  |  | $ | *** |  |  | $ | *** |
2 |  | 31 00 01 |  | Supply, place, compact and grade Granular A (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 100 |  |  | $ | *** |  |  | $ | *** |
3 |  | 31 00 01 |  | Supply, place, compact and grade Granular B (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 100 |  |  | $ | *** |  |  | $ | *** |
4 |  | 31 00 01 |  | Supply, place, and grade Topsoil |  | cubic meters |  |  | 150 |  |  | $ | *** |  |  | $ | *** |
Site Restoration
1 |  | as per Drawings |  | Supply and Install sheds as shown including all footings, etc., inluding all permits |  | square meters |  |  | 17 |  |  | $ | *** |  |  | $ | *** |
2 |  | as per Drawings |  | Supply and Place Gravel Drivway as per specifications |  | square meters |  |  | 106 |  |  | $ | *** |  |  | $ | *** |
3 |  | as per Drawings |  | Supply and Place Asphalt Drivway as per specifications |  | square meters |  |  | 41 |  |  | $ | *** |  |  | $ | *** |
4 |  | as per Drawings |  | Supply and Place Concrete Drivway as per specifications |  | square meters |  |  | 33 |  |  | $ | *** |  |  | $ | *** |
5 |  | as per Drawings |  | Supply and Place Concrete Sidewalk as per specifications |  | square meters |  |  | 4 |  |  | $ | *** |  |  | $ | *** |
6 |  | as per Drawings |  | Supply and install Wooden Deck (front) as shown including all permits |  | square meters |  |  | 20 |  |  | $ | *** |  |  | $ | *** |
7 |  | as per Drawings |  | Supply and install Wooden Deck (rear) as shown including all permits |  | square meters |  |  | 33 |  |  | $ | *** |  |  | $ | *** |
8 |  | as per Drawings |  | Supply and install Wooden Deck (other) as shown including all permits |  | square meters |  |  | 4 |  |  | $ | *** |  |  | $ | *** |
9 |  | as per Drawings |  | Supply and Place Paving Stone / Interlocking Brick Patio as per specifications |  | square meters |  |  | 9 |  |  | $ | *** |  |  | $ | *** |
10 |  | as per Drawings |  | Supply and Place Retaining Wall as per specifications |  | Linear meters |  |  | 21 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 40 | Schedule 2

PROTECTED SENSITIVE

11 |  | 31 32 50 |  | Water management, sampling, transportation, and disposal at LTMWF |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
12 |  | 32 90 00 |  | Landscape Restoration |  | Allowance |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
13 |  | as per Drawings |  | Supply and Place Fence |  | Linear meters |  |  | 36.00 |  |  | $ | *** |  |  | $ | *** |
Total Price - 32 Alexander Street | $ | *** |

Group G Requirements - 30 Alexander Street |  |  |  |  |  |  |  |  |  |  |
Removals
1 |  | 02 61 00 |  | Pre-construction Property Condition Assessment |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
2 |  | 02 61 00 |  | Complete gamma survey and XRF scan of completed excavation surface |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
3 |  | 02 61 00 |  | Collection of soil sample for signature COPCs and the reporting of results following Laboratory Analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
4 |  | 02 61 00 |  | Laboratory analysis of soil sample for signature COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
5 |  | 02 61 00 |  | Collection of soil sample for secondary COPCs and the reporting of results following laboratory analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
6 |  | 02 61 00 |  | Laboratory analysis of composite soil sample for secondary COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
7 |  | 02 61 00 |  | Preparation and submission of Verification Documentation |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
8 |  | 02 41 16 |  | Demolish Existing Site Structures that require removal, verify not radiologically impacted and dispose off site a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 41 | Schedule 2

PROTECTED SENSITIVE

9 |  | 02 41 13 |  | Concrete Sidewalk Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 7 |  |  | $ | *** |  |  | $ | *** |
10 |  | 02 41 13 |  | Concrete Driveway Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 57 |  |  | $ | *** |  |  | $ | *** |
11 |  | 02 41 13 |  | Remove existing fence, verify not radiologically impacted and dispose offiste at licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
12 |  | 02 41 13 |  | Retaining Wall Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
13 |  | 02 41 13 |  | Concrete Stair Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
14 |  | 31 11 00 |  | Remove and Dispose of Trees, shrubs, hedges, and all other plants above ground, verify not radiological impacted and dispose offsite at a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
15 |  | 02 61 00 |  | Remove all other surface landscape features, relocate offsite to secure location for future re-installment |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
16 |  | 02 61 00 |  | Removal of Outbuilding Contents, storage in secured area, and return of objects upon restoration |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
17 |  | 02 61 00 |  | Excavate, stockpile, load, haul and dispose at LTWMF Facility Contaminated soil and tree roots |  | cubic meters |  |  | 540 |  |  | $ | *** |  |  | $ | *** |
18 |  |  |  | Secondary Excavation (if required) |  | cubic meters |  |  |  |  |  | $ | *** |  |  |  |  |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 42 | Schedule 2

PROTECTED SENSITIVE

Earthworks
1 |  | 31 00 01 |  | Supply, place, compact and grade clean imported fill per MPH SOP/SOGs (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 720 |  |  | $ | *** |  |  | $ | *** |
2 |  | 31 00 01 |  | Supply, place, compact and grade Granular A (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 60 |  |  | $ | *** |  |  | $ | *** |
3 |  | 31 00 01 |  | Supply, place, compact and grade Granular B (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 60 |  |  | $ | *** |  |  | $ | *** |
4 |  | 31 00 01 |  | Supply, place, and grade Topsoil |  | cubic meters |  |  | 120 |  |  | $ | *** |  |  | $ | *** |
Site Restoration
1 |  | as per Drawings |  | Supply and Install sheds as shown including all footings, etc., inluding all permits |  | square meters |  |  | 10 |  |  | $ | *** |  |  | $ | *** |
2 |  | as per Drawings |  | Supply and Install detatched Garage as shown including all footings, etc., inluding all permits |  | square meters |  |  | 20 |  |  | $ | *** |  |  | $ | *** |
3 |  | as per Drawings |  | Supply and Place Concrete Drivway as per specifications |  | square meters |  |  | 57 |  |  | $ | *** |  |  | $ | *** |
4 |  | as per Drawings |  | Supply and Place Concrete Sidewalk as per specifications |  | square meters |  |  | 7 |  |  | $ | *** |  |  | $ | *** |
5 |  | as per Drawings |  | Supply and install Wooden Deck (front) as shown including all permits |  | square meters |  |  | 7 |  |  | $ | *** |  |  | $ | *** |
6 |  | as per Drawings |  | Supply and Place Retaining Wall as per specifications |  | Linear meters |  |  | 18 |  |  | $ | *** |  |  | $ | *** |
7 |  | as per Drawings |  | Supply and Install Concrete Steps as per specifications |  | Treads |  |  | 6 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 43 | Schedule 2

PROTECTED SENSITIVE

8 |  | 31 32 50 |  | Water management, sampling, transportation, and disposal at LTMWF |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
9 |  | 32 90 00 |  | Landscape Restoration |  | Allowance |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
10 |  | as per Drawings |  | Supply and Place Fence |  | Linear meters |  |  | 32.00 |  |  | $ | *** |  |  | $ | *** |
Total Price - 30 Alexander Street | $ | *** |

Group G Requirements - 28 Alexander Street |  |  |  |  |  |  |  |  |  |  |
Removals |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 02 61 00 |  | Pre-construction Property Condition Assessment |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
2 |  | 02 61 00 |  | Complete gamma survey and XRF scan of completed excavation surface |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
3 |  | 02 61 00 |  | Collection of soil sample for signature COPCs and the reporting of results following Laboratory Analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
4 |  | 02 61 00 |  | Laboratory analysis of soil sample for signature COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
5 |  | 02 61 00 |  | Collection of soil sample for secondary COPCs and the reporting of results following laboratory analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
6 |  | 02 61 00 |  | Laboratory analysis of composite soil sample for secondary COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
7 |  | 02 61 00 |  | Preparation and submission of Verification Documentation |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
8 |  | 02 41 16 |  | Demolish Existing Site Structures that require removal, verify not radiologically impacted and dispose off site a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 44 | Schedule 2

PROTECTED SENSITIVE

9 |  | 02 41 13 |  | Concrete Stair Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
10 |  | 02 41 13 |  | Remove existing fence, verify not radiologically impacted and dispose offiste at licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
11 |  | 02 41 13 |  | Remove existing Retaining wall, verify not radiologically impacted and dispose offiste at licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
12 |  | 31 11 00 |  | Remove and Dispose of Trees, shrubs, hedges, and all other plants above ground, verify not radiological impacted and dispose offsite at a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
13 |  | 02 41 13 |  | Remove all other surface landscape features, relocate offsite to secure location for future re-installment |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
14 |  | 02 41 13 |  | Removal of Outbuilding Contents, storage in secured area, and return of objects upon restoration |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
15 |  | 02 61 00 |  | Excavate, stockpile, load, haul and dispose at LTWMF Facility Contaminated soil and tree roots |  | cubic meters |  |  | 560 |  |  | $ | *** |  |  | $ | *** |
16 |  |  |  | Secondary Excavation (if required) |  | cubic meters |  |  |  |  |  | $ | *** |  |  |  |  |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 45 | Schedule 2

PROTECTED SENSITIVE

Earthworks |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 31 00 01 |  | Supply, place, compact and grade clean imported fill per MPH SOP/SOGs (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 700 |  |  | $ | *** |  |  | $ | *** |
2 |  | 31 00 01 |  | Supply, place, compact and grade Granular A (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 80 |  |  | $ | *** |  |  | $ | *** |
3 |  | 31 00 01 |  | Supply, place, compact and grade Granular B (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 80 |  |  | $ | *** |  |  | $ | *** |
4 |  | 31 00 01 |  | Supply, place, and grade Topsoil |  | cubic meters |  |  | 130 |  |  | $ | *** |  |  | $ | *** |
Site Restoration |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | as per Drawings |  | Supply and Install sheds as shown including all footings, etc., inluding all permits |  | square meters |  |  | 9 |  |  | $ | *** |  |  | $ | *** |
2 |  | as per Drawings |  | Supply and install Wooden Deck (rear) as shown including all permits |  | square meters |  |  | 31 |  |  | $ | *** |  |  | $ | *** |
3 |  | as per Drawings |  | Supply and install Covered Porch (front) as shown including all permits |  | square meters |  |  | 25 |  |  | $ | *** |  |  | $ | *** |
4 |  | as per Drawings |  | Supply and Place Retaining Wall as per specifications |  | Linear meters |  |  | 17 |  |  | $ | *** |  |  | $ | *** |
5 |  | as per Drawings |  | Supply and Place Retaining Wall as per specifications |  | Linear meters |  |  | 17 |  |  | $ | *** |  |  | $ | *** |
6 |  | as per Drawings |  | Supply and Place concrete stairs as per specifications |  | treads |  |  | 5 |  |  | $ | *** |  |  | $ | *** |
7 |  | 32 90 00 |  | Landscape Restoration |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
8 |  | 31 32 50 |  | Water management, sampling, transportation, and disposal at LTMWF |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
9 |  | as per Drawings |  | Supply and Place Fence |  | Linear meters |  |  | 18.00 |  |  | $ | *** |  |  | $ | *** |
Total Price - 28 Alexander Street | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 46 | Schedule 2

PROTECTED SENSITIVE

Group G Requirements - 26 Alexander Street |  |  |  |  |  |  |  |  |  |  |
Removals |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 02 61 00 |  | Pre-construction Property Condition Assessment |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
2 |  | 02 61 00 |  | Complete gamma survey and XRF scan of completed excavation surface |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
3 |  | 02 61 00 |  | Collection of soil sample for signature COPCs and the reporting of results following Laboratory Analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
4 |  | 02 61 00 |  | Laboratory analysis of soil sample for signature COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
5 |  | 02 61 00 |  | Collection of soil sample for secondary COPCs and the reporting of results following laboratory analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
6 |  | 02 61 00 |  | Laboratory analysis of composite soil sample for secondary COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
7 |  | 02 61 00 |  | Preparation and submission of Verification Documentation |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
8 |  | 02 41 16 |  | Demolish existing Site structures that require removal, verify not radiologically impacted and dispose off site a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
9 |  | 02 41 13 |  | Asphalt Driveway Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 20 |  |  | $ | *** |  |  | $ | *** |
10 |  | 02 41 13 |  | Remove existing fence, verify not radiologically impacted and dispose offiste at licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 47 | Schedule 2

PROTECTED SENSITIVE

11 |  | 31 11 00 |  | Remove and Dispose of Trees, shrubs, hedges, and all other plants above ground, verify not radiological impacted and dispose offsite at a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
12 |  |  |  | Remove all other surface landscape features, relocate offsite to secure location for future re-installment |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
13 |  |  |  | Removal of Outbuilding Contents, storage in secured area, and return of objects upon restoration |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
14 |  | 02 61 00 |  | Excavate, stockpile, load, haul and dispose at LTWMF Facility Contaminated soil and tree roots |  | cubic meters |  |  | 1,350 |  |  | $ | *** |  |  | $ | *** |
15 |  |  |  | Secondary Excavation (if required) |  | cubic meters |  |  |  |  |  | $ | *** |  |  |  |  |
Earthworks |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 31 00 01 |  | Supply, place, compact and grade clean imported fill per MPH SOP/SOGs (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 2,060 |  |  | $ | *** |  |  | $ | *** |
2 |  | 31 00 01 |  | Supply, place, compact and grade Granular A (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 160 |  |  | $ | *** |  |  | $ | *** |
3 |  | 31 00 01 |  | Supply, place, compact and grade Granular B (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 160 |  |  | $ | *** |  |  | $ | *** |
4 |  | 31 00 01 |  | Supply, place, and grade Topsoil |  | cubic meters |  |  | 160 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 48 | Schedule 2

PROTECTED SENSITIVE

Site Restoration |  |  |  |  |  |  |  |  |  | $ | *** |  |  | $ | *** |
1 |  | as per Drawings |  | Supply and Install shed as shown including all footings, etc., inluding all permits |  | square meters |  |  | 7 |  |  | $ | *** |  |  | $ | *** |
2 |  | as per Drawings |  | Supply and Place Asphalt Drivway as per specifications |  | square meters |  |  | 20 |  |  | $ | *** |  |  | $ | *** |
3 |  | as per Drawings |  | Supply and install Wooden Deck (front) as shown including all permits |  | square meters |  |  | 51 |  |  | $ | *** |  |  | $ | *** |
4 |  | as per Drawings |  | Supply and install Wooden Deck (rear) as shown including all permits |  | square meters |  |  | 28 |  |  | $ | *** |  |  | $ | *** |
5 |  | as per Drawings |  | Supply and install Wooden Deck (other) as shown including all permits |  | square meters |  |  | 7 |  |  | $ | *** |  |  | $ | *** |
6 |  | 31 32 50 |  | Water management, sampling, transportation, and disposal at LTMWF |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
7 |  | 32 90 00 |  | Landscape Restoration |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
8 |  | as per Drawings |  | Supply and Place Fence |  | Linear meters |  |  | 41.00 |  |  | $ | *** |  |  | $ | *** |
Total Price -26 Alexander Street |  |  | $ | *** |

Group G Requirements - 18 Alexander Street |  |  |  |  |  |  |  |  |  |  |
Removals |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 02 61 00 |  | Pre-construction Property Condition Assessment |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
2 |  | 02 61 00 |  | Complete gamma survey and XRF scan of completed excavation surface |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
3 |  | 02 61 00 |  | Collection of soil sample for signature COPCs and the reporting of results following Laboratory Analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
4 |  | 02 61 00 |  | Laboratory analysis of soil sample for signature COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | ***
5 |  | 02 61 00 |  | Collection of soil sample for secondary COPCs and the reporting of results following laboratory analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 49 | Schedule 2

PROTECTED SENSITIVE

6 |  | 02 61 00 |  | Laboratory analysis of composite soil sample for secondary COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
7 |  | 02 61 00 |  | Preparation and submission of Verification Documentation |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
8 |  | 02 41 16 |  | Demolish existing Site structures that require removal, verify not radiologically impacted and dispose off site a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
9 |  | 02 41 13 |  | Asphalt Driveway Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 42 |  |  | $ | *** |  |  | $ | *** |
10 |  | 02 41 13 |  | Concrete Patio removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 11 |  |  | $ | *** |  |  | $ | *** |
11 |  | 02 41 13 |  | Retaining Wall Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
12 |  | 02 41 13 |  | Concrete Stair Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
13 |  | 02 41 13 |  | Remove existing fence, verify not radiologically impacted and dispose offiste at licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
14 |  | 31 11 00 |  | Remove and Dispose of Trees, shrubs, hedges, and all other plants above ground, verify not radiological impacted and dispose offsite at a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 50 | Schedule 2

PROTECTED SENSITIVE

15 |  |  |  | Remove all other surface landscape features, relocate offsite to secure location for future re-installment |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
16 |  |  |  | Removal of Outbuilding Contents, storage in secured area, and return of objects upon restoration |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
17 |  | 02 61 00 |  | Excavate, stockpile, load, haul and dispose at LTWMF Facility Contaminated soil and tree roots |  | cubic meters |  |  | 340 |  |  | $ | *** |  |  | $ | *** |
18 |  |  |  | Secondary Excavation (if required) |  | cubic meters |  |  |  |  |  | $ | *** |  |  |  |  |

Earthworks |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 31 00 01 |  | Supply, place, compact and grade clean imported fill per MPH SOP/SOGs (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 480 |  |  | $ | *** |  |  | $ | *** |
2 |  | 31 00 01 |  | Supply, place, compact and grade Granular A (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 50 |  |  | $ | *** |  |  | $ | *** |
3 |  | 31 00 01 |  | Supply, place, compact and grade Granular B (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 50 |  |  | $ | *** |  |  | $ | *** |
4 |  | 31 00 01 |  | Supply, place, and grade Topsoil |  | cubic meters |  |  | 50 |  |  | $ | *** |  |  | $ | *** |

Site Restoration |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | as per Drawings |  | Supply and Place Asphalt Drivway as per specifications |  | square meters |  |  | 42 |  |  | $ | *** |  |  | $ | *** |
2 |  | as per Drawings |  | Supply and Place Concrete Patio as per specifications |  | square meters |  |  | 11 |  |  | $ | *** |  |  | $ | *** |
3 |  | as per Drawings |  | Supply and install Wooden Deck (rear) as shown including all permits |  |  |  |  |  |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 51 | Schedule 2

PROTECTED SENSITIVE

4 |  | as per Drawings |  | Supply and Place Retaining Wall as per specifications |  | Linear meters |  |  | 17 |  |  | $ | *** |  |  | $ | *** |
5 |  | as per Drawings |  | Supply and Place concrete stairs as per specifications |  | treads |  |  | 2 |  |  | $ | *** |  |  | $ | *** |
6 |  | 31 32 50 |  | Water management, sampling, transportation, and disposal at LTMWF |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
7 |  | 32 90 00 |  | Landscape Restoration |  | Allowance |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
8 |  | as per Drawings |  | Supply and Place Fence |  | Linear meters |  |  | 36.00 |  |  | $ | *** |  |  | $ | *** |
Total Price - 18 Alexander Street |  |  | $ | *** |

Group G Requirements - 16 Alexander Street |  |  |  |  |  |  |  |  |  |  |
Removals |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 02 61 00 |  | Pre-construction Property Condition Assessment |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
2 |  | 02 61 00 |  | Complete gamma survey and XRF scan of completed excavation surface |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
3 |  | 02 61 00 |  | Collection of soil sample for signature COPCs and the reporting of results following Laboratory Analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
4 |  | 02 61 00 |  | Laboratory analysis of soil sample for signature COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
5 |  | 02 61 00 |  | Collection of soil sample for secondary COPCs and the reporting of results following laboratory analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
6 |  | 02 61 00 |  | Laboratory analysis of composite soil sample for secondary COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
7 |  | 02 61 00 |  | Preparation and submission of Verification Documentation |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 52 | Schedule 2

PROTECTED SENSITIVE

8 |  | 02 41 16 |  | Demolish existing Site structures that require removal, verify not radiologically impacted and dispose off site a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
9 |  | 02 41 13 |  | Asphalt Driveway Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 90 |  |  | $ | *** |  |  | $ | *** |
10 |  | 02 41 13 |  | Concrete sidewalk removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 4 |  |  | $ | *** |  |  | $ | *** |
11 |  | 02 41 13 |  | Paving stone / interlocking brick patio removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 7 |  |  | $ | *** |  |  | $ | *** |
12 |  | 02 41 13 |  | Concrete patio removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 10 |  |  | $ | *** |  |  | $ | *** |
13 |  | 02 41 13 |  | Remove retaining wall, verify not radiologically impacted and dispose offiste at licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
14 |  | 02 41 13 |  | Concrete Stair Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
15 |  | 31 11 00 |  | Remove and Dispose of Trees, shrubs, hedges, and all other plants above ground, verify not radiological impacted and dispose offsite at a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 53 | Schedule 2

PROTECTED SENSITIVE

16 |  |  |  | Remove all other surface landscape features, relocate offsite to secure location for future re-installment |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
17 |  |  |  | Removal of Outbuilding Contents, storage in secured area, and return of objects upon restoration |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
18 |  | 02 61 00 |  | Excavate, stockpile, load, haul and dispose at LTWMF Facility Contaminated soil and tree roots |  | cubic meters |  |  | 320 |  |  | $ | *** |  |  | $ | *** |
19 |  |  |  | Secondary Excavation (if required) |  | cubic meters |  |  |  |  |  | $ | *** |  |  |  |  |

Earthworks |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 31 00 01 |  | Supply, place, compact and grade clean imported fill per MPH SOP/SOGs (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 400 |  |  | $ | *** |  |  | $ | *** |
2 |  | 31 00 01 |  | Supply, place, compact and grade Granular A (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 60 |  |  | $ | *** |  |  | $ | *** |
3 |  | 31 00 01 |  | Supply, place, compact and grade Granular B (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 60 |  |  | $ | *** |  |  | $ | *** |
4 |  | 31 00 01 |  | Supply, place, and grade Topsoil |  | cubic meters |  |  | 60 |  |  | $ | *** |  |  | $ | *** |

Site Restoration |  |  |  |  |  |  |  |  |  | $ | *** |  |  | $ | *** |
1 |  | as per Drawings |  | Supply and Install shed as shown including all footings, floors etc. |  | square meters |  |  | 12.5 |  |  | $ | *** |  |  | $ | *** |
2 |  | as per Drawings |  | Supply, Place, Asphalt Driveway as per specifications |  | square meters |  |  | 90 |  |  | $ | *** |  |  | $ | *** |
3 |  | as per Drawings |  | Supply and Place concrete sidewalk as per specifications |  | square meters |  |  | 4 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 54 | Schedule 2

PROTECTED SENSITIVE

4 |  | as per Drawings |  | Supply and Place Paving stone / interlocking brick patio as per specifications |  | square meters |  |  | 7 |  |  | $ | *** |  |  | $ | *** |
5 |  | as per Drawings |  | Supply and Place concrete patio as per specifications |  | square meters |  |  | 10 |  |  | $ | *** |  |  | $ | *** |
6 |  | as per Drawings |  | Supply and Place retaining wall as per specifications |  | square meters |  |  | 26 |  |  | $ | *** |  |  | $ | *** |
7 |  | as per Drawings |  | Supply and Place concrete stairs as per specifications |  | treads |  |  | 13 |  |  | $ | *** |  |  | $ | *** |
8 |  | 31 32 50 |  | Water management, sampling, transportation, and disposal at LTMWF |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
9 |  | 32 90 00 |  | Landscape Restoration |  | Allowance |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
Total Price - 16 Alexander Street |  |  |  | $ | *** |

Group G Requirements - 14 Alexander Street |  |  |  |  |  |  |  |  |  |  |
Removals |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 02 61 00 |  | Pre-construction Property Condition Assessment |  | Lump Sum |  |  | 1 |  |  | $ | 21,006.39 |  |  | $ | 21,006.39 |
2 |  | 02 61 00 |  | Complete gamma survey and XRF scan of completed excavation surface |  | Lump Sum |  |  | 1 |  |  | $ | 1,340.26 |  |  | $ | 1,340.26 |
3 |  | 02 61 00 |  | Collection of soil sample for signature COPCs and the reporting of results following Laboratory Analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
4 |  | 02 61 00 |  | Laboratory analysis of soil sample for signature COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
5 |  | 02 61 00 |  | Collection of soil sample for secondary COPCs and the reporting of results following laboratory analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 55 | Schedule 2

PROTECTED SENSITIVE

6 |  | 02 61 00 |  | Laboratory analysis of composite soil sample for secondary COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
7 |  | 02 61 00 |  | Preparation and submission of Verification Documentation |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
8 |  | 02 41 16 |  | Demolish existing Site structures that require removal, verify not radiologically impacted and dispose off site a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
9 |  | 02 41 13 |  | Paving stone / interlocking brick patio removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 20 |  |  | $ | *** |  |  | $ | *** |
10 |  | 02 41 13 |  | Concrete Stair Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
11 |  | 31 11 00 |  | Remove and Dispose of Trees, shrubs, hedges, and all other plants above ground, verify not radiological impacted and dispose offsite at a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
12 |  |  |  | Remove all other surface landscape features, relocate offsite to secure location for future re-installment |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
13 |  |  |  | Removal of Outbuilding Contents, storage in secured area, and return of objects upon restoration |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
14 |  | 02 61 00 |  | Excavate, stockpile, load, haul and dispose at LTWMF Facility Contaminated soil and tree roots |  | cubic meters |  |  | 330 |  |  | $ | *** |  |  | $ | *** |
15 |  |  |  | Secondary Excavation (if required) |  | cubic meters |  |  |  |  |  | $ | *** |  |  |  |  |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 56 | Schedule 2

PROTECTED SENSITIVE

Earthworks |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 31 00 01 |  | Supply, place, compact and grade clean imported fill per MPH SOP/SOGs (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 340 |  |  | $ | *** |  |  | $ | *** |
2 |  | 31 00 01 |  | Supply, place, compact and grade Granular A (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 60 |  |  | $ | *** |  |  | $ | *** |
3 |  | 31 00 01 |  | Supply, place, compact and grade Granular B (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 60 |  |  | $ | *** |  |  | $ | *** |
4 |  | 31 00 01 |  | Supply, place, and grade Topsoil |  | cubic meters |  |  | 100 |  |  | $ | *** |  |  | $ | *** |

Site Restoration |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | as per Drawings |  | Supply and Install sheds as shown including all footings, etc., inluding all permits |  | square meters |  |  | 14 |  |  | $ | *** |  |  | $ | *** |
2 |  | as per Drawings |  | Supply and install Wooden Deck (rear) as shown including all permits |  | square meters |  |  | 5 |  |  | $ | *** |  |  | $ | *** |
3 |  | as per Drawings |  | Supply and Place Paving Stone / Interlocking Brick Patio as per specifications |  | square meters |  |  | 20 |  |  | $ | *** |  |  | $ | *** |
4 |  | as per Drawings |  | Supply and Place concrete stairs as per specifications |  | treads |  |  | 7 |  |  | $ | *** |  |  | $ | *** |
5 |  | 31 32 50 |  | Water management, sampling, transportation, and disposal at LTMWF |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
6 |  | 32 90 00 |  | Landscape Restoration |  | Allowance |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
Total Price - 14 Alexander Street |  |  | $ | *** |
Total Remediation, Earthworks and Restoration Only |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 57 | Schedule 2

PROTECTED SENSITIVE

|  | Specification Reference |  | Description |  | Unit of Measure |  | Estimated Quantity |  |  | Price per Unit |  |  | Total Price |
Group H - General Requirements |  |  |  |  |  |  |  |  |  |  |
1 |  | 02 61 00 |  | Mobilization and Project Startup |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
2 |  | 02 61 00 |  | Demobilization and Project Closeout |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
3 |  | 01 31 19 |  | Project Meetings |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
4 |  | 01 32 00 |  | Construction Progress Documentation |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
5 |  | 01 32 16 |  | Construction Progress Schedule |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
6 |  | 01 35 29 |  | Health and Safety Plan |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
7 |  | 01 35 29 |  | Implementation of Health and Safety - All Sites |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
8 |  | 01 35 30 |  | Radiation Protection Plan - All Sites |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
9 |  | 01 35 30 |  | Implementation of Radiation Protection - All Sites |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
10 |  | 01 35 43 |  | Environmental Protection Manual and Dust Management Plan - All Sites |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
11 |  | 01 35 43 |  | Implementation of Environmental Protection and Dust Management - All Sites |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
12 |  | 01 45 00 |  | Quality Assurance Plan |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
13 |  | 01 45 00 |  | Implementation of QA/QC - All Sites |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
14 |  | 01 51 00 |  | Provision and Maintenance of Temporary Utilities - (Contractor Use) |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
15 |  | 01 52 00 |  | Provision and Construction Facilities - All Sites |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
16 |  | 02 61 00 |  | Permitting as per OBC and MPH SOP-SOG, OMOECC, CN/CP - all sites |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 58 | Schedule 2

PROTECTED SENSITIVE

17 |  |  |  | Traffic Control - All sites |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
18 |  | 01 33 00 |  | All Other Submittals |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
19 |  | 01 14 00 |  | Site Security |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
20 |  |  |  | Bonding & Insurance |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
21 |  | 01 14 00 |  | Training and Security Clearance |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
22 |  | 01 78 00 |  | Closeout Submittal |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
23 |  | 01 56 00 |  | Supply, Install, Maintain, and Remove Sediment Erosion Control fencing |  | Linear meters |  |  | 185 |  |  | $ | *** |  |  | $ | *** |
24 |  | 01 56 00 |  | Supply, Install, Maintain, and Remove - Perimeter Safety Fencing |  | Linear meters |  |  | 550 |  |  | $ | *** |  |  | $ | *** |
25 |  | 02 61 00 |  | Supply, Install, Maintain and Remove Access Gates as shown |  | each |  |  | 10 |  |  | $ | *** |  |  | $ | *** |
26 |  | See Figure attached |  | Tree Protection Fencing |  | Linear meters |  |  | 120 |  |  | $ | *** |  |  | $ | *** |
Total Price - General Requirements |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 59 | Schedule 2

PROTECTED SENSITIVE

Group H Requirements - 39 Hayward Street

Removals |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 02 61 00 |  | Pre-construction Property Condition Assessment |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
2 |  | 02 61 00 |  | Complete gamma survey and XRF scan of completed excavation surface |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
3 |  | 02 61 00 |  | Collection of soil sample for signature COPCs and the reporting of results following Laboratory Analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
4 |  | 02 61 00 |  | Laboratory Analysis of soil sample for signature COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
5 |  | 02 61 00 |  | Collection of soil sample for secondary COPCs and the reporting of results following laboratory analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
6 |  | 02 61 00 |  | Laboratory Analysis of composite soil sample for secondary COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
7 |  | 02 61 00 |  | Preparation and Submission of Verification Documentation |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
8 |  | 02 41 16 |  | Demolish Existing Site Structures that require removal, verify not radiologically impacted and dispose off site a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
9 |  | 02 41 13 |  | Gravel Driveway Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 12 |  |  | $ | *** |  |  | $ | *** |
10 |  | 02 41 13 |  | Concrete Sidewalk Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 48 |  |  | $ | *** |  |  | $ | *** |
11 |  | 02 41 13 |  | Concrete Patio Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 3 |  |  | $ | *** |  |  | $ | *** |
12 |  | 02 41 13 |  | Paving Stone / Interlocking Brick Patio Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 23 |  |  | $ | *** |  |  | $ | *** |
13 |  | 02 41 13 |  | Remove existing fence, verify not radiologically impacted and dispose offiste at licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 60 | Schedule 2

PROTECTED SENSITIVE

14 |  | 02 41 13 |  | Remove Retaining Wall, verify not radiologically impacted and dispose offiste at licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
15 |  | 02 41 13 |  | Concrete Stairs Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
16 |  | 02 61 00 |  | Remove and Dispose of Trees, shrubs, hedges, and all other plants above ground, verify not radiological impacted and dispose offsite at a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
17 |  | 02 61 00 |  | Remove all other surface landscape features, relocate offsite to secure location for future re-installment |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
18 |  | 02 61 00 |  | Removal of Outbuilding Contents,Disposal at Licensed Offiste Facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
19 |  | 02 61 00 |  | Excavate, stockpile, load, haul and dispose at LTWMF Facility Contaminated soil and tree roots |  | cubic meters |  |  | 6,500 |  |  | $ | *** |  |  | $ | *** |
20 |  |  |  | Secondary Excavation (if required) |  | cubic meters |  |  |  |  |  | $ | *** |  |  |  |  |

Earthworks |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 31 00 01 |  | Supply, place, compact and grade clean imported fill per MPH SOP/SOGs (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 11,800 |  |  | $ | *** |  |  | $ | *** |
2 |  | 31 00 01 |  | Supply, place, compact and grade Granular A (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 200 |  |  | $ | *** |  |  | $ | *** |
3 |  | 31 00 01 |  | Supply, place, compact and grade Granular B (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 200 |  |  | $ | *** |  |  | $ | *** |
4 |  | 31 00 01 |  | Supply, place, and grade Topsoil |  | cubic meters |  |  | 400 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 61 | Schedule 2

PROTECTED SENSITIVE

Site Restoration |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 31 32 50 |  | Water management, sampling, transportation, and disposal at LTMWF |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
2 |  | 32 90 00 |  | Landscape Restoration |  | Allowance |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
3 |  |  |  | Supply and Commission Septic Field |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
Total Price - 39 Hayward Street |  |  | $ | *** |

Group H Requirements - 35 Hayward Street

Removals |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 02 61 00 |  | Pre-construction Property Condition Assessment |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
2 |  | 02 61 00 |  | Complete gamma survey and XRF scan of completed excavation surface |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
3 |  | 02 61 00 |  | Collection of soil sample for signature COPCs and the reporting of results following Laboratory Analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
4 |  | 02 61 00 |  | Laboratory analysis of soil sample for signature COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
5 |  | 02 61 00 |  | Collection of soil sample for secondary COPCs and the reporting of results following laboratory analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
6 |  | 02 61 00 |  | Laboratory analysis of composite soil sample for secondary COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 62 | Schedule 2

PROTECTED SENSITIVE

7 |  | 02 61 00 |  | Preparation and submission of Verification Documentation |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
8 |  | 02 41 16 |  | Demolish Existing Site Structures that require removal, verify not radiologically impacted and dispose off site a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
9 |  | 02 41 13 |  | Concrete Sidewalk Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 8 |  |  | $ | *** |  |  | $ | *** |
10 |  | 02 41 13 |  | Gravel Driveway Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 112 |  |  | $ | *** |  |  | $ | *** |
11 |  | 02 41 13 |  | Concrete Patio Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 4 |  |  | $ | *** |  |  | $ | *** |
12 |  | 02 41 13 |  | Remove existing fence, verify not radiologically impacted and dispose offiste at licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
13 |  | 31 11 00 |  | Remove and Dispose of Trees, shrubs, hedges, and all other plants above ground, verify not radiological impacted and dispose offsite at a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
14 |  | 02 61 00 |  | Remove all other surface landscape features, relocate offsite to secure location for future re-installment |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
15 |  | 02 61 00 |  | Excavate, stockpile, load, haul and dispose at LTWMF Facility Contaminated soil and tree roots |  | cubic meters |  |  | 1,120 |  |  | $ | *** |  |  | $ | *** |
16 |  |  |  | Secondary Excavation (if required) |  | cubic meters |  |  |  |  |  | $ | *** |  |  |  |  |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 63 | Schedule 2

PROTECTED SENSITIVE

Earthworks |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 31 00 01 |  | Supply, place, compact and grade clean imported fill per MPH SOP/SOGs (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 1,600 |  |  | $ | *** |  |  | $ | *** |
2 |  | 31 00 01 |  | Supply, place, compact and grade Granular A (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 120 |  |  | $ | *** |  |  | $ | *** |
3 |  | 31 00 01 |  | Supply, place, compact and grade Granular B (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 120 |  |  | $ | *** |  |  | $ | *** |
4 |  | 31 00 01 |  | Supply, place, and grade Topsoil |  | cubic meters |  |  | 200 |  |  | $ | *** |  |  | $ | *** |

Site Restoration |  |  |  |  |  |  |  |  |  | $ | *** |  |  | $ | *** |
1 |  | as per Drawings |  | Supply and Place Gravel Drivway as per specifications |  | square meters |  |  | 112 |  |  | $ | *** |  |  | $ | *** |
2 |  | as per Drawings |  | Supply and Place Concrete Sidewalk as per specifications |  | square meters |  |  | 8 |  |  | $ | *** |  |  | $ | *** |
3 |  | as per Drawings |  | Supply and install Wooden Deck (front) as shown including all permits |  | square meters |  |  | 2 |  |  | $ | *** |  |  | $ | *** |
4 |  | as per Drawings |  | Supply and install Wooden Deck (rear) as shown including all permits |  | square meters |  |  | 12 |  |  | $ | *** |  |  | $ | *** |
5 |  | as per Drawings |  | Supply and Place Concrete Sidewalk as per specifications |  | square meters |  |  | 4 |  |  | $ | *** |  |  | $ | *** |
6 |  | as per Drawings |  | Supply and Install Concrete Steps as per specifications |  | Treads |  |  | 6 |  |  | $ | *** |  |  | $ | *** |
7 |  | 31 32 50 |  | Water management, sampling, transportation, and disposal at LTMWF |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
8 |  | 32 90 00 |  | Landscape Restoration |  | Allowance |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
9 |  | as per Drawings |  | Supply and Place Fence |  | Linear meters |  |  | 13.00 |  |  | $ | *** |  |  | $ | *** |
Total Price - 35 Hayward Street |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 64 | Schedule 2

PROTECTED SENSITIVE

Group H Requirements - 58 Alexander Street

Removals |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 02 61 00 |  | Pre-construction Property Condition Assessment |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
2 |  | 02 61 00 |  | Complete gamma survey and XRF scan of completed excavation surface |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
3 |  | 02 61 00 |  | Collection of soil sample for signature COPCs and the reporting of results following Laboratory Analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
4 |  | 02 61 00 |  | Laboratory analysis of soil sample for signature COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
5 |  | 02 61 00 |  | Collection of soil sample for secondary COPCs and the reporting of results following laboratory analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
6 |  | 02 61 00 |  | Laboratory analysis of composite soil sample for secondary COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
7 |  | 02 61 00 |  | Preparation and submission of Verification Documentation |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
8 |  | 02 41 16 |  | Demolish Existing Site Structures that require removal, verify not radiologically impacted and dispose off site a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
9 |  | 02 41 13 |  | Concrete Sidewalk Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 28 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 65 | Schedule 2

PROTECTED SENSITIVE

10 |  | 02 41 13 |  | Paving Stone / Interlocking Brick Sidewalk Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 5 |  |  | $ | *** |  |  | $ | *** |
11 |  | 02 41 13 |  | Concrete Patio Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 16 |  |  | $ | *** |  |  | $ | *** |
12 |  | 02 41 13 |  | Remove existing fence, verify not radiologically impacted and dispose offiste at licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
13 |  | 31 11 00 |  | Remove and Dispose of Trees, shrubs, hedges, and all other plants above ground, verify not radiological impacted and dispose offsite at a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
14 |  | 02 41 13 |  | Remove all other surface landscape features, relocate offsite to secure location for future re-installment |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
15 |  | 02 41 13 |  | Removal of Outbuilding Contents, storage in secured area, and return of objects upon restoration |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
16 |  | 02 61 00 |  | Excavate, stockpile, load, haul and dispose at LTWMF Facility Contaminated soil and tree roots |  | cubic meters |  |  | 260 |  |  | $ | *** |  |  | $ | *** |
17 |  |  |  | Secondary Excavation (if required) |  | cubic meters |  |  |  |  |  | $ | *** |  |  |  |  |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 66 | Schedule 2

PROTECTED SENSITIVE

Earthworks |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 31 00 01 |  | Supply, place, compact and grade clean imported fill per MPH SOP/SOGs (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 240 |  |  | $ | *** |  |  | $ | *** |
2 |  | 31 00 01 |  | Supply, place, compact and grade Granular A (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 60 |  |  | $ | *** |  |  | $ | *** |
3 |  | 31 00 01 |  | Supply, place, compact and grade Granular B (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 60 |  |  | $ | *** |  |  | $ | *** |
4 |  | 31 00 01 |  | Supply, place, and grade Topsoil |  | cubic meters |  |  | 80 |  |  | $ | *** |  |  | $ | *** |

Site Restoration |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | as per Drawings |  | Supply and Install sheds as shown including all footings, etc., inluding all permits |  | square meters |  |  | 3 |  |  | $ | *** |  |  | $ | *** |
2 |  | as per Drawings |  | Supply and Place Concrete Sidewalk as per specifications |  | square meters |  |  | 28 |  |  | $ | *** |  |  | $ | *** |
3 |  | as per Drawings |  | Supply and Place Concrete Patio as per specifications |  | square meters |  |  | 16 |  |  | $ | *** |  |  | $ | *** |
4 |  | as per Drawings |  | Supply and install Wooden Deck (rear) as shown including all permits |  | square meters |  |  | 11 |  |  | $ | *** |  |  | $ | *** |
5 |  | as per Drawings |  | Supply and install Wooden Deck (other) as shown including all permits |  | square meters |  |  | 31 |  |  | $ | *** |  |  | $ | *** |
6 |  | 32 90 00 |  | Landscape Restoration |  | Allowance |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
7 |  | 31 32 50 |  | Water management, sampling, transportation, and disposal at LTMWF |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
8 |  | as per Drawings |  | Supply and Place Fence |  | Linear meters |  |  | 14.00 |  |  | $ | *** |  |  | $ | *** |
Total Price - 58 Alexander Street |  |  |  |  |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 67 | Schedule 2

PROTECTED SENSITIVE

Group H Requirements - 50 Alexander Street

Removals |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 02 61 00 |  | Pre-construction Property Condition Assessment |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
2 |  | 02 61 00 |  | Complete gamma survey and XRF scan of completed excavation surface |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
3 |  | 02 61 00 |  | Collection of soil sample for signature COPCs and the reporting of results following Laboratory Analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
4 |  | 02 61 00 |  | Laboratory analysis of soil sample for signature COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
5 |  | 02 61 00 |  | Collection of soil sample for secondary COPCs and the reporting of results following laboratory analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
6 |  | 02 61 00 |  | Laboratory analysis of composite soil sample for secondary COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
7 |  | 02 61 00 |  | Preparation and submission of Verification Documentation |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
8 |  | 02 41 16 |  | Demolish existing Site structures that require removal, verify not radiologically impacted and dispose off site a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
9 |  | 02 41 13 |  | Gravel Driveway Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 46 |  |  | $ | *** |  |  | $ | *** |
10 |  | 02 41 13 |  | Concrete Driveway Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 6 |  |  | $ | *** |  |  | $ | *** |
11 |  | 02 41 13 |  | Concrete Sidewalk Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 13 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 68 | Schedule 2

PROTECTED SENSITIVE

12 |  | 02 41 13 |  | Remove existing fence, verify not radiologically impacted and dispose offiste at licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
13 |  | 02 41 13 |  | Retaining Wall Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
14 |  | 02 41 13 |  | Concrete Stair Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
15 |  | 31 11 00 |  | Remove and Dispose of Trees, shrubs, hedges, and all other plants above ground, verify not radiological impacted and dispose offsite at a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
16 |  | 02 41 13 |  | Remove all other surface landscape features, relocate offsite to secure location for future re-installment |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
17 |  | 02 41 13 |  | Removal of Outbuilding Contents, storage in secured area, and return of objects upon restoration |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
18 |  | 02 61 00 |  | Excavate, stockpile, load, haul and dispose at LTWMF Facility Contaminated soil and tree roots |  | cubic meters |  |  | 870 |  |  | $ | *** |  |  | $ | *** |
19 |  |  |  | Secondary Excavation (if required) |  | cubic meters |  |  |  |  |  | $ | *** |  |  |  |  |
Earthworks |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 31 00 01 |  | Supply, place, compact and grade clean imported fill per MPH SOP/SOGs (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 1,240 |  |  | $ | *** |  |  | $ | *** |
2 |  | 31 00 01 |  | Supply, place, compact and grade Granular A (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 100 |  |  | $ | *** |  |  | $ | *** |
3 |  | 31 00 01 |  | Supply, place, compact and grade Granular B (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 100 |  |  | $ | *** |  |  | $ | *** |
4 |  | 31 00 01 |  | Supply, place, and grade Topsoil |  | cubic meters |  |  | 150 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 69 | Schedule 2

PROTECTED SENSITIVE

Site Restoration |  |  |  |  |  |  |  | $ | *** |  |  | $ | *** |
1 |  | as per Drawings |  | Supply and Install shed as shown including all footings, etc., inluding all permits |  | square meters |  |  | 13 |  |  | $ | *** |  |  | $ | *** |
2 |  | as per Drawings |  | Supply and Install detached garage as shown including all footings, etc., inluding all permits |  | square meters |  |  | 26 |  |  | $ | *** |  |  | $ | *** |
3 |  | as per Drawings |  | Supply and Place Concrete Sidewalk as per specifications |  | square meters |  |  | 13 |  |  | $ | *** |  |  | $ | *** |
4 |  | as per Drawings |  | Supply and Place Concrete Drivway as per specifications |  | square meters |  |  | 6 |  |  | $ | *** |  |  | $ | *** |
5 |  | as per Drawings |  | Supply and Place Gravel Drivway as per specifications |  | square meters |  |  | 46 |  |  | $ | *** |  |  | $ | *** |
6 |  | as per Drawings |  | Supply and install Wooden Deck (rear) as shown including all permits |  | square meters |  |  | 2 |  |  | $ | *** |  |  | $ | *** |
7 |  | as per Drawings |  | Supply and install Covered Porch (front) as shown including all permits |  | square meters |  |  | 7 |  |  | $ | *** |  |  | $ | *** |
8 |  | as per Drawings |  | Supply and Install Concrete Steps as per specifications |  | Treads |  |  | 3 |  |  | $ | *** |  |  | $ | *** |
9 |  | as per Drawings |  | Supply and Place Retaining Wall as per specifications |  | Linear meters |  |  | 18 |  |  | $ | *** |  |  | $ | *** |
10 |  | 31 32 50 |  | Water management, sampling, transportation, and disposal at LTMWF |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
11 |  | 32 90 00 |  | Landscape Restoration |  | Allowance |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
12 |  | as per Drawings |  | Supply and Place Fence |  | Linear meters |  |  | 29.00 |  |  | $ | *** |  |  | $ | *** |
Total Price - 50 Alexander Street |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 70 | Schedule 2

PROTECTED SENSITIVE

Group H Requirements - 54 Alexander Street

Removals |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 02 61 00 |  | Pre-construction Property Condition Assessment |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
2 |  | 02 61 00 |  | Complete gamma survey and XRF scan of completed excavation surface |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
3 |  | 02 61 00 |  | Collection of soil sample for signature COPCs and the reporting of results following Laboratory Analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
4 |  | 02 61 00 |  | Laboratory analysis of soil sample for signature COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
5 |  | 02 61 00 |  | Collection of soil sample for secondary COPCs and the reporting of results following laboratory analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
6 |  | 02 61 00 |  | Laboratory analysis of composite soil sample for secondary COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
7 |  | 02 61 00 |  | Preparation and submission of Verification Documentation |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
8 |  | 02 41 16 |  | Demolish existing Site structures that require removal, verify not radiologically impacted and dispose off site a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
9 |  | 02 41 13 |  | Asphalt Driveway Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 75 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 71 | Schedule 2

PROTECTED SENSITIVE

10 |  | 02 41 13 |  | Concrete Stair Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
11 |  | 02 41 13 |  | Remove Retaining Wall - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
12 |  | 02 41 13 |  | Remove existing fence, verify not radiologically impacted and dispose offiste at licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
13 |  | 31 11 00 |  | Remove and Dispose of Trees, shrubs, hedges, and all other plants above ground, verify not radiological impacted and dispose offsite at a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
14 |  |  |  | Remove all other surface landscape features, relocate offsite to secure location for future re-installment |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
15 |  |  |  | Removal of Outbuilding Contents, storage in secured area, and return of objects upon restoration |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
16 |  | 02 61 00 |  | Excavate, stockpile, load, haul and dispose at LTWMF Facility Contaminated soil and tree roots |  | cubic meters |  |  | 370 |  |  | $ | *** |  |  | $ | *** |
17 |  |  |  | Secondary Excavation (if required) |  | cubic meters |  |  |  |  |  | $ | *** |  |  |  |  |
Earthworks |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 31 00 01 |  | Supply, place, compact and grade clean imported fill per MPH SOP/SOGs (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 380 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 72 | Schedule 2

PROTECTED SENSITIVE

2 |  | 31 00 01 |  | Supply, place, compact and grade Granular A (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 80 |  |  | $ | *** |  |  | $ | *** |
3 |  | 31 00 01 |  | Supply, place, compact and grade Granular B (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 80 |  |  | $ | *** |  |  | $ | *** |
4 |  | 31 00 01 |  | Supply, place, and grade Topsoil |  | cubic meters |  |  | 100 |  |  | $ | *** |  |  | $ | *** |
Site Restoration |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | as per Drawings |  | Supply and Install detached garage as shown including all footings, etc., inluding all permits |  | square meters |  |  | 27 |  |  | $ | *** |  |  | $ | *** |
2 |  | as per Drawings |  | Supply and Place Asphalt Drivway as per specifications |  | square meters |  |  | 75 |  |  | $ | *** |  |  | $ | *** |
3 |  | as per Drawings |  | Supply and install Wooden Deck (rear) as shown including all permits |  | square meters |  |  | 10 |  |  | $ | *** |  |  | $ | *** |
4 |  | as per Drawings |  | Supply and Place Retaining Wall as per specifications |  | Linear meters |  |  | 21 |  |  | $ | *** |  |  | $ | *** |
5 |  | as per Drawings |  | Supply and Place concrete stairs as per specifications |  | treads |  |  | 2 |  |  | $ | *** |  |  | $ | *** |
6 |  | 31 32 50 |  | Water management, sampling, transportation, and disposal at LTMWF |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
7 |  | 32 90 00 |  | Landscape Restoration |  | Allowance |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
8 |  | as per Drawings |  | Supply and Place Fence |  | Linear meters |  |  | 28.00 |  |  | $ | *** |  |  | $ | *** |
Total Price - 54 Alexander Street | $ | *** |

Group H Requirements - 60 Alexander Street

Removals |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 02 61 00 |  | Pre-construction Property Condition Assessment |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 73 | Schedule 2

PROTECTED SENSITIVE

2 |  | 02 61 00 |  | Complete gamma survey and XRF scan of completed excavation surface |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
3 |  | 02 61 00 |  | Collection of soil sample for signature COPCs and the reporting of results following Laboratory Analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
4 |  | 02 61 00 |  | Laboratory analysis of soil sample for signature COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
5 |  | 02 61 00 |  | Collection of soil sample for secondary COPCs and the reporting of results following laboratory analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
6 |  | 02 61 00 |  | Laboratory analysis of composite soil sample for secondary COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
7 |  | 02 61 00 |  | Preparation and submission of Verification Documentation |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
8 |  | 02 41 16 |  | Demolish existing Site structures that require removal, verify not radiologically impacted and dispose off site a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
9 |  | 02 41 13 |  | Concrete sidewalk removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 2 |  |  | $ | *** |  |  | $ | *** |
10 |  | 02 41 13 |  | Concrete patio removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 19 |  |  | $ | *** |  |  | $ | *** |
11 |  | 02 41 13 |  | Remove retaining wall, verify not radiologically impacted and dispose offiste at licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 74 | Schedule 2

PROTECTED SENSITIVE

12 |  | 02 41 13 |  | Concrete Stair Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
13 |  | 02 41 13 |  | Remove existing fence, verify not radiologically impacted and dispose offiste at licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
14 |  | 31 11 00 |  | Remove and Dispose of Trees, shrubs, hedges, and all other plants above ground, verify not radiological impacted and dispose offsite at a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
15 |  | 02 41 13 |  | Remove all other surface landscape features, relocate offsite to secure location for future re-installment |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
16 |  | 02 41 13 |  | Removal of Outbuilding Contents, storage in secured area, and return of objects upon restoration |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
17 |  | 02 61 00 |  | Excavate, stockpile, load, haul and dispose at LTWMF Facility Contaminated soil and tree roots |  | cubic meters |  |  | 270 |  |  | $ | *** |  |  | $ | *** |
18 |  |  |  | Secondary Excavation (if required) |  | cubic meters |  |  |  |  |  | $ | *** |  |  |  |  |
Earthworks |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 31 00 01 |  | Supply, place, compact and grade clean imported fill per MPH SOP/SOGs (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 280 |  |  | $ | *** |  |  | $ | *** |
2 |  | 31 00 01 |  | Supply, place, compact and grade Granular A (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 60 |  |  | $ | *** |  |  | $ | *** |
3 |  | 31 00 01 |  | Supply, place, compact and grade Granular B (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 60 |  |  | $ | *** |  |  | $ | *** |
4 |  | 31 00 01 |  | Supply, place, and grade Topsoil |  | cubic meters |  |  | 70 |  |  | $ | *** |  |  | $ | *** |
Site Restoration |  |  |  |  |  |  |  |  |  | $ | *** |  |  | $ | *** |
1 |  | as per Drawings |  | Supply and Install shed as shown including all footings, floors etc. |  | square meters |  |  | 9 |  |  | $ | *** |  |  | $ | *** |
2 |  | as per Drawings |  | Supply and Place concrete sidewalk as per specifications |  | square meters |  |  | 2 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 75 | Schedule 2

PROTECTED SENSITIVE

3 |  | as per Drawings |  | Supply and Place concrete patio as per specifications |  | square meters |  |  | 10 |  |  | $ | *** |  |  | $ | *** |
4 |  | as per Drawings |  | Supply and Install wooden deck (other) as shown including all footings, floors etc. |  | square meters |  |  | 7 |  |  | $ | *** |  |  | $ | *** |
5 |  | as per Drawings |  | Supply and Place retaining wall as per specifications |  | Linear meters |  |  | 14 |  |  | $ | *** |  |  | $ | *** |
6 |  | as per Drawings |  | Supply and Place concrete stairs as per specifications |  | treads |  |  | 4 |  |  | $ | *** |  |  | $ | *** |
7 |  | 31 32 50 |  | Water management, sampling, transportation, and disposal at LTMWF |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
8 |  | 32 90 00 |  | Landscape Restoration |  | Allowance |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
9 |  | as per Drawings |  | Supply and Place Fence |  | Linear meters |  |  | 40.00 |  |  | $ | *** |  |  | $ | *** |
Total Price - 60 Alexander Street | $ | *** |

Group H Requirements - 64 Alexander Street

Removals |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 02 61 00 |  | Pre-construction Property Condition Assessment |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 76 | Schedule 2

PROTECTED SENSITIVE

2 |  | 02 61 00 |  | Complete gamma survey and XRF scan of completed excavation surface |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
3 |  | 02 61 00 |  | Collection of soil sample for signature COPCs and the reporting of results following Laboratory Analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
4 |  | 02 61 00 |  | Laboratory analysis of soil sample for signature COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
5 |  | 02 61 00 |  | Collection of soil sample for secondary COPCs and the reporting of results following laboratory analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
6 |  | 02 61 00 |  | Laboratory analysis of composite soil sample for secondary COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
7 |  | 02 61 00 |  | Preparation and submission of Verification Documentation |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
8 |  | 02 41 16 |  | Demolish existing Site structures that require removal, verify not radiologically impacted and dispose off site a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
9 |  | 02 41 13 |  | Paving stone / interlocking brick sidewalk removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 3 |  |  | $ | *** |  |  | $ | *** |
10 |  | 02 41 13 |  | Concrete Driveway removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 85 |  |  | $ | *** |  |  | $ | *** |
11 |  | 02 41 13 |  | Remove retaining wall, verify not radiologically impacted and dispose offiste at licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 77 | Schedule 2

PROTECTED SENSITIVE

12 |  | 31 11 00 |  | Remove and Dispose of Trees, shrubs, hedges, and all other plants above ground, verify not radiological impacted and dispose offsite at a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
13 |  | 02 41 13 |  | Remove all other surface landscape features, relocate offsite to secure location for future re-installment |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
14 |  | 02 41 13 |  | Removal of Outbuilding Contents, storage in secured area, and return of objects upon restoration |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
15 |  | 02 61 00 |  | Excavate, stockpile, load, haul and dispose at LTWMF Facility Contaminated soil and tree roots |  | cubic meters |  |  | 560 |  |  | $ | *** |  |  | $ | *** |
17 |  |  |  | Secondary Excavation (if required) |  | cubic meters |  |  |  |  |  | $ | *** |  |  |  |  |
Earthworks |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 31 00 01 |  | Supply, place, compact and grade clean imported fill per MPH SOP/SOGs (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 600 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 78 | Schedule 2

PROTECTED SENSITIVE

2 |  | 31 00 01 |  | Supply, place, compact and grade Granular A (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 100 |  |  | $ | *** |  |  | $ | *** |
3 |  | 31 00 01 |  | Supply, place, compact and grade Granular B (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 100 |  |  | $ | *** |  |  | $ | *** |
4 |  | 31 00 01 |  | Supply, place, and grade Topsoil |  | cubic meters |  |  | 160 |  |  | $ | *** |  |  | $ | *** |
Site Restoration |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | as per Drawings |  | Supply and Install shed as shown including all footings, etc., inluding all permits |  | square meters |  |  | 15 |  |  | $ | *** |  |  | $ | *** |
2 |  | as per Drawings |  | Supply and Install detached garage as shown including all footings, etc., inluding all permits |  | square meters |  |  | 27 |  |  | $ | *** |  |  | $ | *** |
3 |  | as per Drawings |  | Supply and Place concrete driveway as per specifications |  | square meters |  |  | 85 |  |  | $ | *** |  |  | $ | *** |
4 |  | as per Drawings |  | Supply and Place concrete patio as per specifications |  | square meters |  |  | 10 |  |  | $ | *** |  |  | $ | *** |
5 |  | as per Drawings |  | Supply and Install wooden deck (other) as shown including all footings, floors etc. |  | square meters |  |  | 11 |  |  | $ | *** |  |  | $ | *** |
6 |  | as per Drawings |  | Supply and Install covered porch (front) as shown including all footings, floors etc. |  | square meters |  |  | 17 |  |  | $ | *** |  |  | $ | *** |
7 |  | as per Drawings |  | Supply and Place retaining wall as per specifications |  | Linear meters |  |  | 11 |  |  | $ | *** |  |  | $ | *** |
8 |  | 31 32 50 |  | Water management, sampling, transportation, and disposal at LTMWF |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
9 |  | 32 90 00 |  | Landscape Restoration |  | Allowance |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
10 |  | as per Drawings |  | Supply and Place Fence |  | Linear meters |  |  | 61.00 |  |  | $ | *** |  |  | $ | *** |
Total Price - 64 Alexander Street | $ | *** |

Group H Requirements - 68 Alexander Street

Removals |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 02 61 00 |  | Pre-construction Property Condition Assessment |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
2 |  | 02 61 00 |  | Complete gamma survey and XRF scan of completed excavation surface |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 79 | Schedule 2

PROTECTED SENSITIVE

3 |  | 02 61 00 |  | Collection of soil sample for signature COPCs and the reporting of results following Laboratory Analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
4 |  | 02 61 00 |  | Laboratory analysis of soil sample for signature COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
5 |  | 02 61 00 |  | Collection of soil sample for secondary COPCs and the reporting of results following laboratory analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
6 |  | 02 61 00 |  | Laboratory analysis of composite soil sample for secondary COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
7 |  | 02 61 00 |  | Preparation and submission of Verification Documentation |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
8 |  | 02 41 16 |  | Demolish existing Site structures that require removal, verify not radiologically impacted and dispose off site a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
9 |  | 02 41 13 |  | Concrete Driveway removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 49 |  |  | $ | *** |  |  | $ | *** |
10 |  | 02 41 13 |  | Concrete Sidewalk removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 45 |  |  | $ | *** |  |  | $ | *** |
11 |  | 02 41 13 |  | Paving Stone / Interlocking Brick Patio removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 5 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 80 | Schedule 2

PROTECTED SENSITIVE

12 |  | 02 41 13 |  | Retaining Wall Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
13 |  | 02 41 13 |  | Concrete Stair Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
14 |  | 02 41 13 |  | Remove existing fence, verify not radiologically impacted and dispose offiste at licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
15 |  | 31 11 00 |  | Remove and Dispose of Trees, shrubs, hedges, and all other plants above ground, verify not radiological impacted and dispose offsite at a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
16 |  | 02 41 13 |  | Remove all other surface landscape features, relocate offsite to secure location for future re-installment |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
17 |  | 02 41 13 |  | Removal of Outbuilding Contents, storage in secured area, and return of objects upon restoration |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
18 |  | 02 61 00 |  | Excavate, stockpile, load, haul and dispose at LTWMF Facility Contaminated soil and tree roots |  | cubic meters |  |  | 850 |  |  | $ | *** |  |  | $ | *** |
19 |  |  |  | Secondary Excavation (if required) |  | cubic meters |  |  |  |  |  | $ | *** |  |  |  |  |
Earthworks |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 31 00 01 |  | Supply, place, compact and grade clean imported fill per MPH SOP/SOGs (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 940 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 81 | Schedule 2

PROTECTED SENSITIVE

2 |  | 31 00 01 |  | Supply, place, compact and grade Granular A (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 160 |  |  | $ | *** |  |  | $ | *** |
3 |  | 31 00 01 |  | Supply, place, compact and grade Granular B (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 160 |  |  | $ | *** |  |  | $ | *** |
4 |  | 31 00 01 |  | Supply, place, and grade Topsoil |  | cubic meters |  |  | 220 |  |  | $ | *** |  |  | $ | *** |
Site Restoration |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | as per Drawings |  | Supply and Install sheds as shown including all footings, etc., inluding all permits |  | square meters |  |  | 6 |  |  | $ | *** |  |  | $ | *** |
2 |  | as per Drawings |  | Supply and Install attached car port as shown including all footings, etc., inluding all permits |  | square meters |  |  | 37 |  |  | $ | *** |  |  | $ | *** |
3 |  | as per Drawings |  | Supply and Place Paving Stone / Interlocking Brick Patio as per specifications |  | square meters |  |  | 5 |  |  | $ | *** |  |  | $ | *** |
4 |  | as per Drawings |  | Supply and Place concrete driveway as per specifications |  | square meters |  |  | 49 |  |  | $ | *** |  |  | $ | *** |
5 |  | as per Drawings |  | Supply and Place concrete sidewalk as per specifications |  | square meters |  |  | 45 |  |  | $ | *** |  |  | $ | *** |
6 |  | as per Drawings |  | Supply and Install wooden deck (rear) as shown including all footings, floors etc. |  | square meters |  |  | 17 |  |  | $ | *** |  |  | $ | *** |
7 |  | as per Drawings |  | Supply and Install covered porch (front) as shown including all footings, floors etc. |  | square meters |  |  | 7 |  |  | $ | *** |  |  | $ | *** |
8 |  | as per Drawings |  | Supply and Place concrete stairs as per specifications |  | treads |  |  | 2 |  |  | $ | *** |  |  | $ | *** |
9 |  | as per Drawings |  | Supply and Place retaining wall as per specifications |  | Linear meters |  |  | 5 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 82 | Schedule 2

PROTECTED SENSITIVE

10 |  | 31 32 50 |  | Water management, sampling, transportation, and disposal at LTMWF |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
11 |  | 32 90 00 |  | Landscape Restoration |  | Allowance |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
12 |  | as per Drawings |  | Supply and Place Fence |  | Linear meters |  |  | 6.00 |  |  | $ | *** |  |  | $ | *** |
Total Price - 68 Alexander Street | $ | *** |

Group H Requirements - PT PL 7 SS Haywood

Removals |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 02 61 00 |  | Pre-construction Property Condition Assessment |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
2 |  | 02 61 00 |  | Complete gamma survey and XRF scan of completed excavation surface |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
3 |  | 02 61 00 |  | Collection of soil sample for signature COPCs and the reporting of results following Laboratory Analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
4 |  | 02 61 00 |  | Laboratory analysis of soil sample for signature COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
5 |  | 02 61 00 |  | Collection of soil sample for secondary COPCs and the reporting of results following laboratory analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
6 |  | 02 61 00 |  | Laboratory analysis of composite soil sample for secondary COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
7 |  | 02 61 00 |  | Preparation and submission of Verification Documentation |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 83 | Schedule 2

PROTECTED SENSITIVE

8 |  | 31 11 00 |  | Remove and Dispose of Trees, shrubs, hedges, and all other plants above ground, verify not radiological impacted and dispose offsite at a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
9 |  | 02 61 00 |  | Excavate, stockpile, load, haul and dispose at LTWMF Facility Contaminated soil and tree roots |  | cubic meters |  |  | 240 |  |  | $ | *** |  |  | $ | *** |
10 |  |  |  | Secondary Excavation (if required) |  | cubic meters |  |  |  |  |  | $ | *** |  |  |  |  |
Earthworks |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 31 00 01 |  | Supply, place, compact and grade clean imported fill per MPH SOP/SOGs (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 280 |  |  | $ | *** |  |  | $ | *** |
2 |  | 31 00 01 |  | Supply, place, compact and grade Granular A (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 0 |  |  | $ | *** |  |  | $ | *** |
3 |  | 31 00 01 |  | Supply, place, compact and grade Granular B (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 0 |  |  | $ | *** |  |  | $ | *** |
4 |  | 31 00 01 |  | Supply, place, and grade Topsoil |  | cubic meters |  |  | 100 |  |  | $ | *** |  |  | $ | *** |
Site Restoration |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 31 32 50 |  | Water management, sampling, transportation, and disposal at LTMWF |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
2 |  | 32 90 00 |  | Landscape Restoration |  | Allowance |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
Total Price - PT PL 7 SS Haywood | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 84 | Schedule 2

PROTECTED SENSITIVE

Group H Requirements - LT 7 SS Haywood

Removals |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 02 61 00 |  | Pre-construction Property Condition Assessment |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
2 |  | 02 61 00 |  | Complete gamma survey and XRF scan of completed excavation surface |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
3 |  | 02 61 00 |  | Collection of soil sample for signature COPCs and the reporting of results following Laboratory Analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
4 |  | 02 61 00 |  | Laboratory analysis of soil sample for signature COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
5 |  | 02 61 00 |  | Collection of soil sample for secondary COPCs and the reporting of results following laboratory analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
6 |  | 02 61 00 |  | Laboratory analysis of composite soil sample for secondary COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
7 |  | 02 61 00 |  | Preparation and submission of Verification Documentation |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
8 |  | 31 11 00 |  | Remove and Dispose of Trees, shrubs, hedges, and all other plants above ground, verify not radiological impacted and dispose offsite at a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
9 |  | 02 61 00 |  | Excavate, stockpile, load, haul and dispose at LTWMF Facility Contaminated soil and tree roots |  | cubic meters |  |  | 440 |  |  | $ | *** |  |  | $ | *** |
10 |  |  |  | Secondary Excavation (if required) |  | cubic meters |  |  |  |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 85 | Schedule 2

PROTECTED SENSITIVE

Earthworks |  |  |  |  |  |  |  |  |  |  |  | $ | *** |  |  | $ | *** |
1 |  | 31 00 01 |  | Supply, place, compact and grade clean imported fill per MPH SOP/SOGs (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 640 |  |  | $ | *** |  |  | $ | *** |
2 |  | 31 00 01 |  | Supply, place, compact and grade Granular A (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 0 |  |  | $ | *** |  |  | $ | *** |
3 |  | 31 00 01 |  | Supply, place, compact and grade Granular B (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 0 |  |  | $ | *** |  |  | $ | *** |
4 |  | 31 00 01 |  | Supply, place, and grade Topsoil |  | cubic meters |  |  | 120 |  |  | $ | *** |  |  | $ | *** |
Site Restoration |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 31 32 50 |  | Water management, sampling, transportation, and disposal at LTMWF |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
2 |  | 32 90 00 |  | Landscape Restoration |  | Allowance |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
Total Price - LT 7 SS Haywood | $ | *** |
Total Remediation, Earthworks and Restoration Only | $ | *** |

|  | Specification Reference |  | Description |  | Unit of Measure |  | Estimated Quantity |  |  | Price per Unit |  |  | Total Price |
Group I - General Requirements |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 02 61 00 |  | Mobilization and Project Startup |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
2 |  | 02 61 00 |  | Demobilization and Project Closeout |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
3 |  | 01 31 19 |  | Project Meetings |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
4 |  | 01 32 00 |  | Construction Progress Documentation |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
5 |  | 01 32 16 |  | Construction Progress Schedule |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 86 | Schedule 2

PROTECTED SENSITIVE

6 |  | 01 35 29 |  | Health and Safety Plan |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
7 |  | 01 35 29 |  | Implementation of Health and Safety - All Sites |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
8 |  | 01 35 30 |  | Radiation Protection Plan - All Sites |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
9 |  | 01 35 30 |  | Implementation of Radiation Protection - All Sites |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
10 |  | 01 35 43 |  | Environmental Protection Manual and Dust Management Plan - All Sites |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
11 |  | 01 35 43 |  | Implementation of Environmental Protection and Dust Management - All Sites |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
12 |  | 01 45 00 |  | Quality Assurance Plan |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
13 |  | 01 45 00 |  | Implementation of QA/QC - All Sites |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
14 |  | 01 51 00 |  | Provision and Maintenance of Temporary Utilities - (Contractor Use) |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
15 |  | 01 52 00 |  | Provision and Construction Facilities - All Sites |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
16 |  | 02 61 00 |  | Permitting as per OBC and MPH SOP-SOG, OMOECC, CN/CP - all sites |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
17 |  |  |  | Traffic Control - All sites |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
18 |  | 01 33 00 |  | All Other Submittals |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
19 |  | 01 14 00 |  | Site Security |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
20 |  |  |  | Bonding & Insurance |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
21 |  | 01 14 00 |  | Training and Security Clearance |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
22 |  | 01 78 00 |  | Closeout Submittal |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 87 | Schedule 2

PROTECTED SENSITIVE

23 |  | 01 56 00 |  | Supply, Install, Maintain, and Remove Sediment Erosion Control fencing |  | Linear meters |  |  | 95 |  |  | $ | *** |  |  | $ | *** |
24 |  | 01 56 00 |  | Supply, Install, Maintain, and Remove - Perimeter Safety Fencing |  | Linear meters |  |  | 185 |  |  | $ | *** |  |  | $ | *** |
25 |  | 02 61 00 |  | Supply, Install, Maintain and Remove Access Gates as shown |  | each |  |  | 4 |  |  | $ | *** |  |  | $ | *** |
26 |  | See Figure Attached |  | Tree Protecton Fencing |  | Linear meters |  |  | 40 |  |  | $ | *** |  |  | $ | *** |
Total Price - General Requirements | $ | *** |

Group I Requirements - 34 Smith Street

Removals |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 02 61 00 |  | Pre-construction Property Condition Assessment |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
2 |  | 02 61 00 |  | Complete gamma survey and XRF scan of completed excavation surface |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
3 |  | 02 61 00 |  | Collection of soil sample for signature COPCs and the reporting of results following Laboratory Analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
4 |  | 02 61 00 |  | Laboratory Analysis of soil sample for signature COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
5 |  | 02 61 00 |  | Collection of soil sample for secondary COPCs and the reporting of results following laboratory analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
6 |  | 02 61 00 |  | Laboratory Analysis of composite soil sample for secondary COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
7 |  | 02 61 00 |  | Preparation and Submission of Verification Documentation |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 88 | Schedule 2

PROTECTED SENSITIVE

8 |  | 02 41 16 |  | Demolish Existing Site Structures that require removal, verify not radiologically impacted and dispose off site a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
9 |  | 02 41 13 |  | Retaining Wall Removal - verify not radiologically impacted, offsite disposal at a licensed receiving facility, include all necessary support and bracing as required |  | Lump sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
10 |  | 02 61 00 |  | Remove and Dispose of Trees, shrubs, hedges, and all other plants above ground, verify not radiological impacted and dispose offsite at a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
11 |  | 02 61 00 |  | Remove all other surface landscape features, relocate offsite to secure location for future re-installment |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
12 |  | 02 61 00 |  | Excavate, stockpile, load, haul and dispose at LTWMF Facility Contaminated soil and tree roots |  | cubic meters |  |  | 110 |  |  | $ | *** |  |  | $ | *** |
13 |  |  |  | Secondary Excavation (if requried) |  | cubic meters |  |  |  |  |  | $ | *** |  |  |  |  |
Earthworks |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 31 00 01 |  | Supply, place, compact and grade clean imported fill per MPH SOP/SOGs (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 120 |  |  | $ | *** |  |  | $ | *** |
2 |  | 31 00 01 |  | Supply, place, compact and grade Granular A (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 10 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 89 | Schedule 2

PROTECTED SENSITIVE

3 |  | 31 00 01 |  | Supply, place, compact and grade Granular B (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 10 |  |  | $ | *** |  |  | $ | *** |
4 |  | 31 00 01 |  | Supply, place, and grade Topsoil |  | cubic meters |  |  | 40 |  |  | $ | *** |  |  | $ | *** |
Site Restoration |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | as per Drawings |  | Supply and Install shed as shown including all footings, etc., inluding all permits |  | square meters |  |  | 9 |  |  | $ | *** |  |  | $ | *** |
2 |  | as per Drawings |  | Supply and install Wooden Deck (Rear) as shown including all permits |  | square meters |  |  | 10 |  |  | $ | *** |  |  | $ | *** |
3 |  | as per Drawings |  | Supply and install Wooden Deck (Other) as shown including all permits |  | square meters |  |  | 5 |  |  | $ | *** |  |  | $ | *** |
4 |  | as per Drawings |  | Supply and Place Retaining Wall as per specifications |  | Linear meters |  |  | 13 |  |  | $ | *** |  |  | $ | *** |
5 |  | as per Drawings |  | Supply and Place concrete stairs as per specifications |  | treads |  |  | 9 |  |  | $ | *** |  |  | $ | *** |
6 |  | 31 32 50 |  | Water management, sampling, transportation, and disposal at LTMWF |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
7 |  | 32 90 00 |  | Landscape Restoration |  | Allowance |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
Total Price - 34 Smith | $ | *** |

Group I Requirements - 36 Smith Street

Removals |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 02 61 00 |  | Pre-construction Property Condition Assessment |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
2 |  | 02 61 00 |  | Complete gamma survey and XRF scan of completed excavation surface |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 90 | Schedule 2

PROTECTED SENSITIVE

3 |  | 02 61 00 |  | Collection of soil sample for signature COPCs and the reporting of results following Laboratory Analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
4 |  | 02 61 00 |  | Laboratory analysis of soil sample for signature COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
5 |  | 02 61 00 |  | Collection of soil sample for secondary COPCs and the reporting of results following laboratory analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
6 |  | 02 61 00 |  | Laboratory analysis of composite soil sample for secondary COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
7 |  | 02 61 00 |  | Preparation and submission of Verification Documentation |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
8 |  | 02 41 16 |  | Demolish Existing Site Structures that require removal, verify not radiologically impacted and dispose off site a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
9 |  | 02 41 13 |  | Concrete Sidewalk Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 8 |  |  | $ | *** |  |  | $ | *** |
10 |  | 02 41 13 |  | Gravel Driveway Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 12 |  |  | $ | *** |  |  | $ | *** |
11 |  | 02 41 13 |  | Remove existing fence, verify not radiologically impacted and dispose offiste at licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
12 |  | 02 41 13 |  | Paving Stone / Interlocking Brick Patio Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 3 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 91 | Schedule 2

PROTECTED SENSITIVE

13 |  | 31 11 00 |  | Remove and Dispose of Trees, shrubs, hedges, and all other plants above ground, verify not radiological impacted and dispose offsite at a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
14 |  | 02 61 00 |  | Remove all other surface landscape features, relocate off-site to secure location for future re-installment |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
15 |  | 02 61 00 |  | Excavate, stockpile, load, haul and dispose at LTWMF Facility Contaminated soil and tree roots |  | cubic meters |  |  | 330 |  |  | $ | *** |  |  | $ | *** |
16 |  |  |  | Secondary Excavation (if requried) |  | cubic meters |  |  |  |  |  | $ | *** |  |  |  |  |
Earthworks |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 31 00 01 |  | Supply, place, compact and grade clean imported fill per MPH SOP/SOGs (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 420 |  |  | $ | *** |  |  | $ | *** |
2 |  | 31 00 01 |  | Supply, place, compact and grade Granular A (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 40 |  |  | $ | *** |  |  | $ | *** |
3 |  | 31 00 01 |  | Supply, place, compact and grade Granular B (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 40 |  |  | $ | *** |  |  | $ | *** |
4 |  | 31 00 01 |  | Supply, place, and grade Topsoil |  | cubic meters |  |  | 80 |  |  | $ | *** |  |  | $ | *** |
Site Restoration |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | as per Drawings |  | Supply and Install shed as shown including all footings, etc., inluding all permits |  | square meters |  |  | 4 |  |  | $ | *** |  |  | $ | *** |
2 |  | as per Drawings |  | Supply and Install covered porch as shown including all footings, etc., inluding all permits |  | square meters |  |  | 3 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 92 | Schedule 2

PROTECTED SENSITIVE

3 |  | as per Drawings |  | Supply and Place Gravel Drivway as per specifications |  | square meters |  |  | 12 |  |  | $ | *** |  |  | $ | *** |
4 |  | as per Drawings |  | Supply and Place Concrete Sidewalk as per specifications |  | square meters |  |  | 8 |  |  | $ | *** |  |  | $ | *** |
5 |  | as per Drawings |  | Supply and Place Paving Stone / Interlocking Brick Patio as per specifications |  | square meters |  |  | 3 |  |  | $ | *** |  |  | $ | *** |
6 |  | as per Drawings |  | Supply and Place concrete stairs as per specifications |  | treads |  |  | 6 |  |  | $ | *** |  |  | $ | *** |
7 |  | 32 90 00 |  | Landscape Restoration |  | Allowance |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
8 |  | 31 32 50 |  | Water management, sampling, transportation, and disposal at LTMWF |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
9 |  | as per Drawings |  | Supply and Place Fence |  | Linear meters |  |  | 29.00 |  |  | $ | *** |  |  | $ | *** |
Total Price - 36 Smith | $ | *** |

Group I Requirements - 38 Smith Street

Removals |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 02 61 00 |  | Pre-construction Property Condition Assessment |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
2 |  | 02 61 00 |  | Complete gamma survey and XRF scan of completed excavation surface |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
3 |  | 02 61 00 |  | Collection of soil sample for signature COPCs and the reporting of results following Laboratory Analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
4 |  | 02 61 00 |  | Laboratory analysis of soil sample for signature COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 93 | Schedule 2

PROTECTED SENSITIVE

5 |  | 02 61 00 |  | Collection of soil sample for secondary COPCs and the reporting of results following laboratory analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
6 |  | 02 61 00 |  | Laboratory analysis of composite soil sample for secondary COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
7 |  | 02 61 00 |  | Preparation and submission of Verification Documentation |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
8 |  | 02 41 16 |  | Demolish Existing Site Structures that require removal, verify not radiologically impacted and dispose off site a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
9 |  | 02 41 13 |  | Gravel Driveway Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 12 |  |  | $ | *** |  |  | $ | *** |
10 |  | 02 41 13 |  | Concrete Sidewalk Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 2 |  |  | $ | *** |  |  | $ | *** |
11 |  | 02 41 13 |  | Paving Stone / Interlocking Brick Sidewalk Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 20 |  |  | $ | *** |  |  | $ | *** |
12 |  | 02 41 13 |  | Paving Stone / Interlocking Brick Patio Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 11 |  |  | $ | *** |  |  | $ | *** |
13 |  | 02 41 13 |  | Concrete Stair Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 94 | Schedule 2

PROTECTED SENSITIVE

14 |  | 02 41 13 |  | Remove existing fence, verify not radiologically impacted and dispose offiste at licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
15 |  | 31 11 00 |  | Remove and Dispose of Trees, shrubs, hedges, and all other plants above ground, verify not radiological impacted and dispose offsite at a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
16 |  |  |  | Remove all other surface landscape features, relocate offsite to secure location for future re-installment |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
17 |  |  |  | Removal of Outbuilding Contents, storage in secured area, and return of objects upon restoration |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
18 |  | 02 61 00 |  | Excavate, stockpile, load, haul and dispose at LTWMF Facility Contaminated soil and tree roots |  | cubic meters |  |  | 90 |  |  | $ | *** |  |  | $ | *** |
19 |  |  |  | Secondary Excavation (if requried) |  | cubic meters |  |  |  |  |  | $ | *** |  |  |  |  |

Earthworks |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 31 00 01 |  | Supply, place, compact and grade clean imported fill per MPH SOP/SOGs (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 60 |  |  | $ | *** |  |  | $ | *** |
2 |  | 31 00 01 |  | Supply, place, compact and grade Granular A (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 20 |  |  | $ | *** |  |  | $ | *** |
3 |  | 31 00 01 |  | Supply, place, compact and grade Granular B (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 20 |  |  | $ | *** |  |  | $ | *** |
4 |  | 31 00 01 |  | Supply, place, and grade Topsoil |  | cubic meters |  |  | 40 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 95 | Schedule 2

PROTECTED SENSITIVE

Site Restoration |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | as per Drawings |  | Supply and Install shed as shown including all footings, floors etc. |  | square meters |  |  | 5 |  |  | $ | *** |  |  | $ | *** |
2 |  | as per Drawings |  | Supply and Place Gravel Driveway as per specifications |  | square meters |  |  | 12 |  |  | $ | *** |  |  | $ | *** |
3 |  | as per Drawings |  | Supply and Place Concrete Sidewalk as per specifications |  | square meters |  |  | 2 |  |  | $ | *** |  |  | $ | *** |
4 |  | as per Drawings |  | Supply and Place Paving Stone / Interlocking Brick Sidewalk as per specifications |  | square meters |  |  | 20 |  |  | $ | *** |  |  | $ | *** |
5 |  | as per Drawings |  | Supply and Place Paving Stone / Interlocking Brick Patio as per specifications |  | square meters |  |  | 11 |  |  | $ | *** |  |  | $ | *** |
6 |  | as per Drawings |  | Supply and install Covered Porch (Front) as shown including all permits |  | square meters |  |  | 3 |  |  | $ | *** |  |  | $ | *** |
7 |  | as per Drawings |  | Supply and install Wooden Deck (other) as shown including all permits |  | square meters |  |  | 4 |  |  | $ | *** |  |  | $ | *** |
8 |  | as per Drawings |  | Supply and Place concrete stairs as per specifications |  | treads |  |  | 6 |  |  | $ | *** |  |  | $ | *** |
9 |  | 32 90 00 |  | Landscape Restoration |  | Allowance |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
10 |  | 31 32 50 |  | Water management, sampling, transportation, and disposal at LTMWF |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
11 |  | as per Drawings |  | Supply and Place Fence |  | Linear meters |  |  | 4.00 |  |  | $ | *** |  |  | $ | *** |
Total Price - 38 Smith | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 96 | Schedule 2

PROTECTED SENSITIVE

Group I Requirements - 40 Smith Street |  |  |  |

Removals |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 02 61 00 |  | Pre-construction Property Condition Assessment |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
2 |  | 02 61 00 |  | Complete gamma survey and XRF scan of completed excavation surface |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
3 |  | 02 61 00 |  | Collection of soil sample for signature COPCs and the reporting of results following Laboratory Analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
4 |  | 02 61 00 |  | Laboratory analysis of soil sample for signature COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
5 |  | 02 61 00 |  | Collection of soil sample for secondary COPCs and the reporting of results following laboratory analysis |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
6 |  | 02 61 00 |  | Laboratory analysis of composite soil sample for secondary COPCs |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
7 |  | 02 61 00 |  | Preparation and submission of Verification Documentation |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
8 |  | 02 41 16 |  | Demolish existing Site structures that require removal, verify not radiologically impacted and dispose off site a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
9 |  | 02 41 13 |  | Gravel Driveway Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 9 |  |  | $ | *** |  |  | $ | *** |
10 |  | 02 41 13 |  | Paving stone / interlocking brick sidewalk removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 13 |  |  | $ | *** |  |  | $ | *** |
11 |  | 02 41 13 |  | Paving stone / interlocking brick patio Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | sq.meters |  |  | 12 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 97 | Schedule 2

PROTECTED SENSITIVE

12 |  | 02 41 13 |  | Concrete Stair Removal - verify not radiological impacted and dispose offsite at a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
13 |  | 02 41 13 |  | Remove existing fence, verify not radiologically impacted and dispose offiste at licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
14 |  | 31 11 00 |  | Remove and Dispose of Trees, shrubs, hedges, and all other plants above ground, verify not radiological impacted and dispose offsite at a licensed receiving facility |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
15 |  |  |  | Remove all other surface landscape features, relocate offsite to secure location for future re-installment |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
16 |  |  |  | Removal of Outbuilding Contents, storage in secured area, and return of objects upon restoration |  | Lump Sum |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
17 |  | 02 61 00 |  | Excavate, stockpile, load, haul and dispose at LTWMF Facility Contaminated soil and tree roots |  | cubic meters |  |  | 440 |  |  | $ | *** |  |  | $ | *** |
18 |  |  |  | Secondary Excavation (if requried) |  | cubic meters |  |  |  |  |  | $ | *** |  |  |  |  |
Earthworks |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | 31 00 01 |  | Supply, place, compact and grade clean imported fill per MPH SOP/SOGs (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 600 |  |  | $ | *** |  |  | $ | *** |
2 |  | 31 00 01 |  | Supply, place, compact and grade Granular A (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 80 |  |  | $ | *** |  |  | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 98 | Schedule 2

PROTECTED SENSITIVE

3 |  | 31 00 01 |  | Supply, place, compact and grade Granular B (based on 2 tonnes per cubic meter) |  | tonnes |  |  | 80 |  |  | $ | *** |  |  | $ | *** |
4 |  | 31 00 01 |  | Supply, place, and grade Topsoil |  | cubic meters |  |  | 60 |  |  | $ | *** |  |  | $ | *** |
Site Restoration |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
1 |  | as per Drawings |  | Supply and Install shed as shown including all footings, floors etc. |  | square meters |  |  | 6 |  |  | $ | *** |  |  | $ | *** |
2 |  | as per Drawings |  | Supply, Place, Gravel Driveway as per specifications |  | square meters |  |  | 9 |  |  | $ | *** |  |  | $ | *** |
3 |  | as per Drawings |  | Supply and Place Paving stone / interlocking brick sidewalk as per specifications |  | square meters |  |  | 13 |  |  | $ | *** |  |  | $ | *** |
4 |  | as per Drawings |  | Supply and Place Paving stone / interlocking brick patio as per specifications |  | square meters |  |  | 12 |  |  | $ | *** |  |  | $ | *** |
5 |  | as per Drawings |  | Supply, Place Covered Porch (Front) as shown including all permits |  | square meters |  |  | 10 |  |  | $ | *** |  |  | $ | *** |
6 |  | 06 15 00 |  | Supply, Place Wooden deck (other) as shown including all permits |  | square meters |  |  | 11 |  |  | $ | *** |  |  | $ | *** |
7 |  | as per Drawings |  | Supply and Place concrete stairs as per specifications |  | treads |  |  | 7 |  |  | $ | *** |  |  | $ | *** |
8 |  | as per Drawings |  | Supply and Place Fence |  | Linear meters |  |  | 51 |  |  | $ | *** |  |  | $ | *** |
9 |  | 31 32 50 |  | Water management, sampling, transportation, and disposal at LTMWF |  | Lump Sum |  |  | 1.00 |  |  | $ | *** |  |  | $ | *** |
10 |  | 32 90 00 |  | Landscape Restoration |  | Allowance |  |  | 1 |  |  | $ | *** |  |  | $ | *** |
Total Price - 40 Smith | $ | *** |
Total Remediation, Earthworks and Restoration Only | $ | *** |

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 99 | Schedule 2

PROTECTED SENSITIVE

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 100 | Schedule 2

PROTECTED SENSITIVE

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 101 | Schedule 2

PROTECTED SENSITIVE

***INDICATES CERTAIN INFORMATION IN THIS DOCUMENT WHICH HAS BEEN OMITTED FROM THIS PUBLIC FILING BECAUSE IT IS NOT MATERIAL AND WOULD LIKELY CAUSE COMPETITIVE HARM TO THE COMPANY IF PUBLICLY DISCLOSED.

CNL Task Order No. 541369 | 102 | Schedule 2

PROTECTED SENSITIVE

SCHEDULE 3 – WORK SCHEDULE

CNL Task Order No. XX | 1 | Schedule 3

PROTECTED SENSITIVE

The Work under this Task Order shall be performed in accordance with the following schedule:

Key Work Milestone |  | Date; On or Before
File the “Notice of Projects (per group)” |  | April 10, 2019
Mobilization |  | May 09, 2019
Field Work Starts |  | May 14, 2019
Completion of General Requirements |  | May 07, 2019
Completion of Group B |  | June 20, 2019
Completion of Group C |  | October 28, 2019
Completion of Group G |  | July 24, 2019
Completion of Group H |  | October 01, 2019
Completion of Group I |  | June 19, 2019
Project Completion |  | December 16, 2019

Milestone schedule date for Completion of SSS Remediation Package 3 will be used as the basis for any Delay Liquidated Damages payable to CNL under GC 7.1.2 of the Framework Agreement. Proponent to provide a Schedule Recovery Plan should the Proponent’s Schedule be delayed more than 10% of the critical path

CNL Task Order No. XX | 2 | Schedule 3

PROTECTED SENSITIVE

SCHEDULE 4 – SPECIAL CONDITIONS

CONTRACTOR’S METHODOLOGY

Refer to Perma-Fix Canada Inc. Framework Agreement 507595 – Exhibit B Schedule or Rates.

CNL Task Order No. XX | 1 | Schedule 4

PROTECTED SENSITIVE

SCHEDULE 5 – SUBCONTRACTORS

CNL Task Order No. 541369 | 1 | Schedule 5

PROTECTED SENSITIVE

SCHEDULE 6 – FIELD EQUIPMENT LIST

CNL Task Order No. 541369 | 1 | Schedule 6

PROTECTED SENSITIVE

FIELD EQUIPMENT LIST

Refer to Schedule 2, Price Schedule, for. Equipment Rates.

CNL Task Order No. 541369 | 2 | Schedule 6

PROTECTED SENSITIVE

SCHEDULE 7 – Aboriginal and/or Local, Small and Medium-sized Business Engagement Plan

Perma-Fix Canada Inc. (Perma-Fix) (Prime), has sourced preferred contractors and sub-contractors that are either Aboriginal-owned or have extensive practical experience with creating employment opportunities for local Aboriginal Status Peoples or Nations that are in proximity to a project or qualify in regards to experience and other qualification requirements. Perma-Fix intends to offer targeted training and mentoring opportunities to Status individuals in order to meet or exceed our targets. Perma-Fix is dedicated to a sustainable inclusion program that will have long-term benefits to the community and Aboriginal Peoples.

As stated in our proposal response to the Master Service Agreement (MSA)/Framework Agreement procurement, Section T8, Perma-Fix’s focus is to achieve a minimum 5% Aboriginal status employment during the implementation of task orders.

CNL Task Order No. 541369 | 1 | Schedule 7

PROTECTED SENSITIVE

SCHEDULE 8 – CONTRACTOR’S STAKEHOLDER ENGAGEMENT

The remediation and transportation of radioactively impacted soils and structures in a public/residential setting provides a unique challenge to Canadian Nuclear Laboratories (CNL) and the contractor performing the work. Radioactive material remediation is usually performed on government licensed sites with layers of security and controls in place. Performing these same tasks in a residential setting requires infrastructure to be developed that is certain to gain the attention of property owners, neighbors, the Municipality of Port Hope, and members of CNL. Through the process of remediation followed by transportation from the residential properties through the municipality to the designated low-level radioactive waste (LLRW) landfill, the attention from community stakeholders will only increase.

Our project CHP, Mr. Andy Lombardo, is a very experienced public speaker and is a subject matter expert in the safe handling and monitoring of uranium, thorium, and radium. He will work hand-in-hand with our Primary Point of Contact for the project, Ms. Lori Brooks and our Project Administration, Ms. Laura Kelly, to develop and implement our project Communications Plan/Strategy. Both are well schooled in public interaction and will be available daily.

Our team is sensitive to homeowner issues, and we will collaborate closely with CNL, members of the community, and other Port Hope Area Initiative (PHAI) stakeholders to minimize inconvenience that may result from our work. Our approach will convey the utmost respect to the residents and their concerns. The following are key components of the Communication protocols for this project:

● | Work with CNL/PHAI to ensure appropriate notification format/distribution methods are in place (e.g., health and safety incident, stakeholder/public relations incident);
● | Provide early training and ongoing coaching to workers on interaction with property owners, tenants, etc.;
● | Use a risk log as a means to track and proactively manage issues throughout the project because this is key to achieving and maintaining excellent community support;
● | Develop processes to receive, record, respond to, and follow-up on community questions or complaints, regardless of the medium (e-mail, project website, telephone, in-person visit);
● | Direct public inquiries to a single point of contact, and provide prompt and courteous responses by a knowledgeable team member;
● | Communicate frequently with the team for safety messages, public issues and concerns, and noteworthy items like lessons learned; and
● | Provide consistent messaging using CNL/PHAI’s key messages, questions, answers, and other scripted material.

CNL Task Order No. 541369 | 1 | Schedule 8