EX-99.1 11 ex99120211231.htm OPINION OF EXPERTS
EXHIBIT 99.1
DeGolyer and MacNaughton
5001 Spring Valley Road
Suite 800 East
Dallas, Texas 75244
January 27, 2022
EOG Resources, Inc.
1111 Bagby Street, Sky Lobby 2
Houston, Texas 77002
Ladies and Gentlemen:
Pursuant to your request, this report of third party presents an independent evaluation, as of December 31, 2021, of the estimated net proved oil, condensate, natural gas liquids (NGL), and gas reserves of certain properties in which EOG Resources, Inc. (EOG) has represented it holds an interest. This evaluation was completed on January 27, 2022. The properties evaluated consist of working and royalty interests located in the States of New Mexico and Texas and offshore from Trinidad. EOG has represented that these properties account for 78.2 percent on a net equivalent barrel basis of EOG’s net proved reserves as of December 31, 2021, and that the net proved reserves estimates have been prepared in accordance with the reserves definitions of Rules 4–10(a) (1)–(32) of Regulation S–X of the United States Securities and Exchange Commission (SEC). It is our opinion that the procedures and methodologies employed by EOG for the preparation of its proved reserves estimates as of December 31, 2021, comply with the current requirements of the SEC. We have reviewed information provided by EOG that it represents to be EOG’s estimates of the net reserves, as of December 31, 2021, for the same properties as those which we evaluated. This report was prepared in accordance with guidelines specified in Item 1202 (a)(8) of Regulation S–K and is to be used for inclusion in certain SEC filings by EOG.
Reserves estimates included herein are expressed as net reserves as represented by EOG. Gross reserves are defined as the total estimated petroleum remaining to be produced from these properties after December 31, 2021. Net reserves are defined as that portion of the gross reserves attributable to the interests held by EOG after deducting all interests held by others.
Estimates of reserves should be regarded only as estimates that may change as further production history and additional information become available. Not only

2
DeGolyer and MacNaughton
are such estimates based on that information which is currently available, but such estimates are also subject to the uncertainties inherent in the application of judgmental factors in interpreting such information.
Information used in the preparation of this report was obtained from EOG and from public sources. Additionally, this information includes data supplied by HIS Markit Inc; Copyright 2021 IHS Markit Inc. In the preparation of this report we have relied, without independent verification, upon information furnished by EOG with respect to the property interests being evaluated, production from such properties, current costs of operation and development, current prices for production, agreements relating to current and future operations and sale of production, and various other information and data that were accepted as represented. A field examination was not considered necessary for the purposes of this report.
Definition of Reserves
Petroleum reserves included in this report are classified as proved. Only proved reserves have been evaluated for this report. Reserves classifications used in this report are in accordance with the reserves definitions of Rules 4–10(a) (1)–(32) of Regulation S–X of the SEC. Reserves are judged to be economically producible in future years from known reservoirs under existing economic and operating conditions and assuming continuation of current regulatory practices using conventional production methods and equipment. In the analyses of production-decline curves, reserves were estimated only to the limit of economic rates of production under existing economic and operating conditions using prices and costs consistent with the effective date of this report, including consideration of changes in existing prices provided only by contractual arrangements but not including escalations based upon future conditions. The petroleum reserves are classified as follows:
Proved oil and gas reserves – Proved oil and gas reserves are those quantities of oil and gas, which, by analysis of geoscience and engineering data, can be estimated with reasonable certainty to be economically producible—from a given date forward, from known reservoirs, and under existing economic conditions, operating methods, and government regulations—prior to the time at which contracts providing the right to operate expire, unless evidence indicates that renewal is reasonably certain, regardless of whether deterministic or probabilistic methods are used for the estimation. The project to extract the hydrocarbons must have commenced or the operator must be reasonably certain that it will commence the project within a reasonable time.

3
DeGolyer and MacNaughton
(i) The area of the reservoir considered as proved includes:
(A) The area identified by drilling and limited by fluid contacts, if any, and (B) Adjacent undrilled portions of the reservoir that can, with reasonable certainty, be judged to be continuous with it and to contain economically producible oil or gas on the basis of available geoscience and engineering data.
(ii) In the absence of data on fluid contacts, proved quantities in a reservoir are limited by the lowest known hydrocarbons (LKH) as seen in a well penetration unless geoscience, engineering, or performance data and reliable technology establishes a lower contact with reasonable certainty.
(iii) Where direct observation from well penetrations has defined a highest known oil (HKO) elevation and the potential exists for an associated gas cap, proved oil reserves may be assigned in the structurally higher portions of the reservoir only if geoscience, engineering, or performance data and reliable technology establish the higher contact with reasonable certainty.
(iv) Reserves which can be produced economically through application of improved recovery techniques (including, but not limited to, fluid injection) are included in the proved classification when:
(A) Successful testing by a pilot project in an area of the reservoir with properties no more favorable than in the reservoir as a whole, the operation of an installed program in the reservoir or an analogous reservoir, or other evidence using reliable technology establishes the reasonable certainty of the engineering analysis on which the project or program was based; and (B) The project has been approved for development by all necessary parties and entities, including governmental entities.
(v) Existing economic conditions include prices and costs at which economic producibility from a reservoir is to be determined. The price shall be the average price during the 12-month period prior to the ending date of the period covered by the report, determined as an unweighted arithmetic average of the first-day-of-the-month price for each month within such period, unless prices are defined by

4
DeGolyer and MacNaughton
contractual arrangements, excluding escalations based upon future conditions.
Developed oil and gas reserves – Developed oil and gas reserves are reserves of any category that can be expected to be recovered:
(i) Through existing wells with existing equipment and operating methods or in which the cost of the required equipment is relatively minor compared to the cost of a new well; and
(ii) Through installed extraction equipment and infrastructure operational at the time of the reserves estimate if the extraction is by means not involving a well.
Undeveloped oil and gas reserves – Undeveloped oil and gas reserves are reserves of any category that are expected to be recovered from new wells on undrilled acreage, or from existing wells where a relatively major expenditure is required for recompletion.
(i) Reserves on undrilled acreage shall be limited to those directly offsetting development spacing areas that are reasonably certain of production when drilled, unless evidence using reliable technology exists that establishes reasonable certainty of economic producibility at greater distances.
(ii) Undrilled locations can be classified as having undeveloped reserves only if a development plan has been adopted indicating that they are scheduled to be drilled within five years, unless the specific circumstances justify a longer time.
(iii) Under no circumstances shall estimates for undeveloped reserves be attributable to any acreage for which an application of fluid injection or other improved recovery technique is contemplated, unless such techniques have been proved effective by actual projects in the same reservoir or an analogous reservoir, as defined in [section 210.4–10 (a) Definitions], or by other evidence using reliable technology establishing reasonable certainty.

5
DeGolyer and MacNaughton
Methodology and Procedures
Estimates of reserves were prepared by the use of appropriate geologic, petroleum engineering, and evaluation principles and techniques that are in accordance with the reserves definitions of Rules 4–10(a) (1)–(32) of Regulation S–X of the SEC and with practices generally recognized by the petroleum industry as presented in the publication of the Society of Petroleum Engineers entitled “Standards Pertaining to the Estimating and Auditing of Oil and Gas Reserves Information (revised June 2019) Approved by the SPE Board on 25 June 2019” and, for properties in the United States, in Monograph 3 and Monograph 4 published by the Society of Petroleum Evaluation Engineers. The method or combination of methods used in the analysis of each reservoir was tempered by experience with similar reservoirs, stage of development, quality and completeness of basic data, and production history.
Based on the current stage of field development, production performance, the development plans provided by EOG, and analyses of areas offsetting existing wells with test or production data, reserves were classified as proved.
The proved undeveloped reserves estimates were based on opportunities in the plan of development provided by EOG.
EOG has represented that its senior management is committed to the development plan provided by EOG and that EOG has the financial capability to execute the development plan, including the drilling and completion of wells and the installation of equipment and facilities.
For the evaluation of unconventional reservoirs, a performance-based methodology integrating the appropriate geology and petroleum engineering data was utilized for this report. Performance-based methodology primarily includes (1) production diagnostics, (2) decline-curve analysis, and (3) model-based analysis (if necessary, based on availability of data). Production diagnostics include data quality control, identification of flow regimes, and characteristic well performance behavior. These analyses were performed for all well groupings (or type-curve areas).
Characteristic rate-decline profiles from diagnostic interpretation were translated to modified hyperbolic rate profiles, including one or multiple b-exponent values followed by an exponential decline. Based on the availability of data, model-based analysis may be integrated to evaluate long-term decline behavior, the effect of dynamic reservoir and fracture parameters on well performance, and complex situations sourced by the nature of unconventional reservoirs.

6
DeGolyer and MacNaughton
For properties offshore from Trinidad, when applicable, the volumetric method was used to estimate the original gas in place (OGIP). Structure maps were prepared to delineate selected reservoirs, and isopach maps were constructed to estimate reservoir volume. Electrical logs, radioactivity logs, core analyses and other available data were used to prepare these maps as well as to estimate representative values for porosity and water saturation. When adequate data were available and when circumstances justified, material-balance methods were used to estimate OGIP.
Estimates of ultimate recovery were obtained after applying recovery factors to OGIP. These recovery factors were based on consideration of the type of energy inherent in the reservoirs, analyses of the petroleum, the structural positions of the properties, and the production histories. When applicable, material-balance and other engineering methods were used to estimate recovery factors based on an analysis of reservoir performance, including production rate, reservoir pressure, and reservoir fluid properties.
For properties offshore from Trinidad, reserves for depletion-type reservoirs or those whose performance disclosed a reliable decline in producing-rate trends or other diagnostic characteristics, were estimated by the application of appropriate decline curves or other performance relationships. In the analyses of production-decline curves, reserves were estimated only to the limits of economic production as defined under the Definition of Reserves heading of this report, contract expiration, or technical well abandonment rate, whichever occurs first.
In the evaluation of undeveloped reserves, type-well analysis was performed using well data from analogous reservoirs for which more complete historical performance data were available.
Data provided by EOG from wells drilled through December 31, 2021, and made available for this evaluation were used to prepare the reserves estimates herein. The reserves estimates for the properties offshore from Trinidad were based on consideration of monthly production data available only through September 2021. The reserves estimates for the properties in the States of New Mexico and Texas were based on consideration of daily and monthly production data through December 2021. Estimated cumulative production, as of December 31, 2021, was deducted from the estimated gross ultimate recovery to estimate gross reserves. This required that production be estimated for up to 3 months for the properties offshore from Trinidad.
Oil and condensate reserves estimated herein are those to be recovered by normal field separation. NGL reserves estimated herein include pentanes and heavier fractions (C 5+)

7
DeGolyer and MacNaughton
and liquefied petroleum gas (LPG), which consists primarily of propane and butane fractions, and are the result of low-temperature plant processing. Oil, condensate, and NGL reserves included in this report are expressed in thousands of barrels (Mbbl). In these estimates, 1 barrel equals 42 United States gallons. For reporting purposes, oil and condensate reserves have been estimated separately and are presented herein as a summed quantity.
Gas quantities estimated herein are expressed as sales gas. Sales gas is defined as the total gas to be produced from the reservoirs, measured at the point of delivery, after reduction for fuel usage, flare, and shrinkage resulting from field separation and processing. Gas reserves estimated herein are reported as sales gas. Gas quantities are expressed at a temperature base of 60 degrees Fahrenheit (°F) and at the pressure base of the state or area in which the quantities are located. Gas quantities included in this report are expressed in millions of cubic feet (MMcf).
Gas quantities are identified by the type of reservoir from which the gas will be produced. Nonassociated gas is gas at initial reservoir conditions with no oil present in the reservoir. Associated gas is both gas-cap gas and solution gas. Gas-cap gas is gas at initial reservoir conditions and is in communication with an underlying oil zone. Solution gas is gas dissolved in oil at initial reservoir conditions. Gas quantities estimated herein include both associated and nonassociated gas.
At the request of EOG, sales gas reserves estimated herein were converted to oil equivalent using an energy equivalent factor of 6,000 cubic feet of gas per 1 barrel of oil equivalent.
Primary Economic Assumptions
This report has been prepared using initial prices, expenses, and costs provided by EOG. Future prices were estimated using guidelines established by the SEC and the Financial Accounting Standards Board (FASB). The following economic assumptions were used for estimating the reserves reported herein:
Oil, Condensate, and NGL Prices
EOG has represented that the oil, condensate, and NGL prices were based on a reference price, calculated as the unweighted arithmetic average of the first-day-of-the-month price for each month within the 12-month period prior to the end of the reporting period, unless

8
DeGolyer and MacNaughton
prices are defined by contractual agreements. EOG supplied differentials to a West Texas Intermediate (WTI) reference price of $66.56 per barrel and the prices were held constant thereafter. The volume-weighted average prices attributable to the estimated proved reserves over the lives of the properties were $68.01 per barrel of oil and condensate and $30.45 per barrel of NGL.
Gas Prices
EOG has represented that the gas prices were based on a reference price, calculated as the unweighted arithmetic average of the first-day-of-the-month price for each month within the 12-month period prior to the end of the reporting period, unless prices are defined by contractual agreements. EOG supplied differentials to a Henry Hub reference price of $3.598 per million Btu ($/MMBtu) and the prices were held constant thereafter. Btu factors provided by EOG were used to convert prices from dollars per million Btu to dollars per thousand cubic feet of gas. The volume-weighted average price attributable to the estimated proved reserves over the lives of the properties was $4.308 per thousand cubic feet of gas.
Production and Ad Valorem Taxes
For properties in the United States, production taxes were calculated using the tax rates for each state in which the reserves are located including, where appropriate, abatements for enhanced recovery programs, and ad valorem taxes were estimated using rates provided by EOG based on recent payments.
Operating Expenses, Capital Costs, and Abandonment Costs
Estimates of operating expenses, provided by EOG and based on current expenses, were held constant for the lives of the properties. Future capital expenditures were estimated using 2021 values, provided by EOG, and were not adjusted for inflation. Abandonment costs, which are those costs associated with the removal of equipment, plugging of wells, and reclamation and restoration associated with the abandonment, were provided by EOG for all properties and were not adjusted for inflation. Operating expenses, capital costs, and abandonment costs were considered, as

9
DeGolyer and MacNaughton
appropriate, in determining the economic viability of undeveloped reserves estimated herein.
In our opinion, the information relating to estimated proved reserves of oil, condensate, NGL, and gas contained in this report has been prepared in accordance with Paragraphs 932-235-50-4, 932-235-50-6, 932-235-50-7, and 932-235-50-9 of the Accounting Standards Update 932-235-50, Extractive Industries – Oil and Gas (Topic 932): Oil and Gas Reserve Estimation and Disclosures (January 2010) of the FASB and Rules 4–10(a) (1)–(32) of Regulation S–X and Rules 302(b), 1201, 1202(a) (1), (2), (3), (4), (8), and 1203(a) of Regulation S–K of the SEC; provided, however, that estimates of proved developed and proved undeveloped reserves are not presented at the beginning of the year.
To the extent the above-enumerated rules, regulations, and statements require determinations of an accounting or legal nature, we, as engineers, are necessarily unable to express an opinion as to whether the above-described information is in accordance therewith or sufficient therefor.
Summary of Conclusions
EOG has represented that its estimated net proved reserves attributable to the properties evaluated herein were based on the definitions of proved reserves of the SEC. EOG’s estimates of the net proved reserves, as of December 31, 2021, attributable to these properties, which represent 78.2 percent of EOG’s total proved reserves on a net equivalent basis, are summarized as follows, expressed in thousands of barrels (Mbbl), millions of cubic feet (MMcf), and thousands of barrels of oil equivalent (Mboe):

| Estimated by EOG Net Proved Reserves as of December 31, 2021
Properties Evaluated by DeGolyer and MacNaughton |  | Oil and Condensate (Mbbl) |  | NGL (Mbbl) |  | Sales Gas (MMcf) |  | Oil Equivalent (Mboe)
Proved Developed |  | 673,074 |  | 276,898 |  | 2,308,589 |  | 1,334,737
Proved Undeveloped |  | 632,892 |  | 396,665 |  | 3,388,507 |  | 1,594,308
Total Proved |  | 1,305,966 |  | 673,563 |  | 5,697,096 |  | 2,929,045
Note: Sales gas reserves estimated herein were converted to oil equivalent using an energy equivalent factor of 6,000 cubic feet of gas per 1 barrel of oil equivalent.

10
DeGolyer and MacNaughton
DeGolyer and MacNaughton’s estimates of EOG’s net proved reserves, as of December 31, 2021, attributable to the properties evaluated herein were based on the definition of proved reserves of the SEC and are summarized as follows, expressed in thousands of barrels (Mbbl), millions of cubic feet (MMcf), and thousands of barrels of oil equivalent (Mboe):

| Estimated by DeGolyer and MacNaughton Net Proved Reserves as of December 31, 2021
Properties Evaluated by DeGolyer and MacNaughton |  | Oil and Condensate (Mbbl) |  | NGL (Mbbl) |  | Sales Gas (MMcf) |  | Oil Equivalent (Mboe)
Proved Developed |  | 669,244 |  | 268,112 |  | 2,225,579 |  | 1,308,287
Proved Undeveloped |  | 673,056 |  | 374,296 |  | 3,186,425 |  | 1,578,422
Total Proved |  | 1,342,300 |  | 642,408 |  | 5,412,004 |  | 2,886,709
Note: Sales gas reserves estimated herein were converted to oil equivalent using an energy equivalent factor of 6,000 cubic feet of gas per 1 barrel of oil equivalent.

11
DeGolyer and MacNaughton
In comparing the detailed net proved reserves estimates prepared by DeGolyer and MacNaughton and by EOG of the properties evaluated herein, differences have been found, both positive and negative, resulting in an aggregate difference of 1.4 percent when compared on the basis of net oil equivalent. It is DeGolyer and MacNaughton’s opinion that there is no material difference between the net proved reserves estimates prepared by EOG and those prepared by DeGolyer and MacNaughton for those properties DeGolyer and MacNaughton evaluated.
While the oil and gas industry may be subject to regulatory changes from time to time that could affect an industry participant’s ability to recover its reserves, we are not aware of any such governmental actions which would restrict the recovery of the December 31, 2021, estimated reserves.
DeGolyer and MacNaughton is an independent petroleum engineering consulting firm that has been providing petroleum consulting services throughout the world since 1936. DeGolyer and MacNaughton does not have any financial interest, including stock ownership, in EOG. Our fees were not contingent on the results of our evaluation. This report has been prepared at the request of EOG. DeGolyer and MacNaughton has used all data, assumptions, procedures, and methods that it considers necessary to prepare this report.
Submitted,
/s/ DeGolyer and MacNaughton
DeGOLYER and MacNAUGHTON
Texas Registered Engineering Firm F-716
____________________________
Dilhan Ilk, P.E.
Senior Vice President
DeGolyer and MacNaughton

DeGolyer and MacNaughton
CERTIFICATE of QUALIFICATION
I, Dilhan Ilk, Petroleum Engineer with DeGolyer and MacNaughton, 5001 Spring Valley Road, Suite 800 East, Dallas, Texas, 75244 U.S.A., hereby certify:
1.That I am a Senior Vice President with DeGolyer and MacNaughton, which firm did prepare the report of third party addressed to EOG dated
January 27, 2022, and that I, as Senior Vice President, was responsible for the preparation of this report of third party.
2.That I attended Istanbul Technical University, and that I graduated with a Bachelor of Science degree in Petroleum Engineering in the year 2003, a Master of Science degree from Texas A&M University in 2005, and a Doctor in Philosophy degree from Texas A&M University in 2010; that I am a Registered Professional Engineer in the State of Texas; that I am a member of the Society of Petroleum Engineers; and that I have in excess of 11 years of experience in oil and gas reservoir studies and reserves evaluations.
____________________________
Dilhan Ilk, P.E.
Senior Vice President
DeGolyer and MacNaughton