EX-99.1 2 a2015-07x06xmarigoldupdate.htm EXHIBIT 99.1

July 6, 2015 | News Release 15–11

SILVER STANDARD REPORTS EXPANDED MARIGOLD EXPLORATION PROGRAM
VANCOUVER, B.C. -- Silver Standard Resources Inc. (NASDAQ: SSRI) (TSX: SSO) (“Silver Standard”) provides an exploration update for recent Mineral Resource development activities at its Marigold mine (“Marigold“) in Nevada, U.S.
Highlights:

▪ | Mineral Resource development drilling at 8 South pit area extends higher-grade gold mineralization. Drillhole MR-6034 intersected 2.48 grams per tonne gold over 91.4 metres from 140.2 metres below surface, as previously reported.

▪ | Mineral Resource development drilling identified a new mineralized structure northwest of the 8 South pit. Drillhole MRA-6104 intersected 1.18 grams per tonne gold over 56.4 metres from 221.0 metres below surface.

▪ | Completed assay program of historical drillholes to increase Mineral Resources and Mineral Reserves estimates for the Mackay Phase 3 pit. Results are expected in the third quarter of 2015. The assay program for the remaining life of mine is ongoing and results will be reported in 2015 and 2016 as they become available.

“Exploration results are adding real value at Marigold beyond what we initially expected,” said John Smith, President and CEO. “With above reserve grade intercepts and a new gold structure to the northwest of the 8 South pit area, we continue to improve our understanding of the mineralization and increase opportunity for the future at Marigold.”
Assay Program
Marigold has a history of positive ore reconciliation. In order to investigate the cause of such results, we initiated an operational excellence program in January 2015. The program reanalyzed select samples from drillholes completed prior to 2008 that were assigned assay values of “zero” in the geological database and that are within the current mine plan. The program is intended to improve our Mineral Resources model to incorporate results from samples that, at the time, were below the historical cut-off grade of the analytical method used. Initial results indicate that there are numerous historical drill intercepts with gold values above the current 0.065 grams per tonne payable gold cut-off grade when assayed with a current analytical method. With the reanalysis incorporated into our Mineral Resources model, it is expected that areas currently classified as waste can be converted to ore, thereby increasing Mineral Resources and Mineral Reserves estimates for Marigold.
Page 1

In the first half of 2015, 34,926 drill samples were sent to American Assays Laboratories in Sparks, Nevada, which is independent from Silver Standard, for assaying and 21,436 results have been received in relation to the Mackay Phase 3 area as of June 30, 2015. We are continuing with the assay program with an additional 65,000 historic drill samples to be assayed during the second half of 2015 for a total of 99,926 drill samples within areas planned to be mined over the next four years. This assay program is expected to be completed by the end of 2016 with a further 90,000 samples assayed, which will cover the remaining production years through the planned Marigold life of mine.
Mineral Resource Development Drilling
The 2015 Mineral Resources development program for Marigold is targeting the discovery and development of gold mineralization proximal to the open pits, following a successful drilling campaign in the fourth quarter of 2014. The primary objective of the program is to upgrade Inferred Mineral Resources to Indicated Mineral Resources and to convert Mineral Resources to Mineral Reserves. As of June 30, 2015 a total of 113 reverse circulation and sonic drillholes have been completed, for a total of 26,066 metres. Approximately 95% of the drillholes, for which assay results have been received, intercepted gold mineralization exceeding the Mineral Resources cut-off grade of 0.065 grams per tonne payable gold and thickness criteria.
Mineralization within the 8 South pit extension area (8SX), previously reported, continues to expand with additional drilling. Another zone of higher grade mineralization has also been delineated to the northwest of 8SX, known as the 8D area. Refer to Figure 1 for the location of all drill collars. Selected results from 13 drillholes with higher-grade gold intercepts are included in Table 1 and labeled in Figure 1. A complete list of the drill assay results received in the first half of 2015 for the Marigold exploration drill program is included in Table 2.
We expect to complete the drill program and modeling of the 8SX mineralization through the second half of 2015. The drilling program is expected to be comprised of an additional 9,100 metres of drilling in 35 reverse circulation holes and 3,800 metres of sonic drilling of rock stockpiles.
Furthermore, drilling continues on the deep sulphide exploration program with two additional core holes planned for the second half of 2015 to test permissive rock units discovered in the initial phase of drilling for sulphide and carbonate-hosted, high-grade gold mineralization.
Page 2

Figure 1. Drillhole Location Plan Map for exploration drill program at the 8 South pit extension area (8SX) and the 8D area at the Marigold mine, Nevada, U.S.
Note: Sonic drilling refers to holes drilled by rotating and vibrating the rod, core barrel and casing at resonant frequencies.
Page 3

Table 1. Selected drillhole highlights from the Marigold Exploration Drill Program.

Hole ID | From (metres) | To (metres) | Width (metres) | Gold Grade (g/tonne) | Deposit Area
MRA6034 | 140.2 | 231.6 | 91.4 | 2.48 | 8SX
Including | 178.3 | 214.9 | 36.6 | 5.86 | 8SX
MR6042 | 210.3 | 259.1 | 48.8 | 1.17 | 8D
Including | 222.5 | 234.7 | 12.2 | 3.03 | 8D
MR6045 | 202.7 | 367.3 | 164.6 | 1.67 | 8D
Including | 242.3 | 262.1 | 19.8 | 3.97 | 8D
Including | 323.1 | 341.4 | 18.3 | 3.86 | 8D
MRA6046 | 213.4 | 266.7 | 53.3 | 1.02 | 8D
Including | 224.0 | 240.8 | 16.8 | 2.11 | 8D
MRA6053 | 196.6 | 260.6 | 64.0 | 0.90 | 8SX
Including | 205.7 | 216.4 | 10.7 | 3.06 | 8SX
MRA6055 | 259.1 | 298.7 | 39.6 | 0.89 | 8SX
MRA6063 | 184.4 | 222.5 | 38.1 | 0.85 | 8SX
MRA6079 | 193.5 | 236.2 | 42.7 | 0.72 | 8D
MRA6080 | 208.8 | 262.1 | 53.3 | 0.78 | 8D
MRA6085 | 201.2 | 230.1 | 28.9 | 0.91 | 8SX
Including | 204.2 | 211.8 | 7.6 | 2.74 | 8SX
MRA6098 | 213.4 | 277.4 | 64.0 | 0.69 | 8D
Including | 257.6 | 266.7 | 9.1 | 2.25 | 8D
MR6103 | 164.6 | 216.4 | 51.8 | 0.91 | 8SX
Including | 181.4 | 192.0 | 10.6 | 3.08 | 8SX
MRA6104 | 221.0 | 277.4 | 56.4 | 1.18 | 8D

Notes: Selected results for down hole intercepts 25 grams x metres and higher. Width values refer to length of down hole intercept. Drillholes MRA-6034 and MR-6045 have been previously reported.
Next Steps
Based on the positive results from the exploration and development programs at Marigold, an additional $2.4 million dollars has been allocated for capitalized exploration, for a total of $4.2 million for full year 2015.
It is expected that these exploration and development program results will be included in an updated Mineral Resources estimate for Marigold in the fourth quarter of 2015 and reported in our annual 2015 Mineral Resources and Mineral Reserves statement to be published in the first quarter of 2016.
Qualified Persons
The scientific and technical data contained in this news release has been reviewed and approved by James N. Carver, SME Registered Member, and Karthik Rathnam, MAusIMM (CP), each of whom is a Qualified Person under National Instrument 43-101 — Standards of Disclosure for Mineral Projects (“NI 43-101”). Mr. Carver and Mr. Rathnam are employed at the Marigold mine as our Chief Geologist and Senior Resource Geologist, respectively.
Page 4

SOURCE: Silver Standard Resources Inc.
For further information contact:
W. John DeCooman, Jr.
Vice President, Business Development and Strategy
Silver Standard Resources Inc.
Vancouver, BC
N.A. toll-free: +1 (888) 338-0046
All others: +1 (604) 689-3846
E-Mail: invest@silverstandard.com
To receive Silver Standard’s news releases by e-mail, please register using the Silver Standard website at www.silverstandard.com.
Cautionary Note Regarding Forward-Looking Statements:
This news release contains forward-looking information within the meaning of Canadian securities laws and forward-looking statements within the meaning of the U.S. Private Securities Litigation Reform Act of 1995 (collectively, “forward-looking statements”) concerning the anticipated developments in our operations in future periods, and other events or conditions that may occur or exist in the future. All statements, other than statements of historical fact, are forward-looking statements.
Generally, forward-looking statements can be identified by the use of words or phrases such as “expects,” “anticipates,” “plans,” “projects,” “estimates,” “assumes,” “intends,” “strategy,” “goals,” “objectives,” “potential” or variations thereof, or stating that certain actions, events or results “may,” “could,” “would,” “might” or “will” be taken, occur or be achieved, or the negative of any of these terms or similar expressions. The forward-looking statements in this news release relate to, among other things: future production of silver, gold and other metals; future costs of inventory, and cash costs and total costs per payable ounce of silver, gold and other metals sold; the prices of silver, gold and other metals; the effects of laws, regulations and government policies affecting our operations or potential future operations; future successful development of our projects; the sufficiency of our current working capital, anticipated operating cash flow or our ability to raise necessary funds; estimated production rates for silver, gold and other metals produced by us; timing of production and the cash costs and total costs of production at the Pirquitas mine and the Marigold mine; the estimated cost of sustaining capital; ongoing or future development plans and capital replacement, improvement or remediation programs; the estimates of expected or anticipated economic returns from our mining projects, including future sales of metals, concentrate or other products produced by us; and our plans and expectations for our properties and operations.
These forward-looking statements are subject to a variety of known and unknown risks, uncertainties and other factors that could cause actual events or results to differ from those expressed or implied, including, without limitation, the following: uncertainty of production, development plans and cost estimates for the Pirquitas mine, the Marigold mine and our projects; our ability to replace Mineral Reserves; commodity price fluctuations; political or economic instability and unexpected regulatory changes; currency fluctuations, particularly the value of the Argentine peso against the U.S. dollar; the possibility of future losses; general economic conditions; fully realizing our interest in Pretium Resources Inc. (“Pretium”) and our other marketable securities, including the price of and market for Pretium’s common shares and such other marketable securities; potential export duty and related interest on current and past production of silver concentrate from the Pirquitas mine; recoverability and tightened controls over the VAT collection process in Argentina; counterparty and market risks related to the sale of our concentrate and metals; uncertainty in the accuracy of Mineral Reserves and Mineral Resources estimates and in our ability to extract mineralization profitably; differences in U.S. and Canadian practices for reporting Mineral Reserves and Mineral Resources; lack of suitable infrastructure or damage to existing infrastructure; future development risks, including start-up delays and operational issues; our ability to obtain adequate financing for further exploration and development programs; uncertainty in acquiring additional commercially mineable mineral rights; delays in obtaining or failure to obtain governmental permits, or non-compliance with permits we have obtained; our ability to attract and retain qualified personnel and management and potential labour unrest, including labour actions by our unionized employees at the Pirquitas mine; governmental laws and regulations, including health, safety and environmental laws and regulations, increased costs and restrictions
Page 5

on operations due to compliance with such regulations; reclamation and closure requirements for our mineral properties; unpredictable risks and hazards related to the development and operation of a mine or mineral property that are beyond our control; assessments by taxation authorities in multiple jurisdictions, including the recent reassessment by the Canada Revenue Agency; claims and legal proceedings, including adverse rulings in current or future litigation against us and/or our directors or officers; compliance with anti-corruption laws and increased regulatory compliance costs; complying with emerging climate change regulations and the impact of climate change; recoverability of deferred consideration to be received in connection with recent divestitures; uncertainties related to title to our mineral properties and the ability to obtain surface rights; our insurance coverage; civil disobedience in the countries where our mineral properties are located; operational safety and security risks; actions required to be taken by us under human rights law; our ability to access, when required, mining equipment and services; competition in the mining industry for mineral properties; shortage or poor quality of equipment or supplies; our ability to complete and successfully integrate an announced acquisition; conflicts of interest that could arise from some of our directors’ and officers’ involvement with other natural resource companies; information systems security risks; certain terms of our convertible notes; and those other various risks and uncertainties identified under the heading “Risk Factors” in our most recent Annual Information Form filed with the Canadian securities regulatory authorities and Annual Report on Form 40-F filed with the U.S. Securities and Exchange Commission (“SEC”).
This list is not exhaustive of the factors that may affect any of our forward-looking statements. Our forward-looking statements are based on what our management currently considers to be reasonable assumptions, beliefs, expectations and opinions based on the information currently available to it. Assumptions have been made regarding, among other things: our ability to carry on our exploration and development activities; our ability to meet our obligations under our property agreements; the timing and results of drilling programs; the discovery of Mineral Resources and Mineral Reserves on our mineral properties; the timely receipt of required approvals and permits, including those approvals and permits required for successful project permitting, construction and operation of our projects; the price of the minerals we produce; the costs of operating and exploration expenditures; our ability to operate in a safe, efficient and effective manner; our ability to obtain financing as and when required and on reasonable terms; and our ability to continue operating the Pirquitas mine and the Marigold mine. You are cautioned that the foregoing list is not exhaustive of all factors and assumptions which may have been used. We cannot assure you that actual events, performance or results will be consistent with these forward-looking statements, and management’s assumptions may prove to be incorrect. Our forward-looking statements reflect current expectations regarding future events and operating performance and speak only as of the date hereof and we do not assume any obligation to update forward-looking statements if circumstances or management’s beliefs, expectations or opinions should change other than as required by applicable law. For the reasons set forth above, you should not place undue reliance on forward-looking statements.
Cautionary Note to U.S. Investors
This news release includes Mineral Reserves and Mineral Resources classification terms that comply with reporting standards in Canada and the Mineral Reserves and the Mineral Resources estimates are made in accordance with NI 43-101. NI 43-101 is a rule developed by the Canadian Securities Administrators that establishes standards for all public disclosure an issuer makes of scientific and technical information concerning mineral projects. These standards differ significantly from the requirements of the SEC set out in Industry Guide 7. Consequently, Mineral Reserves and Mineral Resources information included in this news release is not comparable to similar information that would generally be disclosed by domestic U.S. reporting companies subject to the reporting and disclosure requirements of the SEC. Under SEC standards, mineralization may not be classified as a “reserve” unless the determination has been made that the mineralization could be economically produced or extracted at the time the reserve determination is made. In addition, the SEC’s disclosure standards normally do not permit the inclusion of information concerning “Measured Mineral Resources,” “Indicated Mineral Resources” or “Inferred Mineral Resources” or other descriptions of the amount of mineralization in mineral deposits that do not constitute “reserves” by U.S. standards in documents filed with the SEC. U.S. investors should understand that “Inferred Mineral Resources” have a great amount of uncertainty as to their existence and great uncertainty as to their economic and legal feasibility. Moreover, the requirements of NI 43-101 for identification of “reserves” are also not the same as those of the SEC, and reserves reported by us in compliance with NI 43-101 may not qualify as “reserves” under SEC standards. Accordingly, information concerning mineral deposits set forth herein may not be comparable with information made public by companies that report in accordance with U.S. standards.
Page 6

Table 2. Reverse circulation and sonic drilling assay results received in H1 2015 for the Marigold Exploration Drill Program.

Hole ID | UTM-N (Nad27 Zone 11) | UTM-E (Nad27 Zone 11) | Elevation (masl) | Azimuth (deg.) | Dip (deg.) | Length (metres) | Classification | Area
MRA6025 | 4510322 | 486716 | 1482 | 89 | -50 | 230 | NSA | 8D
MRA6031 | 4509640 | 486170 | 1524 | 268 | -75 | 398 | Resource | 8SX
MRA6032 | 4509677 | 486130 | 1524 | 88 | -76 | 230 | Resource | 8SX
MR6034 | 4509705 | 486091 | 1525 | 325 | -90 | 306 | Highlights | 8SX
MR6038 | 4510169 | 486578 | 1486 | 320 | -90 | 154 | Resource | 8D
MRA6040 | 4510169 | 486579 | 1486 | 91 | -66 | 154 | Resource | 8D
MR6041 | 4510322 | 486715 | 1482 | 9 | -90 | 184 | NSA | 8D
MR6042 | 4510747 | 486013 | 1481 | 323 | -89 | 291 | Highlights | 8D
MRA6043 | 4510747 | 486014 | 1481 | 86 | -56 | 261 | Resource | 8D
MRA6044 | 4508359 | 485067 | 1486 | 90 | -55 | 244 | Resource | Terry Zone
MR6045 | 4510624 | 485967 | 1484 | 145 | -89 | 367 | Highlights | 8D
MRA6046 | 4510624 | 485966 | 1484 | 268 | -68 | 337 | Highlights | 8D
MR6047 | 4510505 | 485982 | 1487 | 46 | -88 | 367 | Resource | 8D
MRA6048 | 4510443 | 486030 | 1489 | 270 | -84 | 322 | Resource | 8D
MR6049 | 4509302 | 486111 | 1526 | 84 | -90 | 139 | Resource | 8SX
MRA6050 | 4509302 | 486111 | 1526 | 246 | -64 | 184 | Resource | 8SX
MRA6051 | 4509651 | 486042 | 1523 | 217 | -64 | 306 | Resource | 8SX
MRA6052 | 4509650 | 486041 | 1523 | 218 | -45 | 415 | Resource | 8SX
MRA6053 | 4509681 | 486043 | 1524 | 266 | -78 | 306 | Highlights | 8SX
MRA6054 | 4509620 | 485717 | 1521 | 118 | -70 | 294 | Resource | 8SX
MRA6055 | 4509620 | 485718 | 1521 | 120 | -48 | 459 | Highlights | 8SX
MR6056 | 4509559 | 485671 | 1522 | 82 | -89 | 306 | Resource | 8SX
MRA6057 | 4509555 | 485674 | 1522 | 272 | -70 | 215 | Resource | 8SX
MRA6058 | 4509405 | 485573 | 1524 | 88 | -47 | 337 | Resource | 8SX
MRA6059 | 4509437 | 485597 | 1524 | 90 | -65 | 352 | Resource | 8SX
MRA6060 | 4509041 | 485478 | 1527 | 67 | -64 | 230 | Resource | 8SX
MRA6061 | 4509042 | 485480 | 1526 | 65 | -44 | 373 | Resource | 8SX
MRA6062 | 4509558 | 485562 | 1558 | 266 | -75 | 306 | Resource | 8SX
MRA6063 | 4509619 | 485575 | 1564 | 270 | -70 | 276 | Highlights | 8SX
MR6064 | 4509682 | 485834 | 1521 | 321 | -90 | 312 | Resource | 8SX
MRA6065 | 4509681 | 485834 | 1521 | 135 | -61 | 378 | Resource | 8SX
MRA6066 | 4508473 | 485149 | 1394 | 166 | -80 | 213 | Resource | Terry Zone/ Core Pre-Collar
MRA6067 | 4510383 | 485992 | 1491 | 270 | -79 | 300 | Resource | 8D
MR6068 | 4510166 | 486045 | 1485 | 221 | -90 | 306 | Resource | 8D
MR6069 | 4510259 | 485977 | 1493 | 285 | -88 | 337 | Resource | 8D
MRA6070 | 4510260 | 485978 | 1493 | 89 | -60 | 306 | Resource | 8D
MRA6071 | 4509407 | 486024 | 1553 | 265 | -56 | 180 | Resource | 8SX
MRA6072 | 4509571 | 486226 | 1524 | 86 | -69 | 197 | Resource | 8SX
MRA6073 | 4509634 | 486234 | 1524 | 72 | -79 | 215 | Resource | 8SX
MRA6074 | 4510322 | 485939 | 1493 | 88 | -79 | 312 | Resource | 8D
MRA6075 | 4510443 | 486157 | 1454 | 269 | -76 | 306 | Resource | 8D
MR6076 | 4509687 | 486289 | 1501 | 245 | -89 | 184 | Resource | 8SX
MRA6077 | 4509687 | 486288 | 1501 | 270 | -60 | 184 | Resource | 8SX
MRA6078 | 4509530 | 486114 | 1524 | 270 | -60 | 373 | Resource | 8SX
MR6079 | 4510566 | 485983 | 1486 | 67 | -89 | 338 | Highlights | 8D
MRA6080 | 4510566 | 485982 | 1486 | 272 | -71 | 337 | Highlights | 8D

Page 7

Hole ID | UTM-N (Nad27 Zone 11) | UTM-E (Nad27 Zone 11) | Elevation (masl) | Azimuth (deg.) | Dip (deg.) | Length (metres) | Classification | Area
MRA6081 | 4509710 | 486413 | 1497 | 92 | -80 | 139 | Resource | 8SX
MRA6082 | 4509710 | 486414 | 1497 | 90 | -56 | 154 | Resource | 8SX
MR6083 | 4510536 | 486045 | 1486 | 138 | -89 | 322 | NSA | 8D
MRA6084 | 4510536 | 486045 | 1486 | 92 | -69 | 367 | Resource | 8D
MRA6085 | 4509530 | 486115 | 1524 | 273 | -69 | 398 | Highlights | 8SX
MR6086 | 4509726 | 486305 | 1501 | 254 | -89 | 154 | Resource | 8SX
MRA6087 | 4509726 | 486305 | 1502 | 272 | -74 | 184 | Resource | 8SX
MRA6088 | 4509530 | 486115 | 1524 | 271 | -80 | 343 | Resource | 8SX
MRA6089 | 4509529 | 486163 | 1526 | 269 | -81 | 245 | Assay Pending | 8SX
MRA6090 | 4510672 | 485962 | 1483 | 82 | -68 | 291 | Resource | 8D
MRA6091 | 4510672 | 486032 | 1483 | 79 | -59 | 261 | Resource | 8D
MRA6092 | 4509529 | 486166 | 1525 | 0 | -90 | 245 | Assay Pending | 8SX
MRA6093 | 4509560 | 486114 | 1524 | 270 | -70 | 308 | Assay Pending | 8SX
MRA6094 | 4509531 | 485892 | 1591 | 186 | -80 | 428 | Resource | 8SX
MRA6095 | 4509408 | 485832 | 1609 | 268 | -86 | 343 | Resource | 8SX
MRA6096 | 4509164 | 485724 | 1610 | 273 | -86 | 361 | Resource | 8SX
MRA6097 | 4509590 | 486095 | 1524 | 268 | -75 | 306 | Resource | 8SX
MRA6098 | 4510749 | 485929 | 1482 | 85 | -74 | 322 | Highlights | 8D
MRA6099 | 4509621 | 486074 | 1524 | 270 | -86 | 312 | Resource | 8SX
MRA6100 | 4510748 | 486117 | 1480 | 90 | -60 | 215 | Resource | 8D
MRA6101 | 4509651 | 486090 | 1524 | 271 | -66 | 291 | Resource | 8SX
MRA6102 | 4510809 | 485906 | 1480 | 98 | -84 | 306 | Resource | 8D
MR6103 | 4509710 | 486066 | 1525 | 0 | -90 | 291 | Highlights | 8SX
MRA6104 | 4510626 | 485935 | 1484 | 89 | -84 | 346 | Highlights | 8D
MRA6105 | 4509711 | 486066 | 1525 | 90 | -61 | 261 | Resource | 8SX
MRA6106 | 4510626 | 485971 | 1484 | 95 | -69 | 352 | Resource | 8D
MRA6107 | 4509499 | 486116 | 1524 | 269 | -60 | 373 | Resource | 8SX
MRA6108 | 4509498 | 486117 | 1524 | 275 | -75 | 367 | Resource | 8SX
MR6111 | 4509434 | 485844 | 1610 | 21 | -89 | 396 | Assay Pending | 8SX
MRA6112 | 4509560 | 486115 | 1524 | 270 | -80 | 404 | Resource | 8SX
MRA6113 | 4509529 | 486166 | 1525 | 92 | -74 | 245 | Assay Pending | 8SX
MRA6114 | 4509621 | 486072 | 1524 | 272 | -60 | 343 | Assay Pending | 8SX
MRA6116 | 4509635 | 486237 | 1525 | 90 | -50 | 184 | Assay Pending | 8SX
MRA6117 | 4509681 | 486027 | 1523 | 272 | -58 | 337 | Assay Pending | 8SX
MRA6118 | 4509711 | 486029 | 1524 | 0 | -90 | 306 | Assay Pending | 8SX
MR6123 | 4509704 | 486130 | 1526 | 122 | -88 | 276 | Resource | 8SX
SON-1 | 4510028 | 486065 | 1503 | 0 | -90 | 30 | Resource | Rock Stockpile
SON-2 | 4509918 | 486129 | 1501 | 0 | -90 | 46 | Resource | Rock Stockpile
SON-3 | 4509755 | 486292 | 1501 | 0 | -90 | 73 | Resource | Rock Stockpile
SON-4 | 4509164 | 485724 | 1610 | 273 | -86 | 101 | Resource | Rock Stockpile
SON-5 | 4509408 | 485832 | 1609 | 268 | -86 | 113 | Resource | Rock Stockpile
SON-6 | 4509531 | 485892 | 1591 | 186 | -80 | 101 | Resource | Rock Stockpile
SON-7 | 4509369 | 486237 | 1537 | 0 | -90 | 23 | Resource | Decommissioned Leach Cell
SON-8 | 4509172 | 486288 | 1557 | 0 | -90 | 41 | Resource | Decommissioned Leach Cell
SON-9 | 4511217 | 488083 | 1458 | 0 | -90 | 12 | Resource | Tailings Storage Facility
SON-10 | 4511065 | 488351 | 1455 | 0 | -90 | 9 | Assay Pending | Tailings Storage Facility
SON-11 | 4509553 | 486522 | 1529 | 0 | -90 | 26 | Assay Pending | Decommissioned Leach Cell

Page 8

Hole ID | UTM-N (Nad27 Zone 11) | UTM-E (Nad27 Zone 11) | Elevation (masl) | Azimuth (deg.) | Dip (deg.) | Length (metres) | Classification | Area
SON-12 | 4509411 | 486434 | 1524 | 180 | -30 | 23 | Assay Pending | Decommissioned Leach Cell
SON-13 | 4509976 | 486151 | 1502 | 90 | -70 | 135 | Resource | Rock Stockpile
SON-14 | 4509779 | 485524 | 1580 | 0 | -90 | 67 | Resource | Rock Stockpile
SON-15 | 4510314 | 486180 | 1467 | 0 | -90 | 70 | NSA | Rock Stockpile
SON-16 | 4509510 | 486370 | 1525 | 0 | -90 | 18 | Resource | Decommissioned Leach Cell
SON-17 | 4510130 | 487001 | 1535 | 0 | -90 | 52 | Resource | Decommissioned Leach Cell
SON-18 | 4510204 | 486895 | 1526 | 0 | -90 | 43 | Assay Pending | Decommissioned Leach Cell
SON-19 | 4509864 | 486212 | 1500 | 0 | -90 | 107 | Assay Pending | Rock Stockpile
SON-20 | 4509117 | 485747 | 1601 | 0 | -90 | 78 | Assay Pending | Rock Stockpile
SON-21 | 4509175 | 485785 | 1608 | 0 | -90 | 88 | Assay Pending | Rock Stockpile
SON-22 | 4509102 | 485652 | 1609 | 0 | -90 | 88 | Assay Pending | Rock Stockpile
SON-23 | 4509224 | 485743 | 1610 | 0 | -90 | 90 | Assay Pending | Rock Stockpile
SRC-24 | 4509266 | 485756 | 1610 | 0 | -90 | 107 | Assay Pending | Rock Stockpile
SON-26 | 4509150 | 485658 | 1611 | 0 | -90 | 90 | Assay Pending | Rock Stockpile
SRC-28 | 4509173 | 485751 | 1609 | 0 | -90 | 91 | Assay Pending | Rock Stockpile
SON-29 | 4509286 | 485820 | 1613 | 0 | -90 | 94 | Assay Pending | Rock Stockpile
SRC-31 | 4509285 | 486037 | 1550 | 0 | -90 | 40 | Assay Pending | Rock Stockpile
SRC-32 | 4509187 | 485702 | 1609 | 0 | -90 | 104 | Assay Pending | Rock Stockpile
SON-39 | 4509394 | 485898 | 1609 | 0 | -90 | 98 | Assay Pending | Rock Stockpile
SRC-40 | 4509342 | 485785 | 1609 | 0 | -90 | 107 | Assay Pending | Rock Stockpile

Note: Drillholes not reported in Table 2 have not yet been drilled. Descriptions for Classification include: ‘Highlights’, which refers to ‘Highlighted Result’ included in Table 1 and Figure 1, ‘Resource’ which indicates that the Resource Intercept meets the Mineral Resources grade criteria, and ‘NSA’ which refers to ‘No Significant Assay’.
Page 9