EX-99.1 2 ssrminingannouncespositive.htm EX-99.1

|  | News Release

November 28, 2022
SSR MINING ANNOUNCES POSITIVE EXPLORATION RESULTS AT MARIGOLD CREATING PATHWAYS FOR MINE PLAN ENHANCEMENT AND EXTENSION
Oxide Intercepts Include 4.2 g/t Au Over 26 Meters and 2.7 g/t Au Over 17 Meters at New Millennium; Updated Technical Report on Track for 2023
DENVER - SSR Mining Inc. (NASDAQ/TSX: SSRM, ASX: SSR) ("SSR Mining" or the “Company") is pleased to announce results from 316 drillholes completed at the Marigold mine in Nevada, USA, for the period from October, 2021 to August, 2022 (Figure 1) at the New Millennium, Trenton Canyon and Buffalo Valley oxide targets. These results build upon, and are subsequent to, the Marigold 2021 Technical Report Summary. With an existing Mineral Reserve life of 11 years, exploration at Marigold is focused on adding higher-grade oxide ounces to the mine plan to both enhance and extend the current production profile and life of mine free cash flow generation. The continued exploration success at these key exploration targets has the potential to drive Mineral Reserve and Mineral Resource growth that can be incorporated into an updated Technical Report Summary for Marigold, which is expected in 2023 (the “2023 Marigold TRS”). The 2023 Marigold TRS will evaluate the potential to add New Millennium to the life of mine plan. Future studies will evaluate mining and processing opportunities at the Trenton Canyon and Buffalo Valley satellite targets located four and ten kilometers south of New Millennium, respectively.
The potential development of New Millennium was unlocked by recent brownfield strategic land acquisitions and presents an opportunity to add higher-grade oxide Mineral Reserves and Mineral Resources proximal to existing Marigold infrastructure. The New Millennium target area is comprised of six distinct zones which include East Basalt, Battle Cry, Antler, Section 6, Lil’ Gun and North Antler. These targets are on the periphery of the Antler-Basalt pits that previously produced approximately one million ounces at a grade of 0.75 g/t. Nearly 45,000 meters of drilling was completed at New Millennium across 146 holes, with numerous intercepts significantly above Marigold’s existing Mineral Reserve grade and new mineralization encountered more than five hundred meters south of previously defined Mineral Resources.
New Millennium oxide drilling highlights include (see Figures 2 and 3) (see Table 1):
•MRA7621: 25.9 meters at 4.2 g/t Au from 117.3 meters
•MRA7623: 16.8 meters at 2.7 g/t Au from 120.4 meters
•MRA7629: 22.9 meters at 1.7 g/t Au from 231.6 meters
•MRA7520: 21.3 meters at 1.7 g/t Au from 195.1 meters, and 19.8 meters at 1.9 g/t Au from 225.6 meters
Rod Antal, President and CEO of SSR Mining, said, “These results showcase exceptional oxide grades that have potential to drive Mineral Reserve and Mineral Resource growth and complement the existing Marigold production profile. We expect to include some of this higher-grade oxide material in the 2023 Marigold TRS, which we anticipate will demonstrate an optimized and expanded production profile through the incorporation of New Millennium. In addition, with the recent results from both Trenton Canyon and Buffalo Valley, we believe the future is very bright for Marigold with opportunities to extend the existing 11 year mine life while adding higher grade, lower cost oxide ounces to the near and longer-term mine plan.”

SSR Mining Inc. |  | PAGE 1

Figure 1: Plan view of the Marigold property
Table 1: Significant oxide gold intercepts at New Millennium

Hole ID | From (m) | To (m) | Interval (m) | Grade (g/t Au) | Oxidation State | Area
MRA7621 | 117.3 | 143.3 | 25.9 | 4.2 | Oxide | New Millennium
including | 123.4 | 137.2 | 13.7 | 6.8 | Oxide
MRA7623 | 120.4 | 137.2 | 16.8 | 2.7 | Oxide | New Millennium
including | 125.0 | 129.5 | 4.6 | 5.1 | Oxide
MRA7629 | 231.6 | 254.5 | 22.9 | 1.7 | Oxide | New Millennium
MRA7520 | 195.1 | 216.4 | 21.3 | 1.7 | Oxide | New Millennium
including | 202.7 | 205.7 | 3.0 | 4.7 | Oxide
| 225.6 | 245.4 | 19.8 | 1.9 | Oxide
MR7626 | 198.1 | 239.3 | 41.1 | 0.9 | Oxide | New Millennium
MRA7560 | 118.9 | 144.8 | 25.9 | 1.4 | Oxide | New Millennium
MRA7628 | 221.0 | 245.4 | 24.4 | 1.4 | Oxide | New Millennium
MRA7630 | 222.5 | 242.3 | 19.8 | 1.6 | Oxide | New Millennium
including | 231.6 | 236.2 | 4.6 | 3.7 | Oxide
MRA7755 | 108.2 | 129.5 | 21.3 | 1.4 | Oxide | New Millennium
MRA7624 | 120.4 | 155.4 | 35.1 | 0.8 | Oxide | New Millennium

SSR Mining Inc. |  | PAGE 2

In addition to drilling at New Millennium, SSR Mining continues to explore for supplemental oxide ore sources across the broader Marigold land package. At Trenton Canyon and Buffalo Valley, located approximately four kilometers south and ten kilometers southwest of New Millennium, respectively, drilling has delivered exciting high-grade intercepts of predominantly oxide mineralization. Exploration at these targets aims to define oxide material that leverages existing infrastructure at Marigold to provide an avenue for production growth in the future. Work also continues to delineate and define initial sulfide resources at each target that could represent potential longer-term development opportunities for Marigold.
Trenton Canyon oxide drilling highlights include (see Figures 4 and 5) (see Table 2):
•MRA7795: 15.2 meters at 11.1 g/t Au from 213.4 meters
•MRA7587: 19.8 meters at 5.5 g/t Au from 181.4 meters
•MRA7518: 6.1 meters at 2.0 g/t Au from 41.1 meters and 25.9 meters at 1.2 g/t Au from 50.3 meters
Buffalo Valley oxide drilling highlights include (see Figures 6, 7 and 8) (see Table 2):
•DDH7705: 18.3 meters at 6.2 g/t Au from 126.5 meters
•MRA7730: 42.7 meters at 1.4 g/t Au from 382.5 meters
•MRA7598: 6.1 meters at 2.5 g/t Au from 324.6 meters
Additionally, an infill drill hole from the Valmy pit located to the northeast of New Millennium included the following oxide intercepts:
•DDH7452: 14.3 meters at 4.7 g/t Au from 209.4 meters and 12.5 meters at 0.8 g/t Au from 246.3 meters
Table 2: Significant oxide gold intercepts at Trenton Canyon and Buffalo Valley

Hole ID | From (m) | To (m) | Interval (m) | Grade (g/t Au) | Oxidation State | Area
MRA7795 | 213.4 | 228.6 | 15.2 | 11.1 | Oxide | Trenton Canyon
including | 213.4 | 222.5 | 9.1 | 17.0 | Oxide
DDH7705 | 126.5 | 144.8 | 18.3 | 6.2 | Oxide | Buffalo Valley
including | 127.3 | 132.6 | 5.3 | 13.9 | Oxide
including | 135.6 | 138.8 | 3.2 | 4.8 | Oxide
MRA7587 | 181.4 | 201.2 | 19.8 | 5.5 | Oxide | Trenton Canyon
including | 182.9 | 189.0 | 6.1 | 9.8 | Oxide
including | 192.0 | 198.1 | 6.1 | 6.1 | Oxide
MRA7730 | 382.5 | 425.2 | 42.7 | 1.4 | Oxide | Buffalo Valley
MRA7585 | 65.5 | 68.6 | 3.0 | 18.2 | Oxide | Trenton Canyon
MRA7817 | 219.5 | 230.1 | 10.7 | 4.1 | Oxide | Trenton Canyon
including | 221.0 | 225.6 | 4.6 | 8.3 | Oxide
MRA7578 | 103.6 | 118.9 | 15.2 | 2.8 | Oxide | Trenton Canyon
including | 108.2 | 111.3 | 3.0 | 4.4 | Oxide
including | 114.3 | 117.3 | 3.0 | 6.3 | Oxide
MRA7528 | 73.2 | 89.9 | 16.8 | 2.2 | Oxide | Trenton Canyon
MRA7598 | 324.6 | 330.7 | 6.1 | 2.5 | Oxide | Buffalo Valley
336.8 | 350.5 | 13.7 | 0.9 | Oxide
353.6 | 394.7 | 41.1 | 0.9 | Oxide
MRA7375 | 57.9 | 65.5 | 7.6 | 4.6 | Oxide | Trenton Canyon

SSR Mining Inc. |  | PAGE 3

While the exploration focus is to define and expand oxide inventory across the greater Marigold property, SSR Mining is simultaneously exploring for structurally controlled sulfide mineralization potentially amenable to alternative mining & processing methods than those currently utilized at Marigold. Building on results previously announced in December 2021, exploration efforts at Trenton Canyon have focused on the Tempest zone, a series of high-grade structures proximal to the past-producing South and West pits.
Trenton Canyon sulfide drilling highlights include (see Figures 4 and 5) (see Table 3):
•DDH7525: 6.1 meters at 25.6 g/t Au from 185.8 meters
o Including 3.7m at 41.4 g/t Au from 185.8 meters
•MRA7561: 16.8 meters at 2.6 g/t Au from 144.8 meters
•MRA7708: 12.2 meters at 3.9 g/t Au from 172.2 meters
As the exploration team furthers its understanding of sulfide mineralization at Marigold, it is applying this knowledge to a robust collection of high-quality and underexplored targets throughout the extensive Trenton Canyon and Buffalo Valley properties. One example is the Spitfire target, located approximately two kilometers northwest of the Buffalo Valley pit.
Highlight intercepts from the Spitfire target include (see Figure 6) (see Table 3):
•MRA7609: 6.1 meters at 20.1 g/t Au from 111.3 meters
•DDH7600: 6.9 meters at 2.0 g/t Au from 292.8 meters, including coarse visible gold
Table 3: Significant sulfide gold intercepts at Trenton Canyon and Buffalo Valley

Hole ID | From (m) | To (m) | Interval (m) | Grade (g/t Au) | Oxidation State | Area
DDH7525 | 185.8 | 191.8 | 6.1 | 25.6 | Sulfide | Trenton Canyon
including | 185.8 | 189.4 | 3.7 | 41.4 | Sulfide
MRA7609 | 111.3 | 117.3 | 6.1 | 20.1 | Sulfide | Buffalo Valley
MRA7840 | 362.7 | 385.6 | 22.9 | 4.4 | Sulfide | Trenton Canyon
including | 362.7 | 368.8 | 6.1 | 9.9 | Sulfide
MRA7708 | 172.2 | 184.4 | 12.2 | 3.9 | Sulfide | Trenton Canyon
including | 176.8 | 181.4 | 4.6 | 6.9 | Sulfide
MRA7703 | 259.1 | 269.7 | 10.7 | 3.2 | Sulfide | Trenton Canyon
including | 260.6 | 263.7 | 3.0 | 5.5 | Sulfide
MRA7540 | 266.7 | 271.3 | 4.6 | 7.4 | Sulfide | Trenton Canyon
MRA7842 | 204.2 | 210.3 | 6.1 | 5.2 | Sulfide | Trenton Canyon
MRA7598 | 330.7 | 336.8 | 6.1 | 5.0 | Sulfide | Buffalo Valley
MRA7517 | 327.7 | 330.7 | 3.0 | 8.7 | Sulfide | Trenton Canyon
MRA7561 | 144.8 | 161.5 | 16.8 | 2.6 | Mixed | Trenton Canyon
including | 150.9 | 155.4 | 4.6 | 3.6 | Sulfide

SSR Mining Inc. |  | PAGE 4

Marigold Exploration Figures
Figure 2. New Millennium plan view highlighting recent and historical drilling as well as Mineral Reserve and Mineral Resource pit boundaries
Figure 3. Section showing highlight oxide intercepts and the A – A’ section shown in Figure 2.

SSR Mining Inc. |  | PAGE 5

Figure 4. Trenton Canyon plan view highlighting recent and historical drilling
Figure 5. Section showing highlight oxide and sulfide intercepts at Trenton Canyon and the B – B’ section shown in Figure 4.

SSR Mining Inc. |  | PAGE 6

Figure 6. Buffalo Valley plan view showing recent and historical drilling
Figure 7. Section showing highlight oxide and sulfide intercepts at Buffalo Valley and the C – C’ section shown in Figure 6.

SSR Mining Inc. |  | PAGE 7

Figure 8. Section showing highlight oxide and sulfide intercepts at Buffalo Valley and the D – D’ section shown in Figure 6.

SSR Mining Inc. |  | PAGE 8

Marigold Exploration Overview
SSR Mining’s mineral holdings include a 100% owned approximately 20,000-hectare parcel containing the currently producing Marigold mine as well as the past producing Valmy, Trenton Canyon, North Peak, and Buffalo Valley mines. Activity during the Exploration Period (October 2021 to August, 2022) included 316 drillholes (308 reverse circulation and 8 core drillholes) focused on Mineral Reserve and Mineral Resource additions at New Millennium, Trenton Canyon, and Buffalo Valley, as well as infill drilling at the Mackay pit that improved confidence in existing Mineral Reserves and Mineral Resources.
New Millennium represents a low cost, high probability development opportunity in the Nevada portfolio and drilling at the target will continue with the ultimate goal to enhance and extend operations at Marigold beyond its current 11 year mine life. The New Millennium target area is comprised of six distinct zones which include East Basalt, Battle Cry, Antler, Section 6, Lil’ Gun and North Antler, and was enabled by land acquisitions completed in 2016, 2018 and 2019.
Currently, the Company has four drill rigs on-site at Marigold and is undertaking geotechnical, metallurgical and geophysical studies to better understand the multitude of prospective opportunities across the Marigold property. This includes the recent launch of a UAV magnetics survey across the Trenton Canyon, Buffalo Valley and North Peak targets. North Peak is another past producing oxide pit that is located between Trenton Canyon and Buffalo Valley.
As exploration continues to define opportunities for Mineral Reserve and Mineral Resource growth at these targets, the Company is applying a “District Master Plan” approach to future development, permitting and production of these opportunities. This approach, used successfully at Çöpler in the past, ensures Marigold has a well-defined longer-term pipeline of growth projects.
The Company is also continuing a re-assay program of historical drill samples in the New Millennium area with the potential to build on the success of the re-assay program across the greater Marigold property, including re-assaying in 2015-2016 which yielded a 23% increase in estimated tonnage and a 13% increase in gold ounces within the Mackay pits. The goal of this program is to capture low-grade gold assay values not recorded in the historical dataset and integrate the results with the updated resource model. The first phase of this program, which included the re-analysis of drill samples from two drill sections at New Millennium, yielded positive results and was expanded to encompass the entire project area. The second phase of this program, which included approximately 650 samples, is also yielding positive results. The focus of this phase is to add value to ongoing drilling program.
Technical Procedural Information Sampling and Analytical Procedures
Drill samples from the Marigold mine drilling program were sent for processing and analysis to the offices of American Assay Laboratories, Inc. (“AAL”) in Sparks, Nevada which is an ISO 17025 accredited laboratory independent from SSR Mining. Fire assay was completed on a 30-gram sample (AAL method code FA-PB30-ICP) with an Inductively Coupled Plasma finish after a two acid digestion. Samples with assay results greater than 10 g/t gold were fire assayed on a 30-gram sample (AAL method code Grav Au30) with a gravimetric finish. Buffalo Valley samples greater than one gram are subjected to Screen Fire assays. We employ a rigorous Quality Assurance/Quality Control (“QA/QC”) program, which includes real-time assay quality monitoring through the regular insertion of blanks, duplicates, and certified reference material, as well as reviewing laboratory-provided QA/QC data and confirming results at umpire labs.
External review of data and processes relating to Marigold exploration data have been completed by an independent consultant F. C. Edmunds, P. Geo., in November 2022. There were no adverse material results detected and the QA/QC indicates the information collected is acceptable, and the database can be used for further studies.

SSR Mining Inc. |  | PAGE 9

Qualified Persons
The scientific and technical data contained in this news release relating to the Marigold mine have been reviewed and approved by Richard J. Yancey, Resource Development Manager at Marigold Mine, a Society of Mining, Metallurgy and Exploration Registered Member, and a qualified person for purposes of Subpart 1300 of Regulation S-K and National Instrument 43-101 - Standards of Disclosure for Mineral Projects.
You are encouraged to also review the 2021 Marigold TRS, which is available on SSR Mining’s Current Report on Form 8-K filed with the Securities and Exchange Commission’s EDGAR system (sec.gov) on September 29, 2022.
About SSR Mining
SSR Mining Inc. is a leading, free cash flow focused gold company with four producing assets located in the USA, Türkiye, Canada, and Argentina, combined with a global pipeline of high-quality development and exploration assets. In 2021, the four operating assets produced approximately 794,000 gold-equivalent ounces. SSR Mining is listed under the ticker symbol SSRM on the NASDAQ and the TSX, and SSR on the ASX.
SSR Mining Contacts:
F. Edward Farid, Executive Vice President, Chief Corporate Development Officer
Alex Hunchak, Director, Corporate Development and Investor Relations
SSR Mining Inc.
E-Mail: invest@ssrmining.com
Phone: +1 (888) 338-0046
To receive SSR Mining’s news releases by e-mail, please register using the SSR Mining website at www.ssrmining.com.

SSR Mining Inc. |  | PAGE 10

Cautionary Note Regarding Forward-Looking Information
Except for statements of historical fact relating to us, certain statements contained in this news release constitute forward-looking information, future oriented financial information, or financial outlooks (collectively “forward-looking information”) within the meaning of applicable securities laws. Forward-looking information may be contained in this document and our other public filings. Forward-looking information relates to statements concerning our outlook and anticipated events or results and, in some cases, can be identified by terminology such as “may”, “will”, “could”, “should”, “expect”, “plan”, “anticipate”, “believe”, “intend”, “estimate”, “projects”, “predict”, “potential”, “continue” or other similar expressions concerning matters that are not historical facts.
Forward-looking information and statements in this news release are based on certain key expectations and assumptions made by us. Although we believe that the expectations and assumptions on which such forward-looking information and statements are based are reasonable, undue reliance should not be placed on the forward-looking information and statements because we can give no assurance that they will prove to be correct. Forward-looking information and statements are subject to various risks and uncertainties which could cause actual results and experience to differ materially from the anticipated results or expectations expressed in this news release. The key risks and uncertainties include, but are not limited to: local and global political and economic conditions; governmental and regulatory requirements and actions by governmental authorities, including changes in government policy, government ownership requirements, changes in environmental, tax and other laws or regulations and the interpretation thereof; developments with respect to the COVID-19 pandemic, including the duration, severity and scope of the pandemic and potential impacts on mining operations; and other risk factors detailed from time to time in our reports filed with the Securities and Exchange Commission on EDGAR and the Canadian securities regulatory authorities on SEDAR.
Forward-looking information and statements in this news release include any statements concerning, among other things: preliminary cost reporting in this document; production, operating, cost, and capital expenditure guidance; our operational and development targets and catalysts and the impact of any suspension on operations; forecasts and outlook, including related to production guidance; timing and expectations regarding the impact of any interruptions caused on our operations; the results of any gold reconciliations; the ability to discover additional oxide gold ore; matters relating to proposed exploration; communications with local stakeholders; maintaining community and government relations; negotiations of joint ventures; negotiation and completion of transactions; commodity prices; Mineral Resources, Mineral Reserves, conversion of Mineral Resources, realization of Mineral Reserves, and the existence or realization of Mineral Resource estimates; the development approach; the timing and amount of future production; the timing of studies, announcements, and analysis; the timing of construction and development of proposed mines and process facilities; capital and operating expenditures; economic conditions; availability of sufficient financing; exploration plans; receipt of regulatory approvals; and any and all other timing, exploration, development, operational, financial, budgetary, economic, legal, social, environmental, regulatory, and political matters that may influence or be influenced by future events or conditions.
Such forward-looking information and statements are based on a number of material factors and assumptions, including, but not limited in any manner to, those disclosed in any other of our filings on EDGAR and SEDAR, and include: the inherent speculative nature of exploration results; the ability to explore; communications with local stakeholders; maintaining community and governmental relations; status of negotiations of joint ventures; weather conditions at our operations; commodity prices; the ultimate determination of and realization of Mineral Reserves; existence or realization of Mineral Resources; the development approach; availability and receipt of required approvals, titles, licenses and permits; sufficient working capital to develop and operate the mines and implement development plans; access to adequate services and supplies; foreign currency exchange rates; interest rates; access to capital markets and associated cost of funds; availability of a qualified work force; ability to negotiate, finalize, and execute relevant agreements; lack of social opposition to our mines or facilities; lack of legal challenges with respect to our properties; the timing and amount of future production; the ability to meet production, cost, and capital expenditure targets; timing and ability to produce studies and analyses; capital and operating expenditures; economic conditions; availability of sufficient financing; the ultimate ability to mine, process, and sell mineral products on economically favorable terms; and any and all other timing, exploration, development, operational, financial, budgetary, economic, legal, social, geopolitical, regulatory and political factors that may influence future events or conditions. While we consider these factors and assumptions to be reasonable based on information currently available to us, they may prove to be incorrect.
The above list is not exhaustive of the factors that may affect any of the Company’s forward-looking information. You should not place undue reliance on forward-looking information and statements. Forward-looking information and statements are only predictions based on our current expectations and our projections about future events. Actual results may vary from such forward-looking information for a variety of reasons including, but not limited to, risks and uncertainties disclosed in our filings on our website at www.ssrmining.com, on SEDAR at www.sedar.com, on EDGAR at www.sec.gov and on the ASX at www.asx.com.au and other unforeseen events or circumstances. Other than as required by law, we do not intend, and undertake no obligation to update any forward-looking information to reflect, among other things, new information or future events. The information contained on, or that may be accessed through, our website is not incorporated by reference into, and is not a part of, this document.
Qualified Persons
The scientific and technical information concerning our mineral projects in this news release have been reviewed and approved by a “qualified person” under S-K 1300. For details on the “qualified persons” approving such information, a description of the key assumptions, parameters and methods used to estimate mineral reserves and mineral resources for SSR Mining Inc.’s material properties included in this news release, as well as data verification procedures and a general discussion of the extent to which the estimates may be affected by any known environmental, permitting, legal, title, taxation, sociopolitical, marketing or other relevant factors, please review the Technical Report Summaries for each of the Company’s material properties which are available at www.sec.gov.

SSR Mining Inc. |  | PAGE 11

Table 4: All drill holes completed at Marigold between October 31, 2021 to August 30, 2022.

Hole ID | From (m) | To (m) | Interval (m) | Grade (g/t Au) | Oxidation State | Area
MRA7231 | 185.9 | 198.1 | 12.2 | 0.60 | Oxide | New Millennium
304.8 | 307.8 | 3.0 | 0.53 | Oxide
MRA7255 | 150.9 | 153.9 | 3.0 | 1.53 | Sulfide | Trenton Canyon
323.1 | 327.7 | 4.6 | 1.31 | Sulfide
MRA7327 | 269.7 | 272.8 | 3.0 | 1.59 | Sulfide | Trenton Canyon
MR7370 | 329.2 | 332.2 | 3.0 | 0.47 | Oxide | New Millennium
MRA7371 | NSI | Trenton Canyon
MRA7375 | 57.9 | 65.5 | 7.6 | 4.61 | Oxide | Trenton Canyon
MRA7423 | NSI | Trenton Canyon
DDH7452 | 203.3 | 206.7 | 3.4 | 0.70 | Oxide | Valmy
209.4 | 223.7 | 14.3 | 4.71 | Oxide
including | 209.4 | 213.2 | 3.8 | 14.13 | Oxide
| 246.3 | 258.8 | 12.5 | 0.80 | Oxide
MRA7469 | 259.1 | 263.7 | 4.6 | 0.42 | Oxide | New Millennium
278.9 | 281.9 | 3.0 | 0.52 | Oxide
MRA7474 | NSI | Trenton Canyon
MRA7480 | NSI | Trenton Canyon
MR7484 | 134.1 | 137.2 | 3.0 | 0.59 | Oxide | Mackay
MRA7495 | 157.0 | 164.6 | 7.6 | 0.98 | Oxide | New Millennium
178.3 | 187.5 | 9.1 | 1.08 | Oxide
227.1 | 234.7 | 7.6 | 0.66 | Oxide
291.1 | 294.1 | 3.0 | 0.47 | Oxide
306.3 | 310.9 | 4.6 | 0.89 | Oxide
356.6 | 359.7 | 3.0 | 0.39 | Oxide
MR7500 | 48.8 | 65.5 | 16.8 | 0.72 | Oxide | Mackay
102.1 | 112.8 | 10.7 | 0.42 | Oxide
143.3 | 155.4 | 12.2 | 0.86 | Oxide
MR7501 | NSI | Mackay
MR7502 | NSI | Mackay
MRA7503 | 187.5 | 195.1 | 7.6 | 0.38 | Oxide | New Millennium
271.3 | 274.3 | 3.0 | 1.52 | Mixed
285.0 | 289.6 | 4.6 | 2.39 | Oxide
295.7 | 298.7 | 3.0 | 1.16 | Oxide
327.7 | 330.7 | 3.0 | 0.57 | Oxide
MRA7504 | 216.4 | 221.0 | 4.6 | 0.47 | Oxide | New Millennium
324.6 | 327.7 | 3.0 | 1.28 | Oxide
344.4 | 352.0 | 7.6 | 0.36 | Oxide
MRA7505 | 227.1 | 230.1 | 3.0 | 2.49 | Oxide | Trenton Canyon
230.1 | 233.2 | 3.0 | 9.23 | Mixed
233.2 | 248.4 | 15.2 | 0.79 | Oxide
MRA7506 | 265.2 | 269.7 | 4.6 | 1.78 | Sulfide | Trenton Canyon
277.4 | 289.6 | 12.2 | 1.49 | Sulfide
297.2 | 300.2 | 3.0 | 2.20 | Sulfide

SSR Mining Inc. |  | PAGE 12

Hole ID | From (m) | To (m) | Interval (m) | Grade (g/t Au) | Oxidation State | Area
MRA7507 | 301.8 | 307.8 | 6.1 | 2.66 | Sulfide | Trenton Canyon
323.1 | 326.1 | 3.0 | 3.22 | Sulfide
330.7 | 335.3 | 4.6 | 2.00 | Sulfide
344.4 | 347.5 | 3.0 | 1.37 | Sulfide
MRA7508 | NSI | Trenton Canyon
MRA7509 | NSI | Trenton Canyon
MRA7510 | 269.7 | 278.9 | 9.1 | 2.29 | Sulfide | Trenton Canyon
including | 271.3 | 274.3 | 3.0 | 3.65 | Sulfide
| 281.9 | 288.0 | 6.1 | 1.92 | Sulfide
MRA7511 | NSI | New Millennium
MRA7512 | NSI | New Millennium
MR7515 | NSI | Mackay
MRA7516 | 74.7 | 79.2 | 4.6 | 1.61 | Sulfide | Trenton Canyon
82.3 | 86.9 | 4.6 | 1.57 | Oxide
117.3 | 125.0 | 7.6 | 0.48 | Oxide
146.3 | 152.4 | 6.1 | 1.27 | Oxide
160.0 | 175.3 | 15.2 | 1.53 | Oxide
179.8 | 182.9 | 3.0 | 0.83 | Sulfide
184.4 | 190.5 | 6.1 | 1.67 | Sulfide
MRA7517 | 327.7 | 330.7 | 3.0 | 8.66 | Sulfide | Trenton Canyon
MRA7518 | 4.6 | 10.7 | 6.1 | 1.63 | Oxide | Trenton Canyon
41.1 | 47.2 | 6.1 | 2.02 | Oxide
50.3 | 76.2 | 25.9 | 1.17 | Oxide
80.8 | 88.4 | 7.6 | 1.50 | Oxide
88.4 | 93.0 | 4.6 | 1.53 | Sulfide
97.5 | 100.6 | 3.0 | 3.02 | Oxide
112.8 | 121.9 | 9.1 | 2.75 | Mixed
155.4 | 158.5 | 3.0 | 0.62 | Oxide
221.0 | 227.1 | 6.1 | 1.05 | Sulfide
MRA7519 | NSI | Trenton Canyon
MRA7520 | 195.1 | 216.4 | 21.3 | 1.71 | Oxide | New Millennium
including | 202.7 | 205.7 | 3.0 | 4.73 | Oxide
| 225.6 | 245.4 | 19.8 | 1.95 | Oxide
248.4 | 262.1 | 13.7 | 1.37 | Oxide
MR7521 | NSI | Mackay
MRA7522 | NSI | New Millennium
MRA7523 | NSI | Trenton Canyon
MRA7524 | 310.9 | 315.5 | 4.6 | 0.76 | Oxide | New Millennium
DDH7525 | 185.8 | 191.8 | 6.1 | 25.61 | Sulfide | Trenton Canyon
including | 185.8 | 189.4 | 3.7 | 41.42 | Sulfide
MRA7526 | NSI | Trenton Canyon
MRA7527 | 208.8 | 211.8 | 3.0 | 3.28 | Sulfide | Trenton Canyon
MRA7528 | 73.2 | 89.9 | 16.8 | 2.19 | Oxide | Trenton Canyon
MRA7529 | NSI | Trenton Canyon
MRA7530 | 4.6 | 10.7 | 6.1 | 1.26 | Oxide | Trenton Canyon

SSR Mining Inc. |  | PAGE 13

Hole ID | From (m) | To (m) | Interval (m) | Grade (g/t Au) | Oxidation State | Area
DDH7531 | 244.9 | 248.9 | 4.0 | 0.58 | Oxide | Trenton Canyon
279.7 | 287.3 | 7.6 | 6.98 | Mixed
including | 280.8 | 286.2 | 5.4 | 8.97 | Mixed
MRA7532 | 73.2 | 76.2 | 3.0 | 1.50 | Sulfide | Trenton Canyon
MR7533 | NSI | New Millennium
MR7534 | 350.5 | 353.6 | 3.0 | 0.72 | Oxide | New Millennium
MRA7535 | NSI | Trenton Canyon
MRA7536 | NSI | Trenton Canyon
MR7537 | 155.4 | 163.1 | 7.6 | 0.68 | Oxide | New Millennium
237.7 | 259.1 | 21.3 | 0.62 | Oxide
309.4 | 313.9 | 4.6 | 0.57 | Oxide
MRA7538 | 29.0 | 33.5 | 4.6 | 1.38 | Oxide | Trenton Canyon
MRA7539 | 301.8 | 304.8 | 3.0 | 5.15 | Sulfide | Trenton Canyon
MRA7540 | 38.1 | 42.7 | 4.6 | 3.36 | Oxide | Trenton Canyon
266.7 | 271.3 | 4.6 | 7.44 | Sulfide
352.0 | 356.6 | 4.6 | 1.34 | Sulfide
MRA7541 | 158.5 | 164.6 | 6.1 | 0.45 | Oxide | New Millennium
301.8 | 306.3 | 4.6 | 0.66 | Oxide
MRA7542 | 155.4 | 158.5 | 3.0 | 0.52 | Oxide | New Millennium
175.3 | 178.3 | 3.0 | 0.57 | Oxide
199.6 | 202.7 | 3.0 | 0.37 | Oxide
MRA7545 | 76.2 | 79.2 | 3.0 | 0.91 | Oxide | New Millennium
105.2 | 114.3 | 9.1 | 1.08 | Oxide
MRA7546 | 128.0 | 132.6 | 4.6 | 0.39 | Oxide | New Millennium
135.6 | 138.7 | 3.0 | 0.88 | Oxide
MR7547 | NSI | Trenton Canyon
MR7548 | NSI | Trenton Canyon
MRA7549 | 33.5 | 39.6 | 6.1 | 1.09 | Oxide | Trenton Canyon
MRA7550 | 32.0 | 35.1 | 3.0 | 0.85 | Oxide | Trenton Canyon
MRA7551 | NSI | Buffalo Valley
MRA7552 | 153.9 | 160.0 | 6.1 | 0.89 | Oxide | Buffalo Valley
MRA7553 | NSI | Trenton Canyon
MRA7554 | NSI | Trenton Canyon
MR7555 | 83.8 | 102.1 | 18.3 | 0.79 | Oxide | New Millennium
MRA7556 | 83.8 | 86.9 | 3.0 | 0.47 | Oxide | New Millennium
MRA7557 | 68.6 | 71.6 | 3.0 | 0.56 | Oxide | New Millennium
80.8 | 86.9 | 6.1 | 0.40 | Oxide
MRA7558 | NSI | New Millennium
MRA7559 | 102.1 | 106.7 | 4.6 | 2.91 | Oxide | New Millennium
MRA7560 | 112.8 | 115.8 | 3.0 | 0.41 | Oxide | New Millennium
118.9 | 144.8 | 25.9 | 1.38 | Oxide
166.1 | 175.3 | 9.1 | 0.64 | Oxide
144.8 | 161.5 | 16.8 | 2.62 | Mixed
including | 150.9 | 155.4 | 4.6 | 3.58 | Sulfide
| 161.5 | 166.1 | 4.6 | 1.19 | Oxide
253.0 | 256.0 | 3.0 | 3.34 | Sulfide

SSR Mining Inc. |  | PAGE 14

Hole ID | From (m) | To (m) | Interval (m) | Grade (g/t Au) | Oxidation State | Area
MRA7561 | 144.8 | 161.5 | 16.8 | 2.62 | Mixed | Trenton Canyon
including | 150.9 | 155.4 | 4.6 | 3.58 | Sulfide
| 161.5 | 166.1 | 4.6 | 1.19 | Oxide
253.0 | 256.0 | 3.0 | 3.34 | Sulfide
MRA7562 | NSI | Trenton Canyon
MRA7563 | 54.9 | 64.0 | 9.1 | 2.01 | Mixed | Trenton Canyon
MRA7564 | 53.3 | 65.5 | 12.2 | 0.39 | Oxide | New Millennium
80.8 | 85.3 | 4.6 | 0.60 | Oxide
MRA7565 | NSI | Trenton Canyon
MRA7566 | 192.0 | 195.1 | 3.0 | 0.37 | Oxide | New Millennium
213.4 | 224.0 | 10.7 | 1.31 | Oxide
DDH7567 | 155.3 | 160.2 | 4.9 | 0.81 | Oxide | Buffalo Valley
187.6 | 191.4 | 3.8 | 0.86 | Oxide
290.8 | 294.3 | 3.6 | 2.54 | Oxide
303.4 | 308.0 | 4.6 | 0.42 | Oxide
MRA7568 | 99.1 | 102.1 | 3.0 | 3.16 | Oxide | Trenton Canyon
MRA7569 | 54.9 | 57.9 | 3.0 | 1.73 | Mixed | Trenton Canyon
134.1 | 137.2 | 3.0 | 0.59 | Oxide
146.3 | 155.4 | 9.1 | 0.88 | Oxide
190.5 | 196.6 | 6.1 | 1.66 | Sulfide
MRA7570 | 64.0 | 68.6 | 4.6 | 0.94 | Oxide | Trenton Canyon
109.7 | 114.3 | 4.6 | 0.85 | Oxide
MRA7571 | NSI | New Millennium
MRA7572 | NSI | New Millennium
MRA7573 | 42.7 | 51.8 | 9.1 | 0.58 | Oxide | New Millennium
MRA7574 | NSI | New Millennium
MR7575 | 91.4 | 96.0 | 4.6 | 0.50 | Oxide | Trenton Canyon
MRA7576 | NSI | Trenton Canyon
MRA7577 | 54.9 | 57.9 | 3.0 | 5.25 | Sulfide | Trenton Canyon
80.8 | 100.6 | 19.8 | 1.41 | Oxide
120.4 | 125.0 | 4.6 | 0.75 | Oxide
MRA7578 | 50.3 | 54.9 | 4.6 | 1.46 | Sulfide | Trenton Canyon
76.2 | 79.2 | 3.0 | 1.32 | Oxide
103.6 | 118.9 | 15.2 | 2.78 | Oxide
including | 108.2 | 111.3 | 3.0 | 4.43 | Oxide
including | 114.3 | 117.3 | 3.0 | 6.34 | Oxide
MRA7579 | NSI | Trenton Canyon
MRA7582 | NSI | New Millennium
MRA7583 | NSI | New Millennium
MRA7584 | 88.4 | 91.4 | 3.0 | 0.55 | Oxide | Trenton Canyon
97.5 | 100.6 | 3.0 | 1.22 | Oxide
115.8 | 121.9 | 6.1 | 1.10 | Oxide
128.0 | 137.2 | 9.1 | 0.53 | Oxide
MRA7585 | 61.0 | 65.5 | 4.6 | 2.77 | Sulfide | Trenton Canyon
65.5 | 68.6 | 3.0 | 18.21 | Oxide
100.6 | 109.7 | 9.1 | 0.62 | Oxide

SSR Mining Inc. |  | PAGE 15

Hole ID | From (m) | To (m) | Interval (m) | Grade (g/t Au) | Oxidation State | Area
MRA7586 | 25.9 | 50.3 | 24.4 | 0.84 | Oxide | Trenton Canyon
62.5 | 65.5 | 3.0 | 0.88 | Oxide
MRA7587 | 147.8 | 157.0 | 9.1 | 0.51 | Oxide | Trenton Canyon
181.4 | 201.2 | 19.8 | 5.49 | Oxide
including | 182.9 | 189.0 | 6.1 | 9.78 | Oxide
including | 192.0 | 198.1 | 6.1 | 6.07 | Oxide
MRA7588 | 198.1 | 204.2 | 6.1 | 0.98 | Oxide | New Millennium
MRA7591 | 195.1 | 198.1 | 3.0 | 0.56 | Oxide | Trenton Canyon
202.7 | 207.3 | 4.6 | 2.36 | Sulfide
277.4 | 286.5 | 9.1 | 1.78 | Sulfide
MR7592 | 0.0 | 10.7 | 10.7 | 1.04 | Mixed | Mackay
DDH7592 | 112.0 | 116.6 | 4.6 | 0.40 | Oxide | Buffalo Valley
MR7593 | 134.1 | 137.2 | 3.0 | 0.85 | Oxide | Buffalo Valley
300.2 | 304.8 | 4.6 | 1.55 | Oxide
304.8 | 307.8 | 3.0 | 1.75 | Mixed
315.5 | 318.5 | 3.0 | 0.73 | Oxide
382.5 | 385.6 | 3.0 | 0.57 | Oxide
MR7594 | 239.3 | 249.9 | 10.7 | 0.63 | Oxide | Buffalo Valley
275.8 | 281.9 | 6.1 | 1.13 | Oxide
MR7595 | 295.7 | 304.8 | 9.1 | 0.57 | Oxide | Buffalo Valley
345.9 | 353.6 | 7.6 | 0.53 | Oxide
MRA7596 | 397.8 | 400.8 | 3.0 | 1.94 | Oxide | Buffalo Valley
MRA7597 | 301.8 | 329.2 | 27.4 | 0.74 | Oxide | Buffalo Valley
384.0 | 387.1 | 3.0 | 0.64 | Oxide
MRA7598 | 324.6 | 330.7 | 6.1 | 2.54 | Oxide | Buffalo Valley
330.7 | 336.8 | 6.1 | 5.03 | Sulfide
336.8 | 350.5 | 13.7 | 0.92 | Oxide
353.6 | 394.7 | 41.1 | 0.87 | Oxide
411.5 | 425.2 | 13.7 | 0.51 | Oxide
MRA7599 | 251.5 | 257.6 | 6.1 | 0.42 | Oxide | Buffalo Valley
339.9 | 342.9 | 3.0 | 1.22 | Mixed
DDH7600 | 215.0 | 218.7 | 3.7 | 1.69 | Sulfide | Buffalo Valley
240.8 | 243.8 | 3.0 | 0.60 | Oxide
292.8 | 299.6 | 6.9 | 1.99 | Sulfide
MRA7601 | 242.3 | 253.0 | 10.7 | 0.35 | Oxide | Buffalo Valley
289.6 | 294.1 | 4.6 | 2.20 | Sulfide
MRA7602 | NSI | Buffalo Valley
MR7603 | 163.1 | 166.1 | 3.0 | 0.41 | Oxide | New Millennium
216.4 | 219.5 | 3.0 | 0.54 | Oxide
MR7604 | 178.3 | 181.4 | 3.0 | 0.80 | Oxide | Buffalo Valley
185.9 | 196.6 | 10.7 | 0.83 | Oxide
MRA7605 | 149.4 | 152.4 | 3.0 | 0.78 | Oxide | Buffalo Valley
228.6 | 231.6 | 3.0 | 0.67 | Oxide
MRA7606 | NSI | Buffalo Valley

SSR Mining Inc. |  | PAGE 16

Hole ID | From (m) | To (m) | Interval (m) | Grade (g/t Au) | Oxidation State | Area
MRA7607 | 93.0 | 99.1 | 6.1 | 0.47 | Oxide | New Millennium
248.4 | 253.0 | 4.6 | 1.26 | Oxide
262.1 | 265.2 | 3.0 | 0.38 | Oxide
291.1 | 297.2 | 6.1 | 1.07 | Oxide
MRA7608 | NSI | Buffalo Valley
MRA7609 | 111.3 | 117.3 | 6.1 | 20.11 | Sulfide | Buffalo Valley
158.5 | 161.5 | 3.0 | 0.41 | Oxide
185.9 | 192.0 | 6.1 | 0.50 | Oxide
MRA7610 | 260.6 | 263.7 | 3.0 | 0.49 | Oxide | Buffalo Valley
312.4 | 315.5 | 3.0 | 7.59 | Oxide
326.1 | 329.2 | 3.0 | 1.69 | Sulfide
329.2 | 341.4 | 12.2 | 2.18 | Oxide
including | 333.8 | 336.8 | 3.0 | 7.10 | Oxide
MRA7611 | NSI | Buffalo Valley
MRA7613 | NSI | Buffalo Valley
MR7614 | 362.7 | 368.8 | 6.1 | 1.43 | Sulfide | Mackay
MRA7615 | 178.3 | 196.6 | 18.3 | 1.58 | Oxide | New Millennium
including | 190.5 | 193.5 | 3.0 | 3.75 | Oxide
| 288.0 | 291.1 | 3.0 | 0.92 | Oxide
MR7616 | 313.9 | 324.6 | 10.7 | 1.84 | Oxide | Mackay
including | 317.0 | 320.0 | 3.0 | 4.75 | Oxide
| 329.2 | 335.3 | 6.1 | 0.64 | Oxide
MRA7617 | NSI | Buffalo Valley
MRA7618 | NSI | Buffalo Valley
MRA7619 | 182.9 | 185.9 | 3.0 | 0.49 | Oxide | New Millennium
MRA7621 | 117.3 | 143.3 | 25.9 | 4.20 | Oxide | New Millennium
including | 123.4 | 137.2 | 13.7 | 6.84 | Oxide
| 157.0 | 166.1 | 9.1 | 0.58 | Oxide
175.3 | 178.3 | 3.0 | 0.42 | Oxide
MRA7622 | NSI | Buffalo Valley
MRA7623 | 120.4 | 137.2 | 16.8 | 2.67 | Oxide | New Millennium
including | 125.0 | 129.5 | 4.6 | 5.14 | Oxide
| 185.9 | 190.5 | 4.6 | 0.42 | Oxide
204.2 | 207.3 | 3.0 | 0.39 | Oxide
222.5 | 228.6 | 6.1 | 0.96 | Oxide
239.3 | 242.3 | 3.0 | 0.74 | Oxide
MRA7624 | 120.4 | 155.4 | 35.1 | 0.84 | Oxide | New Millennium
163.1 | 167.6 | 4.6 | 0.96 | Oxide
MR7625 | 163.1 | 166.1 | 3.0 | 0.47 | Oxide | New Millennium
208.8 | 214.9 | 6.1 | 0.41 | Oxide
253.0 | 274.3 | 21.3 | 0.85 | Oxide
298.7 | 306.3 | 7.6 | 0.88 | Oxide
327.7 | 332.2 | 4.6 | 0.44 | Oxide
MR7626 | 149.4 | 158.5 | 9.1 | 0.49 | Oxide | New Millennium
198.1 | 239.3 | 41.1 | 0.91 | Oxide
MR7627 | 201.2 | 207.3 | 6.1 | 0.55 | Oxide | New Millennium

SSR Mining Inc. |  | PAGE 17

Hole ID | From (m) | To (m) | Interval (m) | Grade (g/t Au) | Oxidation State | Area
MRA7628 | 221.0 | 245.4 | 24.4 | 1.40 | Oxide | New Millennium
266.7 | 269.7 | 3.0 | 0.40 | Oxide
MRA7629 | 158.5 | 163.1 | 4.6 | 0.44 | Oxide | New Millennium
221.0 | 227.1 | 6.1 | 0.64 | Oxide
231.6 | 254.5 | 22.9 | 1.72 | Oxide
MRA7630 | 211.8 | 216.4 | 4.6 | 0.76 | Oxide | New Millennium
222.5 | 242.3 | 19.8 | 1.58 | Oxide
including | 231.6 | 236.2 | 4.6 | 3.71 | Oxide
| 291.1 | 295.7 | 4.6 | 0.41 | Oxide
MRA7631 | 201.2 | 204.2 | 3.0 | 0.58 | Oxide | New Millennium
227.1 | 237.7 | 10.7 | 1.09 | Oxide
MRA7633 | 138.7 | 146.3 | 7.6 | 0.67 | Oxide | New Millennium
150.9 | 160.0 | 9.1 | 0.97 | Oxide
MR7634 | 390.1 | 393.2 | 3.0 | 1.41 | Sulfide | Mackay
414.5 | 417.6 | 3.0 | 0.62 | Oxide
451.1 | 454.2 | 3.0 | 0.88 | Oxide
MRA7635 | 164.6 | 181.4 | 16.8 | 1.02 | Oxide | New Millennium
207.3 | 221.0 | 13.7 | 0.49 | Oxide
MRA7636 | 189.0 | 204.2 | 15.2 | 0.70 | Oxide | New Millennium
355.1 | 359.7 | 4.6 | 0.92 | Oxide
MRA7637 | 234.7 | 239.3 | 4.6 | 0.75 | Oxide | New Millennium
MRA7638 | 178.3 | 181.4 | 3.0 | 0.42 | Oxide | New Millennium
198.1 | 201.2 | 3.0 | 0.69 | Oxide
228.6 | 231.6 | 3.0 | 0.43 | Oxide
MR7639 | 210.3 | 217.9 | 7.6 | 0.66 | Oxide | New Millennium
MRA7641 | 198.1 | 201.2 | 3.0 | 0.35 | Oxide | New Millennium
MRA7642 | NSI | New Millennium
MRA7643 | NSI | New Millennium
MRA7644 | 246.9 | 271.3 | 24.4 | 1.06 | Oxide | New Millennium
MRA7645 | 175.3 | 181.4 | 6.1 | 0.73 | Oxide | New Millennium
195.1 | 202.7 | 7.6 | 2.24 | Oxide
including | 199.6 | 202.7 | 3.0 | 3.88 | Oxide
| 213.4 | 217.9 | 4.6 | 0.42 | Oxide
MR7646 | 410.0 | 413.0 | 3.0 | 0.49 | Oxide | Mackay
MRA7647 | NSI | Buffalo Valley
MRA7648 | 100.6 | 114.3 | 13.7 | 0.48 | Oxide | New Millennium
MRA7649 | 269.7 | 272.8 | 3.0 | 0.58 | Oxide | New Millennium
MRA7650 | 117.3 | 126.5 | 9.1 | 0.45 | Oxide | New Millennium
158.5 | 164.6 | 6.1 | 1.43 | Oxide
228.6 | 233.2 | 4.6 | 0.63 | Oxide
257.6 | 263.7 | 6.1 | 1.06 | Oxide
263.7 | 269.7 | 6.1 | 8.97 | Mixed
including | 265.2 | 268.2 | 3.0 | 15.82 | Mixed
MRA7651 | 118.9 | 126.5 | 7.6 | 0.64 | Oxide | New Millennium
214.9 | 222.5 | 7.6 | 1.53 | Oxide
MRA7652 | 253.0 | 257.6 | 4.6 | 0.50 | Oxide | Buffalo Valley
MR7653 | 184.4 | 193.5 | 9.1 | 1.20 | Oxide | New Millennium

SSR Mining Inc. |  | PAGE 18

Hole ID | From (m) | To (m) | Interval (m) | Grade (g/t Au) | Oxidation State | Area
MRA7654 | 224.0 | 227.1 | 3.0 | 0.45 | Oxide | New Millennium
327.7 | 330.7 | 3.0 | 0.93 | Oxide
MRA7655 | NSI | New Millennium
MRA7656 | NSI | New Millennium
MRA7657 | 219.5 | 224.0 | 4.6 | 0.45 | Oxide | New Millennium
MRA7658 | NSI | New Millennium
MRA7659 | 204.2 | 207.3 | 3.0 | 0.41 | Oxide | New Millennium
216.4 | 219.5 | 3.0 | 0.43 | Oxide
228.6 | 236.2 | 7.6 | 0.58 | Oxide
272.8 | 277.4 | 4.6 | 1.12 | Oxide
MRA7660 | 131.1 | 147.8 | 16.8 | 0.40 | Oxide | New Millennium
170.7 | 176.8 | 6.1 | 0.56 | Oxide
182.9 | 187.5 | 4.6 | 0.40 | Oxide
MRA7661 | 117.3 | 120.4 | 3.0 | 0.40 | Oxide | New Millennium
147.8 | 153.9 | 6.1 | 0.46 | Oxide
158.5 | 172.2 | 13.7 | 1.33 | Oxide
227.1 | 231.6 | 4.6 | 1.17 | Oxide
236.2 | 239.3 | 3.0 | 1.04 | Oxide
MRA7662 | NSI | New Millennium
MRA7663 | NSI | New Millennium
MRA7664 | NSI | Buffalo Valley
MR7665 | 189.0 | 195.1 | 6.1 | 0.45 | Oxide | Mackay
298.7 | 303.3 | 4.6 | 2.13 | Sulfide
MRA7666 | 169.2 | 172.2 | 3.0 | 0.52 | Oxide | New Millennium
175.3 | 181.4 | 6.1 | 0.46 | Oxide
MRA7667 | NSI | New Millennium
MRA7668 | 182.9 | 189.0 | 6.1 | 0.46 | Oxide | New Millennium
MR7669 | 292.6 | 295.7 | 3.0 | 1.33 | Oxide | New Millennium
MRA7670 | 198.1 | 201.2 | 3.0 | 0.88 | Oxide | Buffalo Valley
204.2 | 207.3 | 3.0 | 0.45 | Oxide
219.5 | 222.5 | 3.0 | 0.55 | Oxide
231.6 | 234.7 | 3.0 | 0.37 | Oxide
254.5 | 257.6 | 3.0 | 1.01 | Oxide
257.6 | 266.7 | 9.1 | 1.43 | Sulfide
266.7 | 277.4 | 10.7 | 0.74 | Oxide
417.6 | 420.6 | 3.0 | 6.21 | Mixed
MRA7671 | 172.2 | 187.5 | 15.2 | 0.67 | Oxide | New Millennium
193.5 | 216.4 | 22.9 | 0.64 | Oxide
277.4 | 280.4 | 3.0 | 0.37 | Oxide
MRA7672 | 239.3 | 242.3 | 3.0 | 0.54 | Oxide | New Millennium
MRA7673 | 152.4 | 155.4 | 3.0 | 0.45 | Oxide | New Millennium
189.0 | 192.0 | 3.0 | 0.52 | Oxide
205.7 | 210.3 | 4.6 | 0.56 | Oxide
242.3 | 246.9 | 4.6 | 0.39 | Oxide

SSR Mining Inc. |  | PAGE 19

Hole ID | From (m) | To (m) | Interval (m) | Grade (g/t Au) | Oxidation State | Area
MRA7674 | 106.7 | 118.9 | 12.2 | 0.56 | Oxide | New Millennium
137.2 | 140.2 | 3.0 | 0.52 | Oxide
144.8 | 149.4 | 4.6 | 0.85 | Oxide
196.6 | 201.2 | 4.6 | 0.49 | Oxide
214.9 | 221.0 | 6.1 | 0.44 | Oxide
227.1 | 234.7 | 7.6 | 0.34 | Oxide
249.9 | 257.6 | 7.6 | 0.48 | Oxide
MRA7675 | 135.6 | 166.1 | 30.5 | 0.58 | Oxide | New Millennium
271.3 | 274.3 | 3.0 | 0.59 | Oxide
184.4 | 189.0 | 4.6 | 0.33 | Oxide
MRA7676 | 196.6 | 199.6 | 3.0 | 0.38 | Oxide | New Millennium
349.0 | 353.6 | 4.6 | 0.54 | Oxide
MRA7677 | 153.9 | 157.0 | 3.0 | 0.97 | Oxide | Buffalo Valley
275.8 | 280.4 | 4.6 | 0.46 | Oxide
MRA7678 | NSI | New Millennium
MRA7679 | 157.0 | 160.0 | 3.0 | 0.69 | Oxide | New Millennium
166.1 | 169.2 | 3.0 | 0.45 | Oxide
176.8 | 182.9 | 6.1 | 0.34 | Oxide
MRA7680 | NSI | New Millennium
MR7681 | 222.5 | 227.1 | 4.6 | 0.55 | Oxide | New Millennium
MR7682 | NSI | Mackay
MRA7683 | 117.3 | 120.4 | 3.0 | 0.51 | Oxide | New Millennium
187.5 | 192.0 | 4.6 | 0.76 | Oxide
222.5 | 234.7 | 12.2 | 0.70 | Oxide
MRA7684 | NSI | New Millennium
MRA7685 | 114.3 | 121.9 | 7.6 | 1.28 | Oxide | Buffalo Valley
150.9 | 166.1 | 15.2 | 0.51 | Oxide
312.4 | 315.5 | 3.0 | 0.88 | Oxide
327.7 | 330.7 | 3.0 | 0.43 | Oxide
MRA7686 | 96.0 | 109.7 | 13.7 | 0.62 | Oxide | New Millennium
120.4 | 132.6 | 12.2 | 0.79 | Oxide
135.6 | 140.2 | 4.6 | 0.50 | Oxide
155.4 | 158.5 | 3.0 | 0.36 | Oxide
166.1 | 179.8 | 13.7 | 0.77 | Oxide
190.5 | 201.2 | 10.7 | 0.49 | Oxide
208.8 | 240.8 | 32.0 | 0.48 | Oxide
MRA7687 | NSI | New Millennium
MRA7688 | NSI | New Millennium
MRA7689 | 117.3 | 120.4 | 3.0 | 1.48 | Oxide | New Millennium
199.6 | 202.7 | 3.0 | 0.75 | Oxide
MRA7690 | 207.3 | 214.9 | 7.6 | 0.43 | Oxide | New Millennium
230.1 | 236.2 | 6.1 | 0.35 | Oxide
MRA7691 | 125.0 | 131.1 | 6.1 | 0.76 | Oxide | New Millennium
134.1 | 137.2 | 3.0 | 0.56 | Oxide
166.1 | 175.3 | 9.1 | 0.40 | Oxide
MRA7692 | 137.2 | 140.2 | 3.0 | 0.32 | Oxide | New Millennium
MRA7693 | NSI | New Millennium

SSR Mining Inc. |  | PAGE 20

Hole ID | From (m) | To (m) | Interval (m) | Grade (g/t Au) | Oxidation State | Area
MR7694 | 350.5 | 359.7 | 9.1 | 1.24 | Oxide | Mackay
MRA7695 | 129.5 | 132.6 | 3.0 | 0.76 | Oxide | New Millennium
125.0 | 129.5 | 4.6 | 3.91 | Mixed
306.3 | 309.4 | 3.0 | 0.66 | Oxide
MRA7696 | 125.0 | 134.1 | 9.1 | 2.45 | Sulfide | New Millennium
306.3 | 309.4 | 3.0 | 0.66 | Oxide
MRA7697 | 112.8 | 143.3 | 30.5 | 0.74 | Oxide | New Millennium
MRA7698 | 68.6 | 77.7 | 9.1 | 0.73 | Oxide | New Millennium
208.8 | 211.8 | 3.0 | 0.50 | Oxide
225.6 | 230.1 | 4.6 | 0.48 | Oxide
MRA7699 | 44.2 | 59.4 | 15.2 | 0.64 | Oxide | New Millennium
MRA7700 | 274.3 | 280.4 | 6.1 | 0.83 | Oxide | Buffalo Valley
MRA7701 | NSI | New Millennium
MRA7702 | 259.1 | 262.1 | 3.0 | 2.69 | Sulfide | Trenton Canyon
MRA7703 | 259.1 | 269.7 | 10.7 | 3.20 | Sulfide | Trenton Canyon
including | 260.6 | 263.7 | 3.0 | 5.53 | Sulfide
| 266.7 | 269.7 | 3.0 | 4.49 | Sulfide
MRA7704 | 44.2 | 50.3 | 6.1 | 0.58 | Oxide | New Millennium
56.4 | 61.0 | 4.6 | 0.52 | Oxide
99.1 | 103.6 | 4.6 | 0.60 | Oxide
DDH7705 | 126.5 | 144.8 | 18.3 | 6.20 | Oxide | Buffalo Valley
including | 127.3 | 132.6 | 5.3 | 13.95 | Oxide
including | 135.6 | 138.8 | 3.2 | 4.84 | Oxide
| 156.7 | 161.4 | 4.8 | 1.40 | Oxide
166.1 | 171.9 | 5.9 | 0.36 | Oxide
179.2 | 183.3 | 4.1 | 0.49 | Oxide
MRA7706 | NSI | New Millennium
MRA7707 | 67.1 | 70.1 | 3.0 | 1.09 | Oxide | New Millennium
MRA7708 | 172.2 | 184.4 | 12.2 | 3.89 | Sulfide | Trenton Canyon
including | 176.8 | 181.4 | 4.6 | 6.93 | Sulfide
| 184.4 | 187.5 | 3.0 | 4.12 | Oxide
192.0 | 195.1 | 3.0 | 1.89 | Oxide
275.8 | 280.4 | 4.6 | 2.06 | Sulfide
MRA7709 | NSI | New Millennium
MRA7710 | 80.8 | 86.9 | 6.1 | 0.67 | Oxide | New Millennium
91.4 | 100.6 | 9.1 | 1.04 | Oxide
111.3 | 115.8 | 4.6 | 0.59 | Oxide
196.6 | 202.7 | 6.1 | 0.67 | Oxide
MRA7711 | 157.0 | 190.5 | 33.5 | 0.48 | Oxide | Buffalo Valley
216.4 | 219.5 | 3.0 | 0.40 | Oxide
MRA7712 | NSI | New Millennium
MRA7714 | NSI | New Millennium
MRA7715 | 370.3 | 376.4 | 6.1 | 0.77 | Oxide | Buffalo Valley
384.0 | 396.2 | 12.2 | 0.62 | Oxide
400.8 | 403.9 | 3.0 | 2.81 | Sulfide
MRA7716 | NSI | New Millennium

SSR Mining Inc. |  | PAGE 21

Hole ID | From (m) | To (m) | Interval (m) | Grade (g/t Au) | Oxidation State | Area
MRA7717 | 32.0 | 35.1 | 3.0 | 0.42 | Oxide | New Millennium
259.1 | 263.7 | 4.6 | 2.13 | Oxide
MRA7718 | 176.8 | 184.4 | 7.6 | 0.92 | Oxide | Mackay
195.1 | 204.2 | 9.1 | 0.79 | Oxide
271.3 | 274.3 | 3.0 | 0.80 | Oxide
MRA7719 | 91.4 | 96.0 | 4.6 | 0.74 | Oxide | Mackay
103.6 | 108.2 | 4.6 | 0.47 | Oxide
114.3 | 118.9 | 4.6 | 0.49 | Oxide
213.4 | 216.4 | 3.0 | 0.39 | Oxide
221.0 | 234.7 | 13.7 | 0.67 | Oxide
285.0 | 288.0 | 3.0 | 1.06 | Oxide
MRA7720 | 259.1 | 265.2 | 6.1 | 0.42 | Oxide | New Millennium
MRA7722 | 185.9 | 198.1 | 12.2 | 1.42 | Oxide | Mackay
201.2 | 208.8 | 7.6 | 0.51 | Oxide
225.6 | 231.6 | 6.1 | 0.56 | Oxide
MRA7723 | 121.9 | 125.0 | 3.0 | 0.96 | Oxide | Mackay
128.0 | 132.6 | 4.6 | 2.52 | Oxide
147.8 | 155.4 | 7.6 | 1.30 | Oxide
173.7 | 185.9 | 12.2 | 0.79 | Oxide
MRA7724 | 105.2 | 109.7 | 4.6 | 0.43 | Oxide | Mackay
138.7 | 149.4 | 10.7 | 0.85 | Oxide
161.5 | 173.7 | 12.2 | 1.06 | Oxide
MRA7725 | 132.6 | 143.3 | 10.7 | 0.50 | Oxide | New Millennium
196.6 | 208.8 | 12.2 | 0.55 | Oxide
MRA7726 | 132.6 | 146.3 | 13.7 | 1.65 | Oxide | Mackay
including | 138.7 | 141.7 | 3.0 | 4.14 | Oxide
| 149.4 | 157.0 | 7.6 | 0.65 | Oxide
160.0 | 163.1 | 3.0 | 0.47 | Oxide
167.6 | 173.7 | 6.1 | 0.34 | Oxide
176.8 | 187.5 | 10.7 | 0.63 | Oxide
MRA7727 | 137.2 | 140.2 | 3.0 | 1.15 | Oxide | Mackay
143.3 | 153.9 | 10.7 | 2.68 | Oxide
including | 144.8 | 149.4 | 4.6 | 5.28 | Oxide
| 166.1 | 169.2 | 3.0 | 0.45 | Oxide
MRA7728 | 193.5 | 202.7 | 9.1 | 0.69 | Oxide | Mackay
278.9 | 288.0 | 9.1 | 1.47 | Oxide
318.5 | 321.6 | 3.0 | 1.81 | Sulfide
MRA7729 | 228.6 | 237.7 | 9.1 | 0.64 | Oxide | Mackay
MRA7730 | 285.0 | 292.6 | 7.6 | 0.37 | Oxide | Buffalo Valley
356.6 | 359.7 | 3.0 | 0.46 | Oxide
382.5 | 425.2 | 42.7 | 1.41 | Oxide
MRA7731 | 190.5 | 199.6 | 9.1 | 1.03 | Oxide | Mackay
324.6 | 332.2 | 7.6 | 0.47 | Oxide
MRA7732 | NSI | Mackay
MRA7733 | NSI | Mackay
MRA7734 | 249.9 | 254.5 | 4.6 | 0.39 | Oxide | Mackay

SSR Mining Inc. |  | PAGE 22

Hole ID | From (m) | To (m) | Interval (m) | Grade (g/t Au) | Oxidation State | Area
MRA7735 | 41.1 | 54.9 | 13.7 | 0.39 | Oxide | New Millennium
211.8 | 214.9 | 3.0 | 0.74 | Oxide
MRA7736 | 65.5 | 68.6 | 3.0 | 1.54 | Oxide | New Millennium
74.7 | 77.7 | 3.0 | 0.35 | Oxide
MRA7737 | 178.3 | 190.5 | 12.2 | 0.94 | Oxide | Mackay
195.1 | 219.5 | 24.4 | 1.61 | Oxide
including | 204.2 | 208.8 | 4.6 | 3.83 | Oxide
MRA7738 | NSI | New Millennium
MRA7739 | NSI | New Millennium
MRA7740 | 76.2 | 88.4 | 12.2 | 1.51 | Oxide | New Millennium
including | 77.7 | 80.8 | 3.0 | 3.48 | Oxide
| 93.0 | 96.0 | 3.0 | 1.00 | Oxide
MRA7741 | 115.8 | 144.8 | 29.0 | 0.96 | Oxide | New Millennium
MRA7742 | 225.6 | 231.6 | 6.1 | 0.49 | Oxide | Mackay
MRA7743 | NSI | New Millennium
MRA7744 | 83.8 | 99.1 | 15.2 | 0.57 | Oxide | New Millennium
MRA7745 | 152.4 | 164.6 | 12.2 | 1.04 | Oxide | Mackay
167.6 | 172.2 | 4.6 | 1.08 | Oxide
MRA7746 | 109.7 | 123.4 | 13.7 | 0.90 | Oxide | New Millennium
132.6 | 135.6 | 3.0 | 0.50 | Oxide
MRA7747 | NSI | New Millennium
MRA7748 | NSI | New Millennium
MRA7749 | 146.3 | 157.0 | 10.7 | 0.43 | Oxide | Mackay
251.5 | 265.2 | 13.7 | 0.39 | Oxide
283.5 | 288.0 | 4.6 | 0.89 | Oxide
MR7750 | 248.4 | 253.0 | 4.6 | 0.40 | Oxide | Mackay
256.0 | 260.6 | 4.6 | 0.85 | Oxide
265.2 | 278.9 | 13.7 | 0.69 | Oxide
368.8 | 373.4 | 4.6 | 1.10 | Oxide
MRA7751 | 25.9 | 47.2 | 21.3 | 1.23 | Oxide | Mackay
93.0 | 96.0 | 3.0 | 0.92 | Oxide
234.7 | 245.4 | 10.7 | 0.83 | Oxide
MRA7752 | 291.1 | 295.7 | 4.6 | 0.38 | Oxide | Mackay
MRA7753 | 111.3 | 125.0 | 13.7 | 1.48 | Oxide | Mackay
240.8 | 249.9 | 9.1 | 0.50 | Oxide
MRA7754 | 143.3 | 146.3 | 3.0 | 0.59 | Oxide | Mackay
149.4 | 173.7 | 24.4 | 1.20 | Oxide
MRA7755 | 70.1 | 74.7 | 4.6 | 0.56 | Oxide | New Millennium
83.8 | 93.0 | 9.1 | 0.77 | Oxide
108.2 | 129.5 | 21.3 | 1.43 | Oxide
including | 117.3 | 120.4 | 3.0 | 3.83 | Oxide
| 158.5 | 161.5 | 3.0 | 0.46 | Oxide
MRA7756 | 141.7 | 150.9 | 9.1 | 0.68 | Oxide | Mackay
155.4 | 169.2 | 13.7 | 0.71 | Oxide
178.3 | 189.0 | 10.7 | 1.06 | Oxide

SSR Mining Inc. |  | PAGE 23

Hole ID | From (m) | To (m) | Interval (m) | Grade (g/t Au) | Oxidation State | Area
MRA7757 | 106.7 | 109.7 | 3.0 | 0.64 | Oxide | New Millennium
140.2 | 150.9 | 10.7 | 2.16 | Oxide
including | 143.3 | 147.8 | 4.6 | 3.45 | Oxide
MRA7758 | 161.5 | 164.6 | 3.0 | 0.38 | Oxide | New Millennium
MRA7759 | 157.0 | 160.0 | 3.0 | 0.73 | Oxide | Mackay
164.6 | 192.0 | 27.4 | 0.71 | Oxide
MRA7760 | 126.5 | 132.6 | 6.1 | 0.31 | Oxide | New Millennium
135.6 | 152.4 | 16.8 | 1.05 | Oxide
MRA7761 | 295.7 | 300.2 | 4.6 | 0.33 | Oxide | New Millennium
MRA7762 | 4.6 | 9.1 | 4.6 | 1.07 | Oxide | Mackay
74.7 | 77.7 | 3.0 | 0.73 | Oxide
150.9 | 182.9 | 32.0 | 0.77 | Oxide
DDH7763 | 275.4 | 280.2 | 4.8 | 4.17 | Sulfide | Trenton Canyon
379.8 | 385.6 | 5.8 | 1.08 | Sulfide
MRA7763 | NSI | Mackay
MRA7764 | NSI | Valmy
MR7765 | 217.9 | 225.6 | 7.6 | 1.39 | Oxide | Mackay
MRA7766 | NSI | Valmy
MRA7767 | 158.5 | 163.1 | 4.6 | 0.36 | Oxide | Valmy
MRA7768 | 106.7 | 109.7 | 3.0 | 0.59 | Oxide | Trenton Canyon
114.3 | 120.4 | 6.1 | 0.73 | Oxide
123.4 | 126.5 | 3.0 | 2.09 | Oxide
MRA7769 | 222.5 | 237.7 | 15.2 | 0.86 | Oxide | New Millennium
MRA7770 | 74.7 | 77.7 | 3.0 | 0.36 | Oxide | New Millennium
89.9 | 99.1 | 9.1 | 1.45 | Oxide
117.3 | 120.4 | 3.0 | 0.47 | Oxide
MRA7771 | 146.3 | 149.4 | 3.0 | 0.69 | Oxide | New Millennium
152.4 | 158.5 | 6.1 | 0.80 | Oxide
249.9 | 257.6 | 7.6 | 0.42 | Oxide
MRA7772 | 42.7 | 45.7 | 3.0 | 3.32 | Sulfide | Trenton Canyon
62.5 | 70.1 | 7.6 | 1.11 | Oxide
74.7 | 83.8 | 9.1 | 1.38 | Oxide
97.5 | 100.6 | 3.0 | 0.92 | Oxide
137.2 | 140.2 | 3.0 | 1.04 | Oxide
MRA7773 | NSI | New Millennium
MRA7774 | NSI | New Millennium
MRA7775 | 158.5 | 161.5 | 3.0 | 0.46 | Oxide | New Millennium
MRA7776 | 47.2 | 51.8 | 4.6 | 4.39 | Oxide | Trenton Canyon
86.9 | 100.6 | 13.7 | 2.03 | Oxide
including | 88.4 | 93.0 | 4.6 | 4.51 | Oxide
| 103.6 | 118.9 | 15.2 | 1.78 | Oxide
| 123.4 | 126.5 | 3.0 | 0.90 | Oxide
MRA7777 | 166.1 | 172.2 | 6.1 | 1.84 | Mixed | Trenton Canyon
MRA7778 | 166.1 | 198.1 | 32.0 | 0.76 | Oxide | New Millennium
245.4 | 248.4 | 3.0 | 0.54 | Oxide
MRA7779 | 140.2 | 147.8 | 7.6 | 0.56 | Oxide | New Millennium
MRA7780 | 71.6 | 74.7 | 3.0 | 0.46 | Oxide | Trenton Canyon

SSR Mining Inc. |  | PAGE 24

Hole ID | From (m) | To (m) | Interval (m) | Grade (g/t Au) | Oxidation State | Area
MRA7781 | 25.9 | 32.0 | 6.1 | 1.11 | Oxide | Trenton Canyon
MRA7782 | 211.8 | 214.9 | 3.0 | 1.30 | Mixed | Trenton Canyon
242.3 | 246.9 | 4.6 | 0.56 | Oxide
323.1 | 327.7 | 4.6 | 2.28 | Sulfide
MRA7783 | 13.7 | 16.8 | 3.0 | 0.42 | Oxide | Trenton Canyon
MRA7786 | 64.0 | 73.2 | 9.1 | 0.48 | Oxide | New Millennium
83.8 | 88.4 | 4.6 | 1.57 | Oxide
MRA7787 | NSI | New Millennium
MRA7788 | 86.9 | 91.4 | 4.6 | 0.83 | Oxide | New Millennium
MRA7789 | 129.5 | 135.6 | 6.1 | 0.49 | Oxide | New Millennium
MRA7791 | NSI | New Millennium
MRA7792 | 74.7 | 80.8 | 6.1 | 1.06 | Oxide | New Millennium
105.2 | 108.2 | 3.0 | 1.01 | Oxide
MRA7793 | 272.8 | 275.8 | 3.0 | 1.16 | Sulfide | Trenton Canyon
MRA7795 | 9.1 | 12.2 | 3.0 | 0.44 | Oxide | Trenton Canyon
213.4 | 228.6 | 15.2 | 11.06 | Oxide
including | 213.4 | 222.5 | 9.1 | 17.05 | Oxide
| 228.6 | 233.2 | 4.6 | 1.54 | Sulfide
MRA7796 | NSI | Trenton Canyon
MRA7797 | 144.8 | 152.4 | 7.6 | 0.85 | Oxide | Mackay
MRA7799 | 29.0 | 38.1 | 9.1 | 0.94 | Oxide | Mackay
51.8 | 54.9 | 3.0 | 0.35 | Oxide
86.9 | 89.9 | 3.0 | 1.18 | Oxide
MRA7800 | NSI | Mackay
MRA7801 | NSI | Mackay
MRA7802 | 24.4 | 27.4 | 3.0 | 3.23 | Sulfide | Mackay
MRA7803 | 15.2 | 18.3 | 3.0 | 2.38 | Oxide | Mackay
MRA7804 | 224.0 | 240.8 | 16.8 | 1.10 | Oxide | Trenton Canyon
246.9 | 253.0 | 6.1 | 0.81 | Oxide
MRA7805 | 57.9 | 67.1 | 9.1 | 1.09 | Oxide | Mackay
88.4 | 96.0 | 7.6 | 2.86 | Oxide
MRA7806 | 57.9 | 64.0 | 6.1 | 0.61 | Oxide | Mackay
MRA7807 | NSI | Mackay
MRA7808 | NSI | Mackay
MRA7809 | 219.5 | 224.0 | 4.6 | 4.29 | Sulfide | Trenton Canyon
including | 219.5 | 222.5 | 3.0 | 5.11 | Sulfide
| 356.6 | 362.7 | 6.1 | 1.16 | Sulfide
MRA7814 | 157.0 | 161.5 | 4.6 | 0.77 | Oxide | Trenton Canyon
164.6 | 169.2 | 4.6 | 0.55 | Oxide
179.8 | 185.9 | 6.1 | 2.26 | Oxide
including | 179.8 | 182.9 | 3.0 | 3.75 | Oxide
MRA7817 | 19.8 | 22.9 | 3.0 | 0.58 | Oxide | Trenton Canyon
125.0 | 128.0 | 3.0 | 0.56 | Oxide
131.1 | 138.7 | 7.6 | 1.70 | Oxide
193.5 | 196.6 | 3.0 | 0.51 | Oxide
219.5 | 230.1 | 10.7 | 4.08 | Oxide
including | 221.0 | 225.6 | 4.6 | 8.28 | Oxide

SSR Mining Inc. |  | PAGE 25

Hole ID | From (m) | To (m) | Interval (m) | Grade (g/t Au) | Oxidation State | Area
MRA7819 | 103.6 | 108.2 | 4.6 | 0.52 | Oxide | Trenton Canyon
126.5 | 129.5 | 3.0 | 3.35 | Oxide
138.7 | 141.7 | 3.0 | 1.14 | Oxide
147.8 | 150.9 | 3.0 | 0.93 | Oxide
MRA7820 | 144.8 | 147.8 | 3.0 | 1.21 | Oxide | Trenton Canyon
MRA7821 | 222.5 | 227.1 | 4.6 | 0.61 | Oxide | New Millennium
MRA7822 | NSI | Trenton Canyon
MRA7823 | 138.7 | 141.7 | 3.0 | 1.16 | Sulfide | Trenton Canyon
144.8 | 149.4 | 4.6 | 1.12 | Oxide
MRA7824 | 45.7 | 50.3 | 4.6 | 1.23 | Oxide | Mackay
61.0 | 70.1 | 9.1 | 1.56 | Oxide
MRA7840 | 362.7 | 385.6 | 22.9 | 4.44 | Sulfide | Trenton Canyon
including | 362.7 | 368.8 | 6.1 | 9.92 | Sulfide
MRA7842 | 149.4 | 155.4 | 6.1 | 0.34 | Oxide | Trenton Canyon
204.2 | 210.3 | 6.1 | 5.16 | Sulfide

Drill intervals reported at a nominal 0.3 g/t gold cut-off and with a maximum 2.5m contiguous dilution are given. All thicknesses are down hole length and true widths are not known at this stage. NSI – No significant intercept

SSR Mining Inc. |  | PAGE 26

Supporting Drilling Information to SSR Mining Announcement
This document provides supporting drill collar locations and composite assay results for the Marigold drilling program referenced in the announcement “SSR Mining Announces Positive Exploration Results at Marigold Creating Pathways for Mine Plan Enhancement and Extension”, November 28, 2022.
Drill collar locations are surveyed in UTM Zone 11, NAD27 grid using differential GPS in units of meters. The Hole ID prefix DDH is used for HQ (63.5 mm core diameter) and NQ (47.6 mm core diameter) core drilling, the MR and MRA prefixes designate reverse circulation drill holes.
Table 5: Drill Collar Coordinates

Hole ID | Easting | Northing | Elevation (m) | Azimuth (deg.) | Dip (deg.) | Length (m) | Area
MRA7231 | 484936 | 4502763 | 1814 | 90 | -70 | 367.3 | New Millennium
MRA7255 | 485611 | 4499108 | 2045 | 270 | -88 | 370.3 | Trenton Canyon
MRA7327 | 485562 | 4498429 | 2114 | 270 | -80 | 294.1 | Trenton Canyon
MR7370 | 485145 | 4502563 | 1833 | 90 | -90 | 373.4 | New Millennium
MRA7371 | 484801 | 4500114 | 1980 | 270 | -55 | 214.9 | Trenton Canyon
MRA7375 | 484728 | 4500332 | 1950 | 290 | -45 | 214.9 | Trenton Canyon
MRA7423 | 484750 | 4500364 | 1931 | 290 | -45 | 214.9 | Trenton Canyon
DDH7452 | 487362 | 4504349 | 1895 | 270 | -80 | 1101.1 | Valmy
MRA7469 | 484753 | 4502891 | 1757 | 270 | -70 | 367.3 | New Millennium
MRA7474 | 485047 | 4499444 | 2165 | 270 | -65 | 123.4 | Trenton Canyon
MRA7480 | 484967 | 4499469 | 2166 | 270 | -65 | 184.4 | Trenton Canyon
MR7484 | 484873 | 4508427 | 1565 | 0 | -90 | 493.8 | Mackay
MRA7495 | 485014 | 4502698 | 1832 | 90 | -70 | 367.3 | New Millennium
MR7500 | 485117 | 4506694 | 1627 | 0 | -90 | 560.8 | Mackay
MR7501 | 484125 | 4507505 | 1647 | 88 | -90 | 426.7 | Mackay
MR7502 | 484866 | 4508307 | 1569 | 0 | -90 | 493.8 | Mackay
MRA7503 | 484876 | 4502764 | 1796 | 88 | -73 | 367.3 | New Millennium
MRA7504 | 484874 | 4502641 | 1797 | 92 | -74 | 367.3 | New Millennium
MRA7505 | 484630 | 4499201 | 2379 | 270 | -45 | 336.8 | Trenton Canyon
MRA7506 | 484632 | 4499201 | 2379 | 270 | -65 | 336.8 | Trenton Canyon
MRA7507 | 484645 | 4499170 | 2385 | 270 | -80 | 367.3 | Trenton Canyon
MRA7508 | 484643 | 4499170 | 2385 | 270 | -60 | 336.8 | Trenton Canyon
MRA7509 | 484639 | 4499144 | 2389 | 270 | -60 | 367.3 | Trenton Canyon
MRA7510 | 484648 | 4499231 | 2371 | 270 | -65 | 367.3 | Trenton Canyon
MRA7511 | 485070 | 4502701 | 1837 | 90 | -70 | 367.3 | New Millennium
MRA7512 | 484940 | 4502700 | 1813 | 90 | -70 | 367.3 | New Millennium
MR7515 | 486097 | 4507214 | 1621 | 0 | -90 | 426.7 | Mackay
MRA7516 | 484921 | 4499089 | 2290 | 270 | -50 | 367.3 | Trenton Canyon
MRA7517 | 484773 | 4498954 | 2323 | 270 | -55 | 367.3 | Trenton Canyon
MRA7518 | 484915 | 4499142 | 2301 | 270 | -60 | 367.3 | Trenton Canyon
MRA7519 | 484747 | 4499015 | 2346 | 270 | -65 | 275.8 | Trenton Canyon
MRA7520 | 484838 | 4502459 | 1776 | 90 | -65 | 356.6 | New Millennium
MR7521 | 485123 | 4506591 | 1630 | 0 | -90 | 560.8 | Mackay
MRA7522 | 485466 | 4503050 | 1827 | 90 | -70 | 341.4 | New Millennium
MRA7523 | 484776 | 4500265 | 1962 | 270 | -45 | 214.9 | Trenton Canyon
MRA7524 | 484899 | 4502368 | 1787 | 90 | -55 | 349 | New Millennium
DDH7525 | 484642 | 4499560 | 2261 | 270 | -63 | 547.4 | Trenton Canyon
MRA7526 | 485076 | 4499308 | 2175 | 16 | -55 | 245.4 | Trenton Canyon

SSR Mining Inc. |  | PAGE 27

Hole ID | Easting | Northing | Elevation (m) | Azimuth (deg.) | Dip (deg.) | Length (m) | Area
MRA7527 | 485076 | 4499308 | 2175 | 16 | -65 | 245.4 | Trenton Canyon
MRA7528 | 485207 | 4499234 | 2178 | 275 | -65 | 458.7 | Trenton Canyon
MRA7529 | 485215 | 4499231 | 2178 | 16 | -65 | 275.8 | Trenton Canyon
MRA7530 | 485216 | 4499231 | 2178 | 16 | -55 | 275.8 | Trenton Canyon
DDH7531 | 484643 | 4498943 | 2392 | 25 | -72 | 370.9 | Trenton Canyon
MRA7532 | 484987 | 4499427 | 2192 | 16 | -35 | 138.7 | Trenton Canyon
MR7533 | 485668 | 4502339 | 1857 | 0 | -90 | 268.2 | New Millennium
MR7534 | 485185 | 4502564 | 1837 | 90 | -90 | 356.6 | New Millennium
MRA7535 | 485294 | 4499283 | 2127 | 16 | -85 | 245.4 | Trenton Canyon
MRA7536 | 485294 | 4499284 | 2127 | 16 | -55 | 245.4 | Trenton Canyon
MR7537 | 485106 | 4502561 | 1829 | 90 | -90 | 373.4 | New Millennium
MRA7538 | 485163 | 4499258 | 2177 | 270 | -65 | 458.7 | Trenton Canyon
MRA7539 | 484729 | 4499717 | 2162 | 270 | -65 | 367.3 | Trenton Canyon
MRA7540 | 484676 | 4499506 | 2263 | 270 | -85 | 382.5 | Trenton Canyon
MRA7541 | 485156 | 4502779 | 1821 | 90 | -70 | 306.3 | New Millennium
MRA7542 | 485319 | 4502746 | 1810 | 90 | -65 | 349 | New Millennium
MRA7545 | 485438 | 4502749 | 1810 | 90 | -55 | 275.8 | New Millennium
MRA7546 | 485382 | 4502748 | 1808 | 90 | -60 | 364.2 | New Millennium
MR7547 | 484485 | 4499691 | 2221 | 270 | -90 | 367.3 | Trenton Canyon
MRA7548 | 484484 | 4499691 | 2221 | 270 | -80 | 367.3 | Trenton Canyon
MRA7549 | 484484 | 4499691 | 2221 | 270 | -60 | 367.3 | Trenton Canyon
MRA7550 | 484483 | 4499691 | 2221 | 270 | -50 | 336.8 | Trenton Canyon
MRA7551 | 477694 | 4495811 | 1619 | 90 | -65 | 367.3 | Buffalo Valley
MRA7552 | 477693 | 4495811 | 1619 | 60 | -65 | 367.3 | Buffalo Valley
MRA7553 | 484447 | 4499711 | 2201 | 270 | -60 | 336.8 | Trenton Canyon
MRA7554 | 484447 | 4499711 | 2201 | 270 | -80 | 382.5 | Trenton Canyon
MR7555 | 485426 | 4502775 | 1808 | 90 | -90 | 184.4 | New Millennium
MRA7556 | 485452 | 4502774 | 1813 | 90 | -75 | 345.9 | New Millennium
MRA7557 | 485514 | 4502805 | 1833 | 90 | -60 | 388.6 | New Millennium
MRA7558 | 485594 | 4502802 | 1844 | 90 | -55 | 388.6 | New Millennium
MRA7559 | 485411 | 4502748 | 1809 | 90 | -60 | 364.2 | New Millennium
MRA7560 | 485354 | 4502747 | 1808 | 90 | -60 | 358.1 | New Millennium
MRA7561 | 484732 | 4499414 | 2263 | 270 | -40 | 382.5 | Trenton Canyon
MRA7562 | 485449 | 4499223 | 2061 | 16 | -85 | 214.9 | Trenton Canyon
MRA7563 | 485449 | 4499222 | 2061 | 16 | -55 | 214.9 | Trenton Canyon
MRA7564 | 485549 | 4502806 | 1838 | 90 | -55 | 388.6 | New Millennium
MRA7565 | 485030 | 4499849 | 2026 | 270 | -55 | 367.3 | Trenton Canyon
MRA7566 | 485195 | 4502778 | 1816 | 90 | -60 | 245.4 | New Millennium
DDH7567 | 479233 | 4494132 | 1770 | 61 | -53 | 597.6 | Buffalo Valley
MRA7568 | 484713 | 4500378 | 1932 | 290 | -45 | 214.9 | Trenton Canyon
MRA7569 | 484879 | 4499016 | 2278 | 270 | -40 | 367.3 | Trenton Canyon
MRA7570 | 484834 | 4498957 | 2286 | 270 | -85 | 443.5 | Trenton Canyon
MRA7571 | 485562 | 4503052 | 1821 | 90 | -70 | 342.9 | New Millennium
MRA7572 | 485830 | 4503051 | 1873 | 90 | -75 | 379.5 | New Millennium
MRA7573 | 485675 | 4503048 | 1856 | 90 | -70 | 382.5 | New Millennium
MRA7574 | 485872 | 4503114 | 1871 | 90 | -75 | 379.5 | New Millennium
MR7575 | 484821 | 4498927 | 2288 | 60 | -90 | 153.9 | Trenton Canyon

SSR Mining Inc. |  | PAGE 28

Hole ID | Easting | Northing | Elevation (m) | Azimuth (deg.) | Dip (deg.) | Length (m) | Area
MRA7576 | 484822 | 4498927 | 2288 | 60 | -65 | 62.5 | Trenton Canyon
MRA7577 | 484809 | 4498896 | 2292 | 138 | -88 | 184.4 | Trenton Canyon
MRA7578 | 484809 | 4498897 | 2292 | 60 | -80 | 153.9 | Trenton Canyon
MRA7579 | 484809 | 4498897 | 2292 | 60 | -60 | 93 | Trenton Canyon
MRA7582 | 485910 | 4503115 | 1867 | 90 | -75 | 370.3 | New Millennium
MRA7583 | 485943 | 4503112 | 1872 | 90 | -75 | 355.1 | New Millennium
MRA7584 | 484804 | 4498856 | 2296 | 60 | -60 | 184.4 | Trenton Canyon
MRA7585 | 484804 | 4498856 | 2296 | 60 | -75 | 214.9 | Trenton Canyon
MRA7586 | 484805 | 4498857 | 2296 | 60 | -40 | 123.4 | Trenton Canyon
MRA7587 | 484805 | 4498858 | 2295 | 305 | -59 | 306.3 | Trenton Canyon
MRA7588 | 484801 | 4503978 | 1769 | 90 | -65 | 245.4 | New Millennium
MRA7591 | 484993 | 4499122 | 2262 | 270 | -45 | 336.8 | Trenton Canyon
DDH7592 | 478995 | 4494631 | 1725 | 60 | -65 | 228.9 | Buffalo Valley
MR7592 | 484852 | 4508311 | 1570 | 90 | -90 | 91.4 | Mackay
MR7593 | 478130 | 4494017 | 1643 | 0 | -90 | 428.2 | Buffalo Valley
MR7594 | 478325 | 4494274 | 1665 | 0 | -90 | 428.2 | Buffalo Valley
MR7595 | 478080 | 4494490 | 1647 | 0 | -90 | 428.2 | Buffalo Valley
MRA7596 | 478325 | 4494273 | 1665 | 60 | -75 | 428.2 | Buffalo Valley
MRA7597 | 478080 | 4494489 | 1647 | 90 | -75 | 428.2 | Buffalo Valley
MRA7598 | 478325 | 4494273 | 1665 | 90 | -70 | 428.2 | Buffalo Valley
MRA7599 | 478130 | 4494017 | 1643 | 90 | -70 | 379.5 | Buffalo Valley
DDH7600 | 478282 | 4496086 | 1661 | 270 | -70 | 609.9 | Buffalo Valley
MRA7601 | 478080 | 4494490 | 1647 | 90 | -60 | 428.2 | Buffalo Valley
MRA7602 | 477694 | 4495811 | 1619 | 110 | -65 | 367.3 | Buffalo Valley
MR7603 | 484879 | 4502845 | 1791 | 125 | -89 | 336.8 | New Millennium
MR7604 | 477912 | 4496230 | 1637 | 0 | -90 | 428.2 | Buffalo Valley
MRA7605 | 477912 | 4496230 | 1637 | 290 | -70 | 367.3 | Buffalo Valley
MRA7606 | 475554 | 4494322 | 1507 | 130 | -50 | 428.2 | Buffalo Valley
MRA7607 | 484802 | 4502360 | 1754 | 90 | -55 | 367.3 | New Millennium
MRA7608 | 478296 | 4496648 | 1654 | 90 | -70 | 367.3 | Buffalo Valley
MRA7609 | 478291 | 4496651 | 1654 | 290 | -70 | 367.3 | Buffalo Valley
MRA7610 | 478290 | 4496648 | 1654 | 230 | -70 | 367.3 | Buffalo Valley
MRA7611 | 475695 | 4494552 | 1516 | 90 | -50 | 428.2 | Buffalo Valley
MRA7613 | 475686 | 4494837 | 1518 | 90 | -50 | 364.2 | Buffalo Valley
MR7614 | 484624 | 4507805 | 1612 | 90 | -90 | 548.6 | Mackay
MRA7615 | 484923 | 4502466 | 1783 | 90 | -65 | 367.3 | New Millennium
MR7616 | 484627 | 4507802 | 1613 | 90 | -90 | 539.5 | Mackay
MRA7617 | 478946 | 4496852 | 1698 | 110 | -60 | 420.6 | Buffalo Valley
MRA7618 | 479173 | 4496826 | 1715 | 100 | -50 | 428.2 | Buffalo Valley
MRA7619 | 485037 | 4502964 | 1802 | 90 | -55 | 285 | New Millennium
MRA7621 | 484963 | 4502930 | 1804 | 90 | -65 | 214.9 | New Millennium
MRA7622 | 475580 | 4495132 | 1514 | 90 | -50 | 358.1 | Buffalo Valley
MRA7623 | 484946 | 4502964 | 1797 | 90 | -55 | 330.7 | New Millennium
MRA7624 | 484927 | 4502931 | 1797 | 90 | -65 | 245.4 | New Millennium
MR7625 | 484943 | 4502841 | 1811 | 112 | -89 | 367.3 | New Millennium
MR7626 | 485004 | 4502843 | 1824 | 0 | -90 | 367.3 | New Millennium
MR7627 | 485005 | 4502866 | 1822 | 0 | -90 | 306.3 | New Millennium

SSR Mining Inc. |  | PAGE 29

Hole ID | Easting | Northing | Elevation (m) | Azimuth (deg.) | Dip (deg.) | Length (m) | Area
MRA7628 | 484958 | 4502810 | 1817 | 90 | -70 | 367.3 | New Millennium
MRA7629 | 484968 | 4502744 | 1822 | 90 | -75 | 275.8 | New Millennium
MRA7630 | 484966 | 4502781 | 1822 | 90 | -75 | 367.3 | New Millennium
MRA7631 | 484970 | 4502599 | 1817 | 90 | -75 | 306.3 | New Millennium
MRA7633 | 485038 | 4502747 | 1834 | 90 | -75 | 275.8 | New Millennium
MR7634 | 484371 | 4507312 | 1624 | 90 | -90 | 557.8 | Mackay
MRA7635 | 485015 | 4502717 | 1832 | 90 | -75 | 367.3 | New Millennium
MRA7636 | 484979 | 4502718 | 1825 | 90 | -75 | 367.3 | New Millennium
MRA7637 | 484829 | 4502780 | 1781 | 90 | -75 | 355.1 | New Millennium
MRA7638 | 484973 | 4502688 | 1824 | 90 | -75 | 367.3 | New Millennium
MR7639 | 484827 | 4502841 | 1777 | 0 | -90 | 275.8 | New Millennium
MRA7641 | 484975 | 4502627 | 1821 | 90 | -75 | 306.3 | New Millennium
MRA7642 | 484735 | 4502840 | 1752 | 90 | -70 | 275.8 | New Millennium
MRA7643 | 484830 | 4502870 | 1775 | 90 | -70 | 367.3 | New Millennium
MRA7644 | 484829 | 4503023 | 1769 | 90 | -65 | 336.8 | New Millennium
MRA7645 | 485007 | 4502596 | 1822 | 90 | -75 | 306.3 | New Millennium
MR7646 | 484397 | 4507179 | 1625 | 90 | -90 | 563.9 | Mackay
MRA7647 | 475634 | 4495614 | 1515 | 90 | -50 | 365.8 | Buffalo Valley
MRA7648 | 484868 | 4503023 | 1777 | 90 | -65 | 336.8 | New Millennium
MRA7649 | 484838 | 4502901 | 1774 | 90 | -70 | 275.8 | New Millennium
MRA7650 | 484798 | 4503205 | 1754 | 90 | -65 | 306.3 | New Millennium
MRA7651 | 484799 | 4503205 | 1754 | 90 | -45 | 263.7 | New Millennium
MRA7652 | 475454 | 4495319 | 1510 | 90 | -50 | 339.9 | Buffalo Valley
MR7653 | 484757 | 4502832 | 1761 | 0 | -90 | 275.8 | New Millennium
MRA7654 | 484786 | 4502871 | 1766 | 90 | -70 | 367.3 | New Millennium
MRA7655 | 484792 | 4502902 | 1765 | 90 | -65 | 275.8 | New Millennium
MRA7656 | 484783 | 4502959 | 1757 | 90 | -55 | 359.7 | New Millennium
MRA7657 | 484833 | 4502961 | 1767 | 90 | -55 | 367.3 | New Millennium
MRA7658 | 484874 | 4502962 | 1777 | 90 | -55 | 263.7 | New Millennium
MRA7659 | 484857 | 4502934 | 1777 | 90 | -65 | 306.3 | New Millennium
MRA7660 | 484892 | 4502931 | 1787 | 90 | -65 | 278.9 | New Millennium
MRA7661 | 484761 | 4503265 | 1745 | 90 | -60 | 245.4 | New Millennium
MRA7662 | 484733 | 4502960 | 1747 | 90 | -55 | 367.3 | New Millennium
MRA7663 | 484686 | 4503111 | 1728 | 90 | -50 | 306.3 | New Millennium
MRA7664 | 478282 | 4493785 | 1660 | 90 | -50 | 428.2 | Buffalo Valley
MR7665 | 485442 | 4511046 | 1484 | 0 | -90 | 347.5 | Mackay
MRA7666 | 484691 | 4503175 | 1727 | 90 | -65 | 275.8 | New Millennium
MRA7667 | 484645 | 4503998 | 1740 | 90 | -60 | 367.3 | New Millennium
MRA7668 | 484744 | 4503023 | 1747 | 90 | -65 | 336.8 | New Millennium
MR7669 | 484759 | 4506471 | 1614 | 0 | -90 | 396.2 | New Millennium
MRA7670 | 478280 | 4493943 | 1661 | 90 | -50 | 428.2 | Buffalo Valley
MRA7671 | 484748 | 4503055 | 1747 | 90 | -65 | 391.7 | New Millennium
MRA7672 | 484781 | 4503861 | 1749 | 90 | -65 | 306.3 | New Millennium
MRA7673 | 484691 | 4503236 | 1727 | 90 | -75 | 275.8 | New Millennium
MRA7674 | 484702 | 4503266 | 1730 | 90 | -55 | 367.3 | New Millennium
MRA7675 | 484761 | 4503144 | 1748 | 90 | -65 | 413 | New Millennium
MRA7676 | 484720 | 4503146 | 1734 | 90 | -65 | 426.7 | New Millennium

SSR Mining Inc. |  | PAGE 30

Hole ID | Easting | Northing | Elevation (m) | Azimuth (deg.) | Dip (deg.) | Length (m) | Area
MRA7677 | 478274 | 4494102 | 1661 | 90 | -50 | 428.2 | Buffalo Valley
MRA7678 | 484746 | 4503922 | 1745 | 90 | -65 | 275.8 | New Millennium
MRA7679 | 484727 | 4503178 | 1737 | 90 | -65 | 275.8 | New Millennium
MRA7680 | 485708 | 4503171 | 1804 | 90 | -55 | 306.3 | New Millennium
MR7681 | 485614 | 4503162 | 1813 | 0 | -90 | 306.3 | New Millennium
MR7682 | 484566 | 4506880 | 1616 | 0 | -90 | 548.6 | Mackay
MRA7683 | 485007 | 4504259 | 1806 | 90 | -65 | 367.3 | New Millennium
MRA7684 | 484907 | 4504133 | 1803 | 90 | -65 | 367.3 | New Millennium
MRA7685 | 478554 | 4494093 | 1687 | 92 | -69 | 428.2 | Buffalo Valley
MRA7686 | 484729 | 4503295 | 1738 | 90 | -60 | 260.6 | New Millennium
MRA7687 | 484954 | 4504046 | 1806 | 90 | -65 | 245.4 | New Millennium
MRA7688 | 484915 | 4503981 | 1796 | 90 | -65 | 214.9 | New Millennium
MRA7689 | 484936 | 4503921 | 1790 | 90 | -65 | 367.3 | New Millennium
MRA7690 | 484632 | 4503924 | 1733 | 90 | -65 | 275.8 | New Millennium
MRA7691 | 484730 | 4503207 | 1736 | 90 | -70 | 306.3 | New Millennium
MRA7692 | 484695 | 4503390 | 1728 | 90 | -75 | 306.3 | New Millennium
MRA7693 | 485343 | 4502963 | 1818 | 90 | -70 | 342.9 | New Millennium
MR7694 | 484485 | 4506974 | 1629 | 0 | -90 | 560.8 | Mackay
MRA7695 | 485407 | 4502962 | 1830 | 90 | -70 | 358.1 | New Millennium
MRA7696 | 485043 | 4504140 | 1815 | 90 | -65 | 358.1 | New Millennium
MRA7697 | 484790 | 4503888 | 1751 | 90 | -65 | 214.9 | New Millennium
MRA7698 | 484867 | 4503871 | 1765 | 90 | -65 | 245.4 | New Millennium
MRA7699 | 484946 | 4503862 | 1767 | 90 | -65 | 214.9 | New Millennium
MRA7700 | 478001 | 4493940 | 1637 | 90 | -50 | 428.2 | Buffalo Valley
MRA7701 | 485728 | 4503000 | 1853 | 280 | -80 | 306.3 | New Millennium
MRA7702 | 484429 | 4499428 | 2248 | 268 | -80 | 336.8 | Trenton Canyon
MRA7703 | 484730 | 4499414 | 2262 | 274 | -63 | 275.9 | Trenton Canyon
MRA7704 | 485620 | 4502925 | 1850 | 280 | -80 | 306.3 | New Millennium
DDH7705 | 478300 | 4494548 | 1662 | 90 | -60 | 587 | Buffalo Valley
MRA7706 | 485739 | 4502812 | 1868 | 280 | -75 | 306.3 | New Millennium
MRA7707 | 485647 | 4502828 | 1859 | 280 | -75 | 306.3 | New Millennium
MRA7708 | 484475 | 4499534 | 2256 | 96 | -60 | 374.9 | Trenton Canyon
MRA7709 | 485779 | 4502836 | 1876 | 280 | -80 | 367.3 | New Millennium
MRA7710 | 485561 | 4502874 | 1854 | 280 | -80 | 306.3 | New Millennium
MRA7711 | 478278 | 4493861 | 1657 | 90 | -50 | 428.2 | Buffalo Valley
MRA7712 | 484867 | 4504251 | 1774 | 90 | -65 | 367.3 | New Millennium
MRA7714 | 485686 | 4502761 | 1845 | 280 | -65 | 367.3 | New Millennium
MRA7715 | 478279 | 4494016 | 1664 | 90 | -50 | 428.2 | Buffalo Valley
MRA7716 | 485691 | 4502909 | 1860 | 280 | -80 | 306.3 | New Millennium
MRA7717 | 485623 | 4502980 | 1835 | 280 | -80 | 306.3 | New Millennium
MRA7718 | 485134 | 4507333 | 1570 | 90 | -75 | 324.6 | Mackay
MRA7719 | 485123 | 4507490 | 1570 | 90 | -65 | 382.5 | Mackay
MRA7720 | 484812 | 4504041 | 1780 | 90 | -65 | 275.8 | New Millennium
MRA7722 | 485113 | 4507144 | 1570 | 90 | -60 | 297.2 | Mackay
MRA7723 | 485292 | 4507397 | 1570 | 90 | -50 | 230.1 | Mackay
MRA7724 | 485318 | 4507424 | 1570 | 90 | -58 | 245.4 | Mackay
MRA7725 | 484836 | 4503916 | 1766 | 90 | -65 | 245.4 | New Millennium

SSR Mining Inc. |  | PAGE 31

Hole ID | Easting | Northing | Elevation (m) | Azimuth (deg.) | Dip (deg.) | Length (m) | Area
MRA7726 | 485312 | 4507456 | 1570 | 90 | -60 | 278.9 | Mackay
MRA7727 | 485248 | 4507510 | 1570 | 90 | -70 | 260.6 | Mackay
MRA7728 | 485137 | 4507173 | 1569 | 90 | -60 | 321.6 | Mackay
MRA7729 | 485052 | 4507201 | 1569 | 90 | -75 | 330.7 | Mackay
MRA7730 | 478302 | 4494172 | 1664 | 90 | -50 | 428.2 | Buffalo Valley
MRA7731 | 484935 | 4507303 | 1592 | 90 | -70 | 336.8 | Mackay
MRA7732 | 485126 | 4507207 | 1570 | 90 | -55 | 309.4 | Mackay
MRA7733 | 485205 | 4507387 | 1570 | 90 | -80 | 281.9 | Mackay
MRA7734 | 485205 | 4507387 | 1570 | 90 | -70 | 275.8 | Mackay
MRA7735 | 484871 | 4503887 | 1768 | 90 | -65 | 214.9 | New Millennium
MRA7736 | 484966 | 4503873 | 1771 | 90 | -65 | 214.9 | New Millennium
MRA7737 | 485151 | 4507240 | 1570 | 90 | -65 | 306.3 | Mackay
MRA7738 | 485676 | 4502594 | 1864 | 90 | -70 | 214.9 | New Millennium
MRA7739 | 485796 | 4502895 | 1878 | 280 | -80 | 306.3 | New Millennium
MRA7740 | 485592 | 4502592 | 1854 | 90 | -60 | 214.9 | New Millennium
MRA7741 | 485580 | 4502562 | 1852 | 90 | -70 | 275.8 | New Millennium
MRA7742 | 484929 | 4507667 | 1579 | 90 | -58 | 318.5 | Mackay
MRA7743 | 485533 | 4502565 | 1845 | 90 | -70 | 306.3 | New Millennium
MRA7744 | 485519 | 4502591 | 1841 | 90 | -60 | 214.9 | New Millennium
MRA7745 | 485314 | 4507546 | 1541 | 90 | -50 | 214.9 | Mackay
MRA7746 | 485505 | 4502621 | 1838 | 90 | -60 | 245.4 | New Millennium
MRA7747 | 485453 | 4502630 | 1832 | 90 | -60 | 245.4 | New Millennium
MRA7748 | 485841 | 4502945 | 1880 | 280 | -80 | 306.3 | New Millennium
MRA7749 | 484910 | 4507695 | 1578 | 90 | -65 | 333.8 | Mackay
MR7750 | 484970 | 4510471 | 1503 | 0 | -90 | 457.2 | Mackay
MRA7751 | 485033 | 4507730 | 1524 | 90 | -65 | 245.4 | Mackay
MRA7752 | 484866 | 4506943 | 1605 | 90 | -65 | 312.4 | Mackay
MRA7753 | 485072 | 4507699 | 1523 | 90 | -60 | 260.6 | Mackay
MRA7754 | 485314 | 4509007 | 1535 | 90 | -75 | 207.3 | Mackay
MRA7755 | 485502 | 4502647 | 1838 | 93 | -64 | 245.4 | New Millennium
MRA7756 | 485261 | 4508944 | 1538 | 90 | -65 | 221 | Mackay
MRA7757 | 485485 | 4502685 | 1830 | 90 | -80 | 245.4 | New Millennium
MRA7758 | 485408 | 4502657 | 1828 | 90 | -65 | 275.8 | New Millennium
MRA7759 | 485286 | 4509068 | 1533 | 90 | -75 | 199.6 | Mackay
MRA7760 | 485393 | 4502685 | 1822 | 90 | -70 | 245.4 | New Millennium
MRA7761 | 485837 | 4503010 | 1875 | 280 | -80 | 306.3 | New Millennium
MRA7762 | 485265 | 4508985 | 1537 | 90 | -75 | 199.6 | Mackay
MRA7763 | 484916 | 4506927 | 1610 | 90 | -55 | 263.7 | Mackay
DDH7763 | 484675 | 4499504 | 2262 | 270 | -85 | 406.3 | Trenton Canyon
MRA7764 | 486181 | 4506423 | 1660 | 90 | -75 | 245.4 | Valmy
MR7765 | 485157 | 4510768 | 1499 | 0 | -90 | 457.2 | Mackay
MRA7766 | 486160 | 4506348 | 1665 | 90 | -75 | 245.4 | Valmy
MRA7767 | 486140 | 4506281 | 1675 | 90 | -75 | 245.4 | Valmy
MRA7768 | 485485 | 4502778 | 1820 | 96 | -61 | 367.3 | New Millennium
MRA7769 | 486220 | 4503017 | 1927 | 90 | -80 | 382.5 | New Millennium
MRA7770 | 485577 | 4502760 | 1830 | 280 | -80 | 306.3 | New Millennium
MRA7771 | 485247 | 4502778 | 1810 | 90 | -70 | 275.8 | New Millennium

SSR Mining Inc. |  | PAGE 32

Hole ID | Easting | Northing | Elevation (m) | Azimuth (deg.) | Dip (deg.) | Length (m) | Area
MRA7772 | 484457 | 4499104 | 2339 | 305 | -56 | 153.9 | Trenton Canyon
MRA7773 | 486147 | 4503020 | 1914 | 90 | -80 | 373.4 | New Millennium
MRA7774 | 486083 | 4503021 | 1898 | 90 | -80 | 367.3 | New Millennium
MRA7775 | 485544 | 4502774 | 1827 | 90 | -50 | 245.4 | New Millennium
MRA7776 | 484519 | 4499065 | 2356 | 270 | -55 | 214.9 | Trenton Canyon
MRA7777 | 484588 | 4499017 | 2381 | 270 | -55 | 214.9 | Trenton Canyon
MRA7778 | 485305 | 4502777 | 1805 | 90 | -70 | 275.8 | New Millennium
MRA7779 | 485361 | 4502781 | 1802 | 90 | -80 | 245.4 | New Millennium
MRA7780 | 484489 | 4498976 | 2372 | 270 | -55 | 184.4 | Trenton Canyon
MRA7781 | 484564 | 4498956 | 2382 | 270 | -55 | 245.4 | Trenton Canyon
MRA7782 | 484639 | 4499143 | 2389 | 266 | -40 | 336.8 | Trenton Canyon
MRA7783 | 484642 | 4499140 | 2391 | 266 | -52 | 332.2 | Trenton Canyon
MRA7786 | 485507 | 4502840 | 1843 | 90 | -65 | 275.8 | New Millennium
MRA7787 | 485555 | 4502835 | 1847 | 90 | -65 | 245.4 | New Millennium
MRA7788 | 485389 | 4502808 | 1814 | 90 | -70 | 259.1 | New Millennium
MRA7789 | 485279 | 4502746 | 1813 | 90 | -75 | 275.8 | New Millennium
MRA7791 | 485460 | 4502806 | 1826 | 90 | -70 | 245.4 | New Millennium
MRA7792 | 485467 | 4502748 | 1816 | 90 | -65 | 214.9 | New Millennium
MRA7793 | 484663 | 4499108 | 2395 | 275 | -58 | 382.5 | Trenton Canyon
MRA7795 | 484450 | 4499484 | 2255 | 270 | -65 | 291.1 | Trenton Canyon
MRA7796 | 484700 | 4499040 | 2374 | 265 | -52 | 336.8 | Trenton Canyon
MRA7797 | 485152 | 4507665 | 1515 | 90 | -70 | 199.6 | Mackay
MRA7799 | 485244 | 4507648 | 1508 | 90 | -70 | 190.5 | Mackay
MRA7800 | 485169 | 4507969 | 1356 | 270 | -70 | 68.6 | Mackay
MRA7801 | 485193 | 4507969 | 1355 | 270 | -75 | 108.2 | Mackay
MRA7802 | 485315 | 4507971 | 1341 | 90 | -80 | 68.6 | Mackay
MRA7803 | 485213 | 4508003 | 1342 | 90 | -75 | 68.6 | Mackay
MRA7804 | 484639 | 4499143 | 2389 | 266 | -52 | 336.8 | Trenton Canyon
MRA7805 | 485219 | 4507943 | 1353 | 90 | -70 | 111.3 | Mackay
MRA7806 | 485256 | 4507912 | 1349 | 90 | -70 | 102.1 | Mackay
MRA7807 | 485207 | 4507881 | 1364 | 90 | -70 | 77.7 | Mackay
MRA7808 | 485263 | 4507818 | 1371 | 90 | -70 | 62.5 | Mackay
MRA7809 | 484761 | 4499354 | 2263 | 185 | -72 | 367.3 | Trenton Canyon
MRA7814 | 484693 | 4499036 | 2374 | 62 | -72 | 275.8 | Trenton Canyon
MRA7817 | 484762 | 4499044 | 2346 | 84 | -55 | 245.4 | Trenton Canyon
MRA7819 | 484761 | 4499042 | 2346 | 55 | -65 | 184.4 | Trenton Canyon
MRA7820 | 484750 | 4499014 | 2345 | 62 | -82 | 169.2 | Trenton Canyon
MRA7821 | 485149 | 4502964 | 1790 | 90 | -55 | 275.8 | New Millennium
MRA7822 | 484759 | 4498980 | 2337 | 62 | -50 | 109.7 | Trenton Canyon
MRA7823 | 484754 | 4498872 | 2329 | 62 | -78 | 275.8 | Trenton Canyon
MRA7824 | 485137 | 4506936 | 1557 | 90 | -65 | 126.5 | Mackay
MRA7840 | 484640 | 4499550 | 2262 | 260 | -72 | 428.2 | Trenton Canyon
MRA7842 | 484668 | 4499500 | 2262 | 260 | -54 | 306.3 | Trenton Canyon

SSR Mining Inc. |  | PAGE 33