EX-99.1 10 exhibit991-ryderscottlette.htm EXHIBIT 99.1
EXHIBIT 99.1
SM ENERGY COMPANY
Estimated
Future Reserves
Attributable to Certain
Leasehold Interests
SEC Parameters
As of
December 31, 2017

/s/ Michael F. Stell |  | /s/ James L. Baird
Michael F. Stell, P.E. |  | James L. Baird
TBPE License No. 56416 |  | Colorado License No. 41521
Advising Senior Vice President |  | Managing Senior Vice President

| RYDER SCOTT COMPANY, L.P. TBPE Firm Registration No. F-1580 |

RYDER SCOTT COMPANY PETROLEUM CONSULTANTS

January 15, 2018
Mr. Levi J. Briese
Reserves Engineering Supervisor
SM Energy Company
1775 Sherman Street, Suite 1200
Denver, Colorado 80203
Gentlemen:
At the request of SM Energy Company (SM Energy), Ryder Scott Company, L.P. (Ryder Scott) has conducted a reserves audit of the estimates of the proved reserves as of December 31, 2017 prepared by SM Energy’s engineering and geological staff based on the definitions and disclosure guidelines of the United States Securities and Exchange Commission (SEC) contained in Title 17, Code of Federal Regulations, Modernization of Oil and Gas Reporting, Final Rule released January 14, 2009 in the Federal Register (SEC regulations). Our third party reserves audit, completed on December 22, 2017 and presented herein, was prepared for public disclosure by SM Energy in filings made with the SEC in accordance with the disclosure requirements set forth in the SEC regulations. The estimated reserves shown herein represent SM Energy’s estimated net reserves attributable to the leasehold interests in certain properties owned by SM Energy and the portion of those reserves reviewed by Ryder Scott, as of December 31, 2017. The properties reviewed by Ryder Scott incorporate 1,504 SM Energy reserve determinations and are located in the states of North Dakota, Texas and Wyoming.
The properties reviewed by Ryder Scott account for a portion of SM Energy’s total net proved reserves as of December 31, 2017. Based on the estimates of total net proved reserves prepared by SM Energy, the reserves audit conducted by Ryder Scott addresses 91.4 percent of the total proved developed net liquid hydrocarbon reserves, 91.6 percent of the total proved developed net gas reserves, 65.1 percent of the total proved undeveloped net liquid hydrocarbon reserves, and 46.9 percent of the total proved undeveloped net gas reserves of SM Energy.
As prescribed by the Society of Petroleum Engineers in Paragraph 2.2(f) of the Standards Pertaining to the Estimating and Auditing of Oil and Gas Reserves Information (SPE auditing standards), a reserves audit is defined as “the process of reviewing certain of the pertinent facts interpreted and assumptions made that have resulted in an estimate of reserves and/or Reserves Information prepared by others and the rendering of an opinion about (1) the appropriateness of the methodologies employed; (2) the adequacy and quality of the data relied upon; (3) the depth and thoroughness of the reserves estimation process; (4) the classification of reserves appropriate to the relevant definitions used; and (5) the reasonableness of the estimated reserve quantities and/or Reserves Information.” Reserves Information may consist of various estimates pertaining to the extent and value of petroleum properties.
SUITE 600, 1015 4TH STREET, S.W. CALGARY, ALBERTA T2R 1J4 TEL (403) 262-2799 FAX (403) 262-2790
621 17TH STREET, SUITE 1550 DENVER, COLORADO 80293-1501 TEL (303) 623-9147 FAX (303) 623-4258

SM Energy Company
January 15, 2018
Page 2
Based on our review, including the data, technical processes and interpretations presented by SM Energy, it is our opinion that the overall procedures and methodologies utilized by SM Energy in preparing their estimates of the proved reserves as of December 31, 2017 comply with the current SEC regulations and that the overall proved reserves for the reviewed properties as estimated by SM Energy are, in the aggregate, reasonable within the established audit tolerance guidelines of 10 percent as set forth in the SPE auditing standards.
The estimated reserves presented in this report are related to hydrocarbon prices. SM Energy has informed us that in the preparation of their reserve and income projections, as of December 31, 2017, they used average prices during the 12-month period prior to the “as of date” of this report, determined as the unweighted arithmetic averages of the prices in effect on the first-day-of-the-month for each month within such period, unless prices were defined by contractual arrangements, as required by the SEC regulations. Actual future prices may vary significantly from the prices required by SEC regulations; therefore, volumes of reserves actually recovered and the amounts of income actually received may differ significantly from the estimated quantities presented in this report. The net reserves as estimated by SM Energy attributable to SM Energy's interest in properties that we reviewed and the reserves of properties that we did not review are summarized below:
SEC PARAMETERS
Estimated Net Reserves
Certain Leasehold Interests of
SM Energy Company

As of December 31, 2017

|  | Proved
|  | Developed |  |  |  | Total
|  | Producing |  | Non-Producing |  | Undeveloped |  | Proved
Net Reserves of Properties Audited by Ryder Scott |  |  |  |  |  |  |  |
Oil/Condensate - MBBLS |  | 48,697 |  | 1,499 |  | 78,955 |  | 129,151
Plant Products - MBBLS |  | 48,141 |  | 0 |  | 16,897 |  | 65,038
Gas – MMCF |  | 587,010 |  | 1,671 |  | 298,953 |  | 887,634
Net Reserves of Properties Not Audited by Ryder Scott |  |  |  |  |  |  |  |
Oil/Condensate - MBBLS |  | 5,594 |  | 2,797 |  | 20,678 |  | 29,069
Plant Products - MBBLS |  | 76 |  | 760 |  | 30,667 |  | 31,503
Gas – MMCF |  | 42,645 |  | 11,583 |  | 338,286 |  | 392,514
Total Net Reserves |  |  |  |  |  |  |  |
Oil/Condensate - MBBLS |  | 54,291 |  | 4,296 |  | 99,633 |  | 158,220
Plant Products - MBBLS |  | 48,217 |  | 760 |  | 47,564 |  | 96,541
Gas – MMCF |  | 629,655 |  | 13,254 |  | 637,239 |  | 1,280,148

Liquid hydrocarbons are expressed in standard 42 gallon barrels and shown herein as thousands of barrels (MBBLS). All gas volumes are reported on an “as sold basis” expressed in millions of cubic feet (MMCF) at the official temperature and pressure bases of the areas in which the gas reserves are located.
RYDER SCOTT COMPANY PETROLEUM CONSULTANTS

SM Energy Company
January 15, 2018
Page 3
Reserves Included in This Report
In our opinion, the proved reserves presented in this report conform to the definition as set forth in the Securities and Exchange Commission’s Regulations Part 210.4-10(a). An abridged version of the SEC reserves definitions from 210.4-10(a) entitled “Petroleum Reserves Definitions” is included as an attachment to this report.
The various proved reserve status categories are defined under the attachment entitled “Petroleum Reserves Status Definitions and Guidelines” in this report. The proved developed non-producing reserves included herein consist of the shut-in and behind pipe categories.
Reserves are “estimated remaining quantities of oil and gas and related substances anticipated to be economically producible, as of a given date, by application of development projects to known accumulations.” All reserve estimates involve an assessment of the uncertainty relating the likelihood that the actual remaining quantities recovered will be greater or less than the estimated quantities determined as of the date the estimate is made. The uncertainty depends chiefly on the amount of reliable geologic and engineering data available at the time of the estimate and the interpretation of these data. The relative degree of uncertainty may be conveyed by placing reserves into one of two principal classifications, either proved or unproved. Unproved reserves are less certain to be recovered than proved reserves and may be further sub-classified as probable and possible reserves to denote progressively increasing uncertainty in their recoverability. At SM Energy’s request, this report addresses only the proved reserves attributable to the properties reviewed herein.
Proved oil and gas reserves are “those quantities of oil and gas which, by analysis of geoscience and engineering data, can be estimated with reasonable certainty to be economically producible from a given date forward.” The proved reserves included herein were estimated using deterministic methods. The SEC has defined reasonable certainty for proved reserves, when based on deterministic methods, as a “high degree of confidence that the quantities will be recovered.”
Proved reserve estimates will generally be revised only as additional geologic or engineering data become available or as economic conditions change. For proved reserves, the SEC states that “as changes due to increased availability of geoscience (geological, geophysical, and geochemical), engineering, and economic data are made to the estimated ultimate recovery (EUR) with time, reasonably certain EUR is much more likely to increase or remain constant than to decrease.” Moreover, estimates of proved reserves may be revised as a result of future operations, effects of regulation by governmental agencies or geopolitical or economic risks. Therefore, the proved reserves included in this report are estimates only and should not be construed as being exact quantities, and if recovered could be more or less than the estimated amounts.
Audit Data, Methodology, Procedure and Assumptions
The estimation of reserves involves two distinct determinations. The first determination results in the estimation of the quantities of recoverable oil and gas and the second determination results in the estimation of the uncertainty associated with those estimated quantities in accordance with the definitions set forth by the Securities and Exchange Commission’s Regulations Part 210.4-10(a). The process of estimating the quantities of recoverable oil and gas reserves relies on the use of certain generally accepted analytical procedures. These analytical procedures fall into three broad categories or methods: (1) performance-based methods; (2) volumetric-based methods; and (3) analogy. These methods may be
RYDER SCOTT COMPANY PETROLEUM CONSULTANTS

SM Energy Company
January 15, 2018
Page 4
used individually or in combination by the reserve evaluator in the process of estimating the quantities of reserves. Reserve evaluators must select the method or combination of methods which in their professional judgment is most appropriate given the nature and amount of reliable geoscience and engineering data available at the time of the estimate, the established or anticipated performance characteristics of the reservoir being evaluated and the stage of development or producing maturity of the property.
In many cases, the analysis of the available geoscience and engineering data and the subsequent interpretation of this data may indicate a range of possible outcomes in an estimate, irrespective of the method selected by the evaluator. When a range in the quantity of reserves is identified, the evaluator must determine the uncertainty associated with the incremental quantities of the reserves. If the reserve quantities are estimated using the deterministic incremental approach, the uncertainty for each discrete incremental quantity of the reserves is addressed by the reserve category assigned by the evaluator. Therefore, it is the categorization of reserve quantities as proved, probable and/or possible that addresses the inherent uncertainty in the estimated quantities reported. For proved reserves, uncertainty is defined by the SEC as reasonable certainty wherein the “quantities actually recovered are much more likely than not to be achieved.” The SEC states that “probable reserves are those additional reserves that are less certain to be recovered than proved reserves but which, together with proved reserves, are as likely as not to be recovered.” The SEC states that “possible reserves are those additional reserves that are less certain to be recovered than probable reserves and the total quantities ultimately recovered from a project have a low probability of exceeding proved plus probable plus possible reserves.” All quantities of reserves within the same reserve category must meet the SEC definitions as noted above.
Estimates of reserves quantities and their associated reserve categories may be revised in the future as additional geoscience or engineering data become available. Furthermore, estimates of reserves quantities and their associated reserve categories may also be revised due to other factors such as changes in economic conditions, results of future operations, effects of regulation by governmental agencies or geopolitical or economic risks as previously noted herein.
The proved reserves, prepared by SM Energy, for the properties that we reviewed were estimated by performance methods, the volumetric method, analogy, or a combination of methods. Approximately 100 percent of the proved producing reserves attributable to producing wells and/or reservoirs that we reviewed were estimated by performance methods or a combination of methods. These performance methods include, but may not be limited to, decline curve analysis, material balance and/or reservoir simulation which utilized extrapolations of historical production and pressure data available through November or early December 2017, in those cases where such data were considered to be definitive. The data utilized in this analysis were furnished to Ryder Scott by SM Energy or obtained from public data sources and were considered sufficient for the purpose thereof.
Approximately 100 percent of the proved developed non-producing and undeveloped reserves that we reviewed were estimated by the volumetric method, analogy, or a combination of methods. The volumetric analysis utilized pertinent well and seismic data furnished to Ryder Scott by SM Energy for our review or which we have obtained from public data sources that were available through December 2017. The data utilized from the analogues in conjunction with well and seismic data incorporated into the volumetric analysis were considered sufficient for the purpose thereof.
To estimate economically recoverable proved oil and gas reserves, many factors and assumptions are considered including, but not limited to, the use of reservoir parameters derived from geological, geophysical and engineering data which cannot be measured directly, economic criteria based on current costs and SEC pricing requirements, and forecasts of future production rates. Under the SEC regulations 210.4-10(a)(22)(v) and (26), proved reserves must be anticipated to be economically producible from a given date forward based on existing economic conditions including the prices and costs at which economic producibility from a reservoir is to be determined. While it may reasonably be anticipated that the future
RYDER SCOTT COMPANY PETROLEUM CONSULTANTS

SM Energy Company
January 15, 2018
Page 5
prices received for the sale of production and the operating costs and other costs relating to such production may increase or decrease from those under existing economic conditions, such changes were, in accordance with rules adopted by the SEC, omitted from consideration in conducting this review.
As stated previously, proved reserves must be anticipated to be economically producible from a given date forward based on existing economic conditions including the prices and costs at which economic producibility from a reservoir is to be determined. To confirm that the proved reserves reviewed by us meet the SEC requirements to be economically producible, we have reviewed certain primary economic data utilized by SM Energy relating to hydrocarbon prices and costs as noted herein.
The hydrocarbon prices furnished by SM Energy for the properties reviewed by us are based on SEC price parameters using the average prices during the 12-month period prior to the “as of date” of this report, determined as the unweighted arithmetic averages of the prices in effect on the first-day-of-the-month for each month within such period, unless prices were defined by contractual arrangements. For hydrocarbon products sold under contract, the contract prices, including fixed and determinable escalations exclusive of inflation adjustments, were used until expiration of the contract. Upon contract expiration, the prices were adjusted to the 12-month unweighted arithmetic average as previously described.
The initial SEC hydrocarbon prices in effect on December 31, 2017 for the properties reviewed by us were determined using the 12-month average first-day-of-the-month benchmark prices appropriate to the geographic area where the hydrocarbons are sold. These benchmark prices are prior to the adjustments for differentials as described herein. The table below summarizes the “benchmark prices” and “price reference” used by SM Energy for the geographic area reviewed by us. In certain geographic areas, the price reference and benchmark prices may be defined by contractual arrangements.
The product prices which were actually used by SM Energy to determine the future gross revenue for each property reviewed by us reflect adjustments to the benchmark prices for gravity, quality, local conditions, and/or distance from market, referred to herein as “differentials.” The differentials used by SM Energy were accepted as factual data and reviewed by us for their reasonableness; however, we have not conducted an independent verification of the data used by SM Energy.
The table below summarizes SM Energy’s net volume weighted benchmark prices adjusted for differentials for the properties reviewed by us and referred to herein as SM Energy’s “average realized prices.” The average realized prices shown in the table below were determined from SM Energy’s estimate of the total future gross revenue before production taxes for the properties reviewed by us and SM Energy’s estimate of the total net reserves for the properties reviewed by us for the geographic area. The data shown in the table below is presented in accordance with SEC disclosure requirements for the geographic area reviewed by us.

Geographic Area | Product | Price Reference | Average Benchmark Prices | Average Realized Prices
North America |  |  |  |
| Oil/Condensate | WTI, Cushing | $51.34/BBL | $48.74/BBL
United States | NGLs | NGL | $27.69/BBL | $23.16/BBL
| Gas | Henry Hub | $3.00/MMBTU | $3.34/MCF

The effects of derivative instruments designated as price hedges of oil and gas quantities are not reflected in SM Energy’s individual property evaluations.
RYDER SCOTT COMPANY PETROLEUM CONSULTANTS

SM Energy Company
January 15, 2018
Page 6
Accumulated gas production imbalances, if any, were not taken into account in the proved gas reserve estimates reviewed. The proved gas volumes presented herein do not include volumes of gas consumed in operations as reserves.
Operating costs furnished by SM Energy are based on the operating expense reports of SM Energy and include only those costs directly applicable to the leases or wells for the properties reviewed by us. The operating costs include a portion of general and administrative costs allocated directly to the leases and wells. For operated properties, the operating costs include an appropriate level of corporate general administrative and overhead costs. The operating costs for non-operated properties include the COPAS overhead costs that are allocated directly to the leases and wells under terms of operating agreements. The operating costs furnished by SM Energy were accepted as factual data and reviewed by us for their reasonableness; however, we have not conducted an independent verification of the data used by SM Energy. No deduction was made for loan repayments, interest expenses, or exploration and development prepayments that were not charged directly to the leases or wells.
Development costs furnished by SM Energy are based on authorizations for expenditure for the proposed work or actual costs for similar projects. The development costs furnished by SM Energy were accepted as factual data and reviewed by us for their reasonableness; however, we have not conducted an independent verification of the data used by SM Energy. The estimated net cost of abandonment and salvage was included by SM Energy for properties where abandonment costs and salvage were significant. SM Energy’s estimates of the net abandonment costs were accepted without independent verification.
The proved developed non-producing and undeveloped reserves for the properties reviewed by us have been incorporated herein in accordance with SM Energy’s plans to develop these reserves as of December 31, 2017. The implementation of SM Energy’s development plans as presented to us is subject to the approval process adopted by SM Energy’s management. As the result of our inquiries during the course of our review, SM Energy has informed us that the development activities for the properties reviewed by us have been subjected to and received the internal approvals required by SM Energy’s management at the appropriate local, regional and/or corporate level. In addition to the internal approvals as noted, certain development activities may still be subject to specific partner AFE processes, Joint Operating Agreement (JOA) requirements or other administrative approvals external to SM Energy. Additionally, SM Energy has informed us that they are not aware of any legal, regulatory, or political obstacles that would significantly alter their plans. While these plans could change from those under existing economic conditions as of December 31, 2017, such changes were, in accordance with rules adopted by the SEC, omitted from consideration in making this evaluation.
Current costs used by SM Energy were held constant throughout the life of the properties.
SM Energy’s forecasts of future production rates are based on historical performance from wells currently on production. If no production decline trend has been established, future production rates were held constant, or adjusted for the effects of curtailment where appropriate, until a decline in ability to produce was anticipated. An estimated rate of decline was then applied to depletion of the reserves. If a decline trend has been established, this trend was used as the basis for estimating future production rates.
RYDER SCOTT COMPANY PETROLEUM CONSULTANTS

SM Energy Company
January 15, 2018
Page 7
Test data and other related information were used by SM Energy to estimate the anticipated initial production rates for those wells or locations that are not currently producing. For reserves not yet on production, sales were estimated to commence at an anticipated date furnished by SM Energy. Wells or locations that are not currently producing may start producing earlier or later than anticipated in SM Energy’s estimates due to unforeseen factors causing a change in the timing to initiate production. Such factors may include delays due to weather, the availability of rigs, the sequence of drilling, completing and/or recompleting wells and/or constraints set by regulatory bodies.
The future production rates from wells currently on production or wells or locations that are not currently producing may be more or less than estimated because of changes including, but not limited to, reservoir performance, operating conditions related to surface facilities, compression and artificial lift, pipeline capacity and/or operating conditions, producing market demand and/or allowables or other constraints set by regulatory bodies.
SM Energy’s operations may be subject to various levels of governmental controls and regulations. These controls and regulations may include, but may not be limited to, matters relating to land tenure and leasing, the legal rights to produce hydrocarbons, drilling and production practices, environmental protection, marketing and pricing policies, royalties, various taxes and levies including income tax and are subject to change from time to time. Such changes in governmental regulations and policies may cause volumes of proved reserves actually recovered and amounts of proved income actually received to differ significantly from the estimated quantities.
The estimates of proved reserves presented herein were based upon a review of the properties in which SM Energy owns an interest; however, we have not made any field examination of the properties. No consideration was given in this report to potential environmental liabilities that may exist nor were any costs included by SM Energy for potential liabilities to restore and clean up damages, if any, caused by past operating practices.
Certain technical personnel of SM Energy are responsible for the preparation of reserve estimates on new properties and for the preparation of revised estimates, when necessary, on old properties. These personnel assembled the necessary data and maintained the data and workpapers in an orderly manner. We consulted with these technical personnel and had access to their workpapers and supporting data in the course of our audit.
SM Energy has informed us that they have furnished us all of the material accounts, records, geological and engineering data, and reports and other data required for this investigation. In performing our audit of SM Energy’s forecast of future proved production, we have relied upon data furnished by SM Energy with respect to property interests owned, production and well tests from examined wells, normal direct costs of operating the wells or leases, other costs such as transportation and/or processing fees, ad valorem and production taxes, recompletion and development costs, development plans, abandonment costs and salvage, product prices based on the SEC regulations, adjustments or differentials to product prices, geological structural and isochore maps, well logs, core analyses, and pressure measurements. Ryder Scott reviewed such factual data for its reasonableness; however, we have not conducted an independent verification of the data furnished by SM Energy. The data described herein were accepted as authentic and sufficient for determining the reserves unless, during the course of our examination, a matter of question came to our attention in which case the data were not accepted until all questions were satisfactorily resolved. We consider the factual data furnished to us by SM Energy to be appropriate and sufficient for the purpose of our review of SM Energy’s estimates of reserves. In summary, we consider the assumptions, data, methods and analytical procedures used by SM Energy and as reviewed by us appropriate for the purpose hereof, and we have used all such methods and procedures that we consider necessary and appropriate under the circumstances to render the conclusions set forth herein.
RYDER SCOTT COMPANY PETROLEUM CONSULTANTS

SM Energy Company
January 15, 2018
Page 8
RYDER SCOTT COMPANY PETROLEUM CONSULTANTS

SM Energy Company
January 15, 2018
Page 9
Audit Opinion
Based on our review, including the data, technical processes and interpretations presented by SM Energy, it is our opinion that the overall procedures and methodologies utilized by SM Energy in preparing their estimates of the proved reserves as of December 31, 2017 comply with the current SEC regulations and that the overall proved reserves for the reviewed properties as estimated by SM Energy are, in the aggregate, reasonable within the established audit tolerance guidelines of 10 percent as set forth in the SPE auditing standards. Ryder Scott found the processes and controls used by SM Energy in their estimation of proved reserves to be effective and we found no bias in the utilization and analysis of data in estimates for these properties
We were in reasonable agreement with SM Energy’s estimates of proved reserves for the properties which we reviewed; although in certain cases there was more than an acceptable variance between SM Energy’s estimates and our estimates due to a difference in interpretation of data or due to our having access to data which were not available to SM Energy when its reserve estimates were prepared. However not withstanding, it is our opinion that on an aggregate basis the data presented herein for the properties that we reviewed fairly reflects the estimated net reserves owned by SM Energy.
Other Properties
Other properties, as used herein, are those properties of SM Energy which we did not review. The proved net reserves attributable to the other properties account for 23.8 percent of the total proved net liquid hydrocarbon reserves and 30.7 percent of the total proved net gas reserves based on estimates prepared by SM Energy as of December 31, 2017. The other properties represent 17.1 percent of the total proved discounted future net income based on the unescalated pricing policy of the SEC as taken from reserve and income projections prepared by SM Energy as of December 31, 2017.
The same technical personnel of SM Energy were responsible for the preparation of the reserve estimates for the properties that we reviewed as well as for the properties not reviewed by Ryder Scott.
Standards of Independence and Professional Qualification
Ryder Scott is an independent petroleum engineering consulting firm that has been providing petroleum consulting services throughout the world since 1937. Ryder Scott is employee-owned and maintains offices in Houston, Texas; Denver, Colorado; and Calgary, Alberta, Canada. We have over eighty engineers and geoscientists on our permanent staff. By virtue of the size of our firm and the large number of clients for which we provide services, no single client or job represents a material portion of our annual revenue. We do not serve as officers or directors of any privately-owned or publicly-traded oil and gas company and are separate and independent from the operating and investment decision-making process of our clients. This allows us to bring the highest level of independence and objectivity to each engagement for our services.
Ryder Scott actively participates in industry-related professional societies and organizes an annual public forum focused on the subject of reserves evaluations and SEC regulations. Many of our staff have authored or co-authored technical papers on the subject of reserves related topics. We encourage our staff to maintain and enhance their professional skills by actively participating in ongoing continuing education.
RYDER SCOTT COMPANY PETROLEUM CONSULTANTS

SM Energy Company
January 15, 2018
Page 10
Prior to becoming an officer of the Company, Ryder Scott requires that staff engineers and geoscientists have received professional accreditation in the form of a registered or certified professional engineer’s license or a registered or certified professional geoscientist’s license, or the equivalent thereof, from an appropriate governmental authority or a recognized self-regulating professional organization.
We are independent petroleum engineers with respect to SM Energy. Neither we nor any of our employees have any financial interest in the subject properties, and neither the employment to do this work nor the compensation is contingent on our estimates of reserves for the properties which were reviewed.
The results of this audit, presented herein, are based on technical analysis conducted by teams of geoscientists and engineers from Ryder Scott. The professional qualifications of the undersigned, the technical persons primarily responsible for overseeing the review of the reserves information discussed in this report, are included as attachments to this letter.
Terms of Usage
The results of our third party audit, presented in report form herein, were prepared in accordance with the disclosure requirements set forth in the SEC regulations and intended for public disclosure as an exhibit in filings made with the SEC by SM Energy.
SM Energy makes periodic filings on Form 10-K with the SEC under the 1934 Exchange Act. Furthermore, SM Energy has certain registration statements filed with the SEC under the 1933 Securities Act into which any subsequently filed Form 10-K is incorporated by reference. We have consented to the incorporation by reference thereof into the Company's Registration Statements on Form S-8, of the references to our name as well as to the references to our third party report for SM Energy, which appears in the December 31, 2017 annual report on Form 10-K of SM Energy. Our written consent for such use is included as a separate exhibit to the filings made with the SEC by SM Energy.
We have provided SM Energy with a digital version of the original signed copy of this report letter. In the event there are any differences between the digital version included in filings made by SM Energy and the original signed report letter, the original signed report letter shall control and supersede the digital version.
RYDER SCOTT COMPANY PETROLEUM CONSULTANTS

SM Energy Company
January 15, 2018
Page 11
The data and work papers used in the preparation of this report are available for examination by authorized parties in our offices. Please contact us if we can be of further service.
Very truly yours,

| RYDER SCOTT COMPANY, L.P. TBPE Firm Registration No. F-1580 |
| /s/ Michael F. Stell |
Michael F. Stell, P.E. |
TBPE License No. 56416 |
Advising Senior Vice President |
| /s/ James L. Baird |
| James L. Baird
| Colorado License No. 41521
| Managing Senior Vice President

MFS-JLB (FWZ)/pl
RYDER SCOTT COMPANY PETROLEUM CONSULTANTS

Professional Qualifications of Primary Technical Person
The conclusions presented in this report are the result of technical analysis conducted by teams of geoscientists and engineers from Ryder Scott Company, L.P. Mr. Michael F. Stell was the primary technical person responsible for overseeing the estimate of the reserves, future production and income.
Mr. Stell, an employee of Ryder Scott Company, L.P. (Ryder Scott) since 1992, is an Advising Senior Vice President and is responsible for coordinating and supervising staff and consulting engineers of the company in ongoing reservoir evaluation studies worldwide. Before joining Ryder Scott, Mr. Stell served in a number of engineering positions with Shell Oil Company and Landmark Concurrent Solutions. For more information regarding Mr. Stell’s geographic and job specific experience, please refer to the Ryder Scott Company website at www.ryderscott.com/Company/Employees.
Mr. Stell earned a Bachelor of Science degree in Chemical Engineering from Purdue University in 1979 and a Master of Science Degree in Chemical Engineering from the University of California, Berkeley, in 1981. He is a licensed Professional Engineer in the State of Texas. He is also a member of the Society of Petroleum Engineers and the Society of Petroleum Evaluation Engineers.
In addition to gaining experience and competency through prior work experience, the Texas Board of Professional Engineers requires a minimum of fifteen hours of continuing education annually, including at least one hour in the area of professional ethics, which Mr. Stell fulfills. As part of his 2009 continuing education hours, Mr. Stell attended an internally presented 13 hours of formalized training as well as a day-long public forum relating to the definitions and disclosure guidelines contained in the United States Securities and Exchange Commission Title 17, Code of Federal Regulations, Modernization of Oil and Gas Reporting, Final Rule released January 14, 2009 in the Federal Register. Mr. Stell attended an additional 15 hours of formalized in-house training as well as an additional five hours of formalized external training during 2009 covering such topics as the SPE/WPC/AAPG/SPEE Petroleum Resources Management System, reservoir engineering, geoscience and petroleum economics evaluation methods, procedures and software and ethics for consultants. As part of his 2010 continuing education hours, Mr. Stell attended an internally presented six hours of formalized training and ten hours of formalized external training covering such topics as updates concerning the implementation of the latest SEC oil and gas reporting requirements, reserve reconciliation processes, overviews of the various productive basins of North America, evaluations of resource play reserves, evaluation of enhanced oil recovery reserves, and ethics training. For each year starting 2011 through 2017, as of the date of this report, Mr. Stell has 20 hours of continuing education hours relating to reserves, reserve evaluations, and ethics.
Based on his educational background, professional training and over 35 years of practical experience in the estimation and evaluation of petroleum reserves, Mr. Stell has attained the professional qualifications for a Reserves Estimator and Reserves Auditor set forth in Article III of the “Standards Pertaining to the Estimating and Auditing of Oil and Gas Reserves Information” promulgated by the Society of Petroleum Engineers as of February 19, 2007.
RYDER SCOTT COMPANY PETROLEUM CONSULTANTS

Professional Qualifications of Primary Technical Person
The conclusions presented in this report are the result of technical analysis conducted by teams of geoscientists and engineers from Ryder Scott Company, L.P. James Larry Baird was the primary technical person responsible for overseeing the estimate of the reserves.
Mr. Baird, an employee of Ryder Scott Company, L.P. (Ryder Scott) since 2006, is a Managing Senior Vice President and also serves as Manager of the Denver office, responsible for coordinating and supervising staff and consulting engineers of the company in ongoing reservoir evaluation studies worldwide. Before joining Ryder Scott, Mr. Baird served in a number of engineering positions with Gulf Oil Corporation (1970-1973), Northern Natural Gas (1973-1975) and Questar Exploration & Production (1975-2006). For more information regarding Mr. Baird’s geographic and job specific experience, please refer to the Ryder Scott Company website at www.ryderscott.com/Experience/Employees.
Mr. Baird earned a Bachelor of Science degree in Petroleum Engineering from the University of Missouri at Rolla in 1970. He is a registered Professional Engineer in the States of Colorado and Utah. He is also a Legion of Honor member of the Society of Petroleum Engineers.
In addition to gaining experience and competency through prior work experience, several State Boards of Professional Engineers require a minimum number of hours of continuing education annually, including at least one hour in the area of professional ethics, which Mr. Baird fulfills as part of his registration in two states. As part of his continuing education, Mr. Baird attends internally presented training as well as public forums relating to the definitions and disclosure guidelines contained in the United States Securities and Exchange Commission Title 17, Code of Federal Regulations, Modernization of Oil and Gas Reporting, and Final Rule released January 14, 2009 in the Federal Register. Mr. Baird attends additional hours of formalized internal and external training covering such topics as the SPE/WPC/AAPG/SPEE Petroleum Resources Management System, reservoir engineering and petroleum economics evaluation methods, various analysis software and ethics for consultants.
Based on his educational background, professional training and more than 48 years of practical experience in the estimation and evaluation of petroleum reserves, Mr. Baird has attained the professional qualifications as a Reserves Estimator and Reserves Auditor set forth in Article III of the “Standards Pertaining to the Estimating and Auditing of Oil and Gas Reserves Information” promulgated by the Society of Petroleum Engineers as of February 19, 2007.
RYDER SCOTT COMPANY PETROLEUM CONSULTANTS

PETROLEUM RESERVES DEFINITIONS
As Adapted From:
RULE 4-10(a) of REGULATION S-X PART 210
UNITED STATES SECURITIES AND EXCHANGE COMMISSION (SEC)
PREAMBLE
On January 14, 2009, the United States Securities and Exchange Commission (SEC) published the “Modernization of Oil and Gas Reporting; Final Rule” in the Federal Register of National Archives and Records Administration (NARA). The “Modernization of Oil and Gas Reporting; Final Rule” includes revisions and additions to the definition section in Rule 4-10 of Regulation S-X, revisions and additions to the oil and gas reporting requirements in Regulation S-K, and amends and codifies Industry Guide 2 in Regulation S-K. The “Modernization of Oil and Gas Reporting; Final Rule”, including all references to Regulation S-X and Regulation S-K, shall be referred to herein collectively as the “SEC regulations”. The SEC regulations take effect for all filings made with the United States Securities and Exchange Commission as of December 31, 2009, or after January 1, 2010. Reference should be made to the full text under Title 17, Code of Federal Regulations, Regulation S-X Part 210, Rule 4-10(a) for the complete definitions (direct passages excerpted in part or wholly from the aforementioned SEC document are denoted in italics herein).
Reserves are estimated remaining quantities of oil and gas and related substances anticipated to be economically producible, as of a given date, by application of development projects to known accumulations. All reserve estimates involve an assessment of the uncertainty relating the likelihood that the actual remaining quantities recovered will be greater or less than the estimated quantities determined as of the date the estimate is made. The uncertainty depends chiefly on the amount of reliable geologic and engineering data available at the time of the estimate and the interpretation of these data. The relative degree of uncertainty may be conveyed by placing reserves into one of two principal classifications, either proved or unproved. Unproved reserves are less certain to be recovered than proved reserves and may be further sub-classified as probable and possible reserves to denote progressively increasing uncertainty in their recoverability. Under the SEC regulations as of December 31, 2009, or after January 1, 2010, a company may optionally disclose estimated quantities of probable or possible oil and gas reserves in documents publicly filed with the SEC. The SEC regulations continue to prohibit disclosure of estimates of oil and gas resources other than reserves and any estimated values of such resources in any document publicly filed with the SEC unless such information is required to be disclosed in the document by foreign or state law as noted in §229.1202 Instruction to Item 1202.
Reserves estimates will generally be revised only as additional geologic or engineering data become available or as economic conditions change.
Reserves may be attributed to either natural energy or improved recovery methods. Improved recovery methods include all methods for supplementing natural energy or altering natural forces in the reservoir to increase ultimate recovery. Examples of such methods are pressure maintenance, natural gas cycling, waterflooding, thermal methods, chemical flooding, and the use of miscible and immiscible displacement fluids. Other improved recovery methods may be developed in the future as petroleum technology continues to evolve.
Reserves may be attributed to either conventional or unconventional petroleum accumulations. Petroleum accumulations are considered as either conventional or unconventional based on the nature of their in-place characteristics, extraction method applied, or degree of processing prior to sale. Examples of unconventional petroleum accumulations include coalbed or coalseam methane (CBM/CSM), basin-
RYDER SCOTT COMPANY PETROLEUM CONSULTANTS

PETROLEUM RESERVES DEFINITIONS
Page 2
centered gas, shale gas, gas hydrates, natural bitumen and oil shale deposits. These unconventional accumulations may require specialized extraction technology and/or significant processing prior to sale.
Reserves do not include quantities of petroleum being held in inventory.
Because of the differences in uncertainty, caution should be exercised when aggregating quantities of petroleum from different reserves categories.
RESERVES (SEC DEFINITIONS)
Securities and Exchange Commission Regulation S-X §210.4-10(a)(26) defines reserves as follows:
Reserves. Reserves are estimated remaining quantities of oil and gas and related substances anticipated to be economically producible, as of a given date, by application of development projects to known accumulations. In addition, there must exist, or there must be a reasonable expectation that there will exist, the legal right to produce or a revenue interest in the production, installed means of delivering oil and gas or related substances to market, and all permits and financing required to implement the project.
Note to paragraph (a)(26): Reserves should not be assigned to adjacent reservoirs isolated by major, potentially sealing, faults until those reservoirs are penetrated and evaluated as economically producible. Reserves should not be assigned to areas that are clearly separated from a known accumulation by a non-productive reservoir (i.e., absence of reservoir, structurally low reservoir, or negative test results). Such areas may contain prospective resources (i.e., potentially recoverable resources from undiscovered accumulations).
PROVED RESERVES (SEC DEFINITIONS)
Securities and Exchange Commission Regulation S-X §210.4-10(a)(22) defines proved oil and gas reserves as follows:
Proved oil and gas reserves. Proved oil and gas reserves are those quantities of oil and gas, which, by analysis of geoscience and engineering data, can be estimated with reasonable certainty to be economically producible—from a given date forward, from known reservoirs, and under existing economic conditions, operating methods, and government regulations—prior to the time at which contracts providing the right to operate expire, unless evidence indicates that renewal is reasonably certain, regardless of whether deterministic or probabilistic methods are used for the estimation. The project to extract the hydrocarbons must have commenced or the operator must be reasonably certain that it will commence the project within a reasonable time.
(i) The area of the reservoir considered as proved includes:
(A) The area identified by drilling and limited by fluid contacts, if any, and
(B) Adjacent undrilled portions of the reservoir that can, with reasonable certainty, be judged to be continuous with it and to contain economically producible oil or gas on the basis of available geoscience and engineering data.
RYDER SCOTT COMPANY PETROLEUM CONSULTANTS

PETROLEUM RESERVES DEFINITIONS
Page 3
PROVED RESERVES (SEC DEFINITIONS) CONTINUED
(ii) In the absence of data on fluid contacts, proved quantities in a reservoir are limited by the lowest known hydrocarbons (LKH) as seen in a well penetration unless geoscience, engineering, or performance data and reliable technology establishes a lower contact with reasonable certainty.
(iii) Where direct observation from well penetrations has defined a highest known oil (HKO) elevation and the potential exists for an associated gas cap, proved oil reserves may be assigned in the structurally higher portions of the reservoir only if geoscience, engineering, or performance data and reliable technology establish the higher contact with reasonable certainty.
(iv) Reserves which can be produced economically through application of improved recovery techniques (including, but not limited to, fluid injection) are included in the proved classification when:
(A) Successful testing by a pilot project in an area of the reservoir with properties no more favorable than in the reservoir as a whole, the operation of an installed program in the reservoir or an analogous reservoir, or other evidence using reliable technology establishes the reasonable certainty of the engineering analysis on which the project or program was based; and
(B) The project has been approved for development by all necessary parties and entities, including governmental entities.
(v) Existing economic conditions include prices and costs at which economic producibility from a reservoir is to be determined. The price shall be the average price during the 12-month period prior to the ending date of the period covered by the report, determined as an unweighted arithmetic average of the first-day-of-the-month price for each month within such period, unless prices are defined by contractual arrangements, excluding escalations based upon future conditions.
RYDER SCOTT COMPANY PETROLEUM CONSULTANTS

PETROLEUM RESERVES STATUS DEFINITIONS AND GUIDELINES
As Adapted From:
RULE 4-10(a) of REGULATION S-X PART 210
UNITED STATES SECURITIES AND EXCHANGE COMMISSION (SEC)
and
PETROLEUM RESOURCES MANAGEMENT SYSTEM (SPE-PRMS)
Sponsored and Approved by:
SOCIETY OF PETROLEUM ENGINEERS (SPE)
WORLD PETROLEUM COUNCIL (WPC)
AMERICAN ASSOCIATION OF PETROLEUM GEOLOGISTS (AAPG)
SOCIETY OF PETROLEUM EVALUATION ENGINEERS (SPEE)
Reserves status categories define the development and producing status of wells and reservoirs. Reference should be made to Title 17, Code of Federal Regulations, Regulation S-X Part 210, Rule 4-10(a) and the SPE-PRMS as the following reserves status definitions are based on excerpts from the original documents (direct passages excerpted from the aforementioned SEC and SPE-PRMS documents are denoted in italics herein).
DEVELOPED RESERVES (SEC DEFINITIONS)
Securities and Exchange Commission Regulation S-X §210.4-10(a)(6) defines developed oil and gas reserves as follows:
Developed oil and gas reserves are reserves of any category that can be expected to be recovered:
(i) Through existing wells with existing equipment and operating methods or in which the cost of the required equipment is relatively minor compared to the cost of a new well; and
(ii) Through installed extraction equipment and infrastructure operational at the time of the reserves estimate if the extraction is by means not involving a well.
Developed Producing (SPE-PRMS Definitions)
While not a requirement for disclosure under the SEC regulations, developed oil and gas reserves may be further sub-classified according to the guidance contained in the SPE-PRMS as Producing or Non-Producing.
Developed Producing Reserves
Developed Producing Reserves are expected to be recovered from completion intervals that are open and producing at the time of the estimate.
Improved recovery reserves are considered producing only after the improved recovery project is in operation.
RYDER SCOTT COMPANY PETROLEUM CONSULTANTS

PETROLEUM RESERVES STATUS DEFINITIONS AND GUIDELINES
Page 2
Developed Non-Producing
Developed Non-Producing Reserves include shut-in and behind-pipe reserves.
Shut-In
Shut-in Reserves are expected to be recovered from:

(1) | completion intervals which are open at the time of the estimate, but which have not started producing;

(2) | wells which were shut-in for market conditions or pipeline connections; or

(3) | wells not capable of production for mechanical reasons.

Behind-Pipe
Behind-pipe Reserves are expected to be recovered from zones in existing wells, which will require additional completion work or future re-completion prior to start of production.
In all cases, production can be initiated or restored with relatively low expenditure compared to the cost of drilling a new well.
UNDEVELOPED RESERVES (SEC DEFINITIONS)
Securities and Exchange Commission Regulation S-X §210.4-10(a)(31) defines undeveloped oil and gas reserves as follows:
Undeveloped oil and gas reserves are reserves of any category that are expected to be recovered from new wells on undrilled acreage, or from existing wells where a relatively major expenditure is required for recompletion.

(i) | Reserves on undrilled acreage shall be limited to those directly offsetting development spacing areas that are reasonably certain of production when drilled, unless evidence using reliable technology exists that establishes reasonable certainty of economic producibility at greater distances.

(ii) Undrilled locations can be classified as having undeveloped reserves only if a development plan has been adopted indicating that they are scheduled to be drilled within five years, unless the specific circumstances, justify a longer time.
(iii) Under no circumstances shall estimates for undeveloped reserves be attributable to any acreage for which an application of fluid injection or other improved recovery technique is contemplated, unless such techniques have been proved effective by actual projects in the same reservoir or an analogous reservoir, as defined in paragraph (a)(2) of this section, or by other evidence using reliable technology establishing reasonable certainty.
RYDER SCOTT COMPANY PETROLEUM CONSULTANTS