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MATERIAL CHANGE REPORT UNDER SECTION 75(2) OF


THE SECURITIES ACT (ONTARIO) (THE “ACT”)





1.	Reporting Issuer


	Golden Knight Resources Inc.


	#1180 - 999 West Hastings Street


	Vancouver, B.C.  V6C 2W2





2.	Date of Material Change


	December 22, 1997





3.	Press Release


	


	Date of issuance:		December 22, 1997


	Place of issuance:		Vancouver, British Columbia	





4.	Summary of Material Change


	Drilling at the 90%-owned Seguenega Concession in Burkina Faso has intersected significant gold mineralization in at least three zones within the Gambo area of the concession.  





5.	Full Description of Material Changes


	See attached news release #97-24.





6.	Reliance on Section (75)3 of the Act


	Not applicable





7.	Omitted Information


	No significant facts remain confidential and no information has been omitted in this report.





8.	Senior Officers


	Names:		R.A. Quartermain, President and Director


			Linda J. Sue, Assistant Secretary


	Business Tel:	(604) 689-3846





9.	Statement of Senior Officer


	The foregoing accurately discloses the material change referred to herein.





Dated at Vancouver, British Columbia, this 23rd day of December, 1997.


							Per:	LINDA J. SUE			


								Linda J. Sue


								Assistant Secretary	 





cc:   Toronto Stock Exchange
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Golden Knight Reports Results FRom Drilling in burkina Faso





Vancouver, B.C. --- Golden Knight Resources Inc. reports that drilling at its 90%-owned Seguenega Concession in Burkina Faso has intersected significant gold mineralization in at least three zones within the Gambo area of the concession.  





To date, assay results from 28 reverse circulation holes totalling 2,778 metres on the Gambo II zone have been received.  This program, together with results from an earlier program in 1997, indicate that gold mineralization occurs in lenses within shear-hosted, sub-vertical quartz veins.  In the Gambo II zone, two higher grade lenses with a cumulative strike length of 300 metres, and open at depth, have been defined.  Significant results include 3.4 grams of gold per tonne over 30 metres, 1.7 grams of gold per tonne over 66 metres, 1.2 grams of gold per tonne over 46 metres, and 3.3 grams of gold per tonne over 17 metres.  





Incomplete results from the Gambo I zone, located approximately 500 metres east of Gambo II, indicate potential for additional gold mineralization.  At the Gambo I zone, significant results include 5.2 grams of gold over 7 metres in RC-1 and 5.0 grams of gold per tonne over 5 metres in RC-2.





Results from the Gambo I and Gambo II zones are part of a 4,000-metre program of reverse circulation drilling which tested targets defined by geophysics and trenching in the Gambo, Tiba I and Bakou areas in the southwestern corner of the 400 km2 concession.  Further assay results are pending, and additional drilling will be completed in early 1998.





Golden Knight is among the more active Canadian exploration companies in West Africa.  In addition to the Tarkwa Concession, where production from open pit mining operations is expected to commence in February 1998, the company has interests in 14 other concessions in Ghana and Burkina Faso, as well as the Night Hawk Lake joint venture and the CFM claims in the Timmins gold and base metal camp.
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For further information, contact:





R.A. Quartermain, President	Paul LaFontaine, Manager, Investor Relations


Golden Knight Resources Inc.	Golden Knight Resources Inc.


Vancouver, B.C.	Vancouver, B.C.


(604) 689-3846	(604) 689-3846


	E-mail: invest@golden-knight.com











GAMBO II RC DRILL SUMMARY


Azimuth: 225º, except where noted; dip: -50º





Hole No.�
Coordinates�
From�
To�
Interval�
Gold Grade�
�
�
�
�
(m)�
(m)�
(m)�
(ft)�
oz/ton�
g/tonne�
�
GRC 7 (1)�
27 N�
770 W�
41�
45�
4�
13.1�
0.10�
3.6�
�
�
�
�
53�
83�
30�
98.4�
0.10�
3.4�
�
GRC 8�
91 N�
770 W�
2�
6�
4�
13.1�
0.16�
5.6�
�
�
�
�
36�
56�
20�
65.6�
0.13�
4.6�
�
GRC 30�
140 N�
770 W�
84�
114�
30�
98.4�
0.09�
3.2�
�
GRC 12�
85 N�
850 W�
Anomalous Values�
�
GRC 1 (1)�
36 N�
150 W�
5�
71�
66�
216.5�
0.05�
1.7�
�
GRC 6�
84 N�
150 W�
26�
47�
21�
68.9�
0.03�
1.1�
�
GRC 18�
130 N�
150 W�
81�
85�
4�
13.1�
0.05�
1.8�
�
GRC 2 (1)�
26 N�
50 W�
6�
63�
57�
187.0�
0.07�
2.4�
�
GRC 5�
83 N�
50 W�
42�
80�
38�
124.7�
0.10�
3.3�
�
GRC 22�
110 N�
50 W�
60�
106�
46�
150.9�
0.03�
1.2�
�
GRC 3 (1)�
27 N�
55 E�
14�
36�
22�
72.2�
0.05�
1.7�
�
GRC 4�
89 N�
55 E�
53�
80�
27�
88.6�
0.04�
1.5�
�
GRC 23�
27 N�
55 E�
0�
17�
17�
55.8�
0.10�
3.3�
�
GRC 27�
120 N�
55 E�
84�
113�
29�
95.1�
0.03�
1.1�
�
GRC 10 (1)�
13 N�
150 E�
Anomalous Values�
�
GRC 25�
15 N�
150 E�
Anomalous Values�
�



GAMBO I INITIAL RC DRILL SUMMARY


Azimuth: 280°; dip: -50°


�
�
RC 1�
315 N�
525 E�
1�
12�
11�
36.1�
0.03�
1.2�
�
�
�
�
36�
43�
7�
23.0�
0.15�
5.2�
�
RC 2�
430 N�
340 E�
54�
59�
5�
16.4�
0.15�
5.0�
�
�
�
�
70�
80�
10�
32.8�
0.04�
1.4�
�
(1)  Azimuth: 45°
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